SAFE WORK METHOD STATEMENT (SWMS)
Lay turf · Landscaping · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Business (PCBU) name and ABN
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client and principal contractor
	

	Start date and duration
	

	Working hours
	

	Person responsible for ensuring compliance
	

	Prepared by
	

	Document number and revision
	

	Date given to principal contractor
	

	Review date
	


2. HIGH RISK CONSTRUCTION WORK COVERED BY THIS SWMS
	
	Risk of a person falling more than 2 metres

	
	Work on a telecommunication tower

	
	Demolition of an element of a structure that is load-bearing or related to its physical integrity

	
	Likely to involve disturbing asbestos

	
	Structural alterations or repairs that require temporary support to prevent collapse

	
	Work in or near a confined space

	
	Work in or near a shaft or trench with an excavated depth greater than 1.5 metres

	
	Work in or near a tunnel

	
	Use of explosives

	
	Work on or near pressurised gas distribution mains or piping

	
	Work on or near chemical, fuel or refrigerant lines

	
	Work on or near energised electrical installations or services

	
	Work in an area that may have a contaminated or flammable atmosphere

	
	Work involving tilt-up or precast concrete elements

	
	Work on, in or next to a road, railway, shipping lane or other traffic corridor in use by traffic other than pedestrians

	X
	Work in an area with movement of powered mobile plant

	
	Work in an area with artificial extremes of temperature

	
	Work in or near water or other liquid that involves a risk of drowning

	
	Diving work


3. JOB STEPS, HAZARDS AND CONTROLS
	#
	Job step
	Hazards
	Risk before
	Controls
	Risk after
	Responsible

	1
	Locate irrigation and services before levelling
	Hitting underground services
	Extreme
	- Keep machine buckets well clear of marked services and use a spotter. [Isolate]
- Scan the area with a cable locator before digging and mark services on the ground. [Engineering]
- Hand dig or vacuum excavate to expose services before using a machine near them. [Engineering]
- Lodge a free BYDA (Before You Dig Australia) request and get the plans before any digging. [Administrative]
- Keep plans or locate tickets on site and check them again if the work area grows. [Administrative]
- If you hit a service, stop, get everyone clear, and call the owner and emergency services. [Administrative]
- Wear safety boots, gloves and hi-vis when digging. [PPE]
	Medium
	

	2
	Level and prepare soil with the Bobcat
	Being hit by mobile plant
General dust
	Extreme
	- Separate people and plant with barriers, exclusion zones and marked walkways. [Isolate]
- Use plant with working reversing alarms, cameras and lights. [Engineering]
- Have a traffic management plan showing plant routes, loading areas and pedestrian paths. [Administrative]
- Use a spotter when reversing or working near people. [Administrative]
- Make eye contact with the operator before going near. Stay out of the swing radius. [Administrative]
- Operators hold a High Risk Work Licence where needed (for example forklift) and are trained and assessed on other plant. [Administrative]
- Do a pre-start check on each machine every day and record it. [Administrative]
- Wear hi-vis clothing and a hard hat. [PPE]
- Use low-dust products, such as dust-reduced or pre-mixed compounds. [Substitute]
- Seal off the work area with plastic sheeting in occupied buildings. [Isolate]
- Use tools with dust extraction and a vacuum for clean up. [Engineering]
- Lightly mist the area with water to keep dust down, away from anything electrical. [Engineering]
- Never dry sweep or blow dust off with compressed air. [Administrative]
- Wear a dust mask and safety glasses. [PPE]
	Medium
	

	3
	Lay rolls, lifting with your legs and swapping tasks
	Lifting and carrying heavy loads
Repetitive work and awkward postures
	High
	- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Eliminate]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Substitute]
- Use trolleys, pallet jacks, hoists, vacuum lifters or plant instead of carrying by hand. [Engineering]
- Use a two-person lift for anything heavy, long or awkward. Plan the route first and clear it. [Administrative]
- Keep the load close, back straight and no twisting. Turn with your feet. [Administrative]
- Rotate tasks and take breaks on long lifting jobs. [Administrative]
- Wear gloves for grip and safety boots to protect your feet. [PPE]
- Use tools that cut the effort: powered screwdrivers, long-handled tools and extension poles for overhead work. [Substitute]
- Set work up at waist height on benches or trestles where you can. [Engineering]
- Use light tools with good grips, and keep blades and bits sharp. [Engineering]
- Rotate tasks and take short breaks every hour on repetitive work. [Administrative]
- Warm up before heavy physical work and report aches and pains early. [Administrative]
- Wear knee pads for kneeling work and gloves for grip. [PPE]
	Medium
	

	4
	Apply fertiliser with gloves
	Hazardous chemicals
	Medium
	- Choose the least harmful product that does the job, for example water-based instead of solvent-based. [Substitute]
- Use chemicals in well-ventilated areas, or use fans and extraction in closed rooms. [Engineering]
- Read the Safety Data Sheet (SDS) before use and keep a register of hazardous chemicals on site. [Administrative]
- Keep chemicals in labelled containers. Never decant into drink bottles. [Administrative]
- Store chemicals away from heat, food and drink, and keep products that react with each other apart. [Administrative]
- Have eye wash and a spill kit nearby, and wash hands before eating. [Administrative]
- Wear chemical-resistant gloves and safety glasses or goggles as listed on the SDS. [PPE]
- Use a respirator with the right cartridge if the SDS calls for one. [PPE]
	Medium
	

	5
	Water in, drink plenty and clean up
	Heat stress
Sun exposure (UV)
Poor housekeeping and waste
	High
	- Schedule heavy work for the cooler part of the day. [Eliminate]
- Provide shade over work and rest areas, and fans or cooling in roof spaces. [Engineering]
- Supply cool drinking water close by and drink a cup every 15 to 20 minutes. [Administrative]
- Take regular rest breaks in the shade, more often as it gets hotter. [Administrative]
- Let new and returning workers build up to full work in the heat over about a week. [Administrative]
- Plan outdoor work for early morning or late afternoon when UV is lower. [Eliminate]
- Put shade covers over fixed work areas. [Engineering]
- Check the UV index each day. Use sun protection when it is 3 or higher. [Administrative]
- Check your skin regularly and see a doctor about any new or changing spots. [Administrative]
- Wear a broad-brim hat or hard hat brim, long sleeves, sunglasses and SPF 50+ sunscreen, reapplied every 2 hours. [PPE]
- Order materials to size and send packaging back where you can. [Eliminate]
- Put skip bins and waste chutes close to the work. [Engineering]
- Clean as you go, and do a full clean up at the end of each day. [Administrative]
- Keep exits, stairs and walkways clear at all times. [Administrative]
- Stack materials neatly on level ground, away from edges. [Administrative]
	Medium
	


4. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Steel cap boots
Work gloves
Sun protection (brim hat, long sleeves, SPF 50+)
Knee pads
Hi-vis shirt or vest
Hard hat
P2 dust mask
Safety glasses
Chemical-resistant gloves (nitrile)
Safety goggles
Half-face respirator (P2 or P3 filters)
Overalls
	Skid steer (Bobcat) (Verification of competency (VOC) for the machine)
Wacker plate
Hand tools
Trailer
	None required


5. EMERGENCY ARRANGEMENTS
	Emergency number: 000
	

	Nearest hospital
	

	Assembly point
	

	First aider
	

	First aid kit location
	

	Fire extinguisher location
	


6. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Work Health and Safety Regulations 2011, Part 6.3 (Victoria: OHS Regulations 2017).
Keep this SWMS, and every revised version, until the high risk construction work is finished, where workers and inspectors can see it on site. If a notifiable incident happens during the work, keep it for at least 2 years after the incident.
7. SIGN-OFF
By signing below, each person confirms they have read and understood this SWMS and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/au/swms/landscaping/turf-laying/
