FIELD LEVEL HAZARD ASSESSMENT (FLHA)
Backfill and compaction · Excavation and earthworks · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client / general contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by
	

	Document number and revision
	

	Review date
	


2. JOB STEPS, HAZARDS AND CONTROLS
	#
	Job step
	Hazards
	Risk before
	Controls
	Risk after
	Responsible

	1
	Check services are inspected before backfilling
	Hitting underground services
	Critical
	- Keep machine buckets well clear of marked services and use a spotter. [Engineering (guarding)]
- Scan the area with a cable locator before digging and mark services on the ground. [Engineering]
- Hand expose or hydrovac services before machine digging inside the locate tolerance zone. [Engineering]
- Click Before You Dig: lodge a locate request with your provincial one-call service and wait for the locates. [Administrative]
- Follow your province's ground disturbance rules and keep locate sheets on site. [Administrative]
- Keep plans or locate tickets on site and check them again if the work area grows. [Administrative]
- If you hit a service, stop, get everyone clear, and call the owner and emergency services. [Administrative]
- Wear safety boots, gloves and hi-vis when digging. [PPE]
	Medium
	

	2
	Place fill in layers with the machine, keeping a spotter
	Being hit by heavy equipment
	Critical
	- Separate people and equipment with barriers, exclusion zones and marked walkways. [Engineering (guarding)]
- Use equipment with working backup alarms, cameras and lights. [Engineering]
- Have a site traffic plan showing equipment routes, loading areas and pedestrian paths. [Administrative]
- Use a spotter when backing up or working near people. [Administrative]
- Make eye contact with the operator before going near. Stay out of the swing radius. [Administrative]
- Operators are trained and competent for each machine. [Administrative]
- Do a pre-start check on each machine every day and record it. [Administrative]
- Wear hi-vis clothing and a hard hat. [PPE]
	Medium
	

	3
	Compact each layer, rotating operators to limit vibration
	Hand-arm and whole-body vibration
Loud noise
	High
	- Use low-vibration tools and methods, such as a breaker on an excavator instead of a hand jackhammer. [Substitution]
- Keep tools sharp and well maintained, and use anti-vibration handles and seats. [Engineering]
- Limit trigger time on high-vibration tools and rotate workers. [Administrative]
- Keep hands warm and dry, and take regular breaks. [Administrative]
- Report tingling, numbness or white fingers early. [Administrative]
- Wear gloves to keep hands warm and dry. [PPE]
- Use quieter tools and methods, such as cut-to-size materials, low-noise machines and battery tools. [Substitution]
- Keep noisy equipment away from work areas, and use screens or distance between the noise and people. [Engineering (guarding)]
- Keep tools maintained and use mufflers on compressors and generators. [Engineering]
- Limit time on noisy tools and rotate workers. [Administrative]
- If you have to shout to be heard 1 metre away, wear hearing protection. [Administrative]
- Wear earplugs or earmuffs rated for the noise. [PPE]
	Medium
	

	4
	Keep compactors away from trench edges
	Trench or excavation collapse
	Critical
	- Use methods that keep people out of the trench, such as directional boring or working from the surface. [Elimination]
- Barricade or cover the excavation so people and equipment cannot fall in. [Engineering (guarding)]
- Shore, slope or use a trench box in any trench deeper than 1.2 metres (1.5 metres in Alberta and Manitoba). [Engineering]
- Keep spoil, materials and equipment at least 1 metre back from the edge. [Engineering]
- Provide a safe way in and out, such as a ladder near where people work. [Engineering]
- Inspect the excavation at the start of each shift and after rain or anything that could weaken it. Record it. [Administrative]
- Never work alone in a trench. Watch for water, cracks and bulging walls, and get out if you see them. [Administrative]
- Wear a hard hat, hi-vis and safety boots. [PPE]
	Medium
	

	5
	Clean up and take compaction tests
	Poor housekeeping and waste
	Medium
	- Order materials to size and send packaging back where you can. [Elimination]
- Put waste bins and chutes close to the work. [Engineering]
- Clean as you go, and do a full clean up at the end of each day. [Administrative]
- Keep exits, stairs and walkways clear at all times. [Administrative]
- Stack materials neatly on level ground, away from edges. [Administrative]
- Wear gloves when handling waste. [PPE]
	Low
	


3. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	CSA green triangle safety boots (CSA Z195)
High-visibility vest (CSA Z96)
Hearing protection
Work gloves
Hard hat (CSA Z94.1)
	Plate tamper
Skid steer (Provincial operator training)
Excavator (Provincial operator training)
	Ground disturbance permit / locate


4. EMERGENCY ARRANGEMENTS
	Emergency number: 911
	

	Nearest hospital
	

	Muster point
	

	First aid attendant
	

	First aid kit location
	

	Fire extinguisher location
	


5. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Provincial occupational health and safety law (e.g. Ontario OHSA and O. Reg. 213/91, BC OHS Regulation, Alberta OHS Code).
Keep completed hazard assessments for at least 3 years (COR auditors sample the last 12 months). Review this FLHA and re-sign whenever the task, crew or conditions change.
6. END OF SHIFT REVIEW
	Area cleaned up and safe (yes / no)
	

	Permits closed
	

	Incidents or near misses
	

	Hazards remaining
	


7. SIGN-OFF
By signing below, each person confirms they have read and understood this FLHA and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/ca/flha/excavation/backfill-compaction/
