FIELD LEVEL HAZARD ASSESSMENT (FLHA)
Build a garden suite · General contracting · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client / general contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by
	

	Document number and revision
	

	Review date
	


2. JOB STEPS, HAZARDS AND CONTROLS
	#
	Job step
	Hazards
	Risk before
	Controls
	Risk after
	Responsible

	1
	Set up fencing and keep the main house occupants away from the work
	Public entering the work area
Working in an occupied home or building
	High
	- Fence off the site with secure temporary fencing and lock the gates when you leave. [Engineering (guarding)]
- Give pedestrians a safe, marked path around the work, with ramps for strollers and wheelchairs. [Engineering (guarding)]
- Use hoarding, covered walkways or catch fans where work is above public areas. [Engineering]
- Put signs at each entry: site name, contact number and "No unauthorised entry". [Administrative]
- Make the site safe at the end of each day: cover holes, lower buckets and booms, remove ladders and lock tools away. [Administrative]
- Use a spotter when moving equipment or materials across public paths. [Administrative]
- Plan noisy, dusty or risky work for when the building is empty. [Elimination]
- Close off the work area with barriers, plastic sheeting or locked doors, and put up signs. [Engineering (guarding)]
- Keep fire exits and paths clear at all times. [Administrative]
- Tell occupants before you turn off power, water or gas, and before noisy or dusty work. [Administrative]
- Lock away tools, chemicals and materials each day, out of reach of children. [Administrative]
- Clean up dust and debris at the end of each day. [Administrative]
	Low
	

	2
	Excavate and pour the slab
	Hitting underground services
Being hit by heavy equipment
Wet concrete and cement burns
	Critical
	- Keep machine buckets well clear of marked services and use a spotter. [Engineering (guarding)]
- Scan the area with a cable locator before digging and mark services on the ground. [Engineering]
- Hand expose or hydrovac services before machine digging inside the locate tolerance zone. [Engineering]
- Click Before You Dig: lodge a locate request with your provincial one-call service and wait for the locates. [Administrative]
- Follow your province's ground disturbance rules and keep locate sheets on site. [Administrative]
- Keep plans or locate tickets on site and check them again if the work area grows. [Administrative]
- Separate people and equipment with barriers, exclusion zones and marked walkways. [Engineering (guarding)]
- Use equipment with working backup alarms, cameras and lights. [Engineering]
- Have a site traffic plan showing equipment routes, loading areas and pedestrian paths. [Administrative]
- Use a spotter when backing up or working near people. [Administrative]
- Make eye contact with the operator before going near. Stay out of the swing radius. [Administrative]
- Use long-handled tools and pumps to cut down contact. [Engineering]
- Wash concrete off skin straight away with clean water. [Administrative]
- Have clean water and eye wash at the pour. [Administrative]
- Wear waterproof gloves, long sleeves and rubber boots with pants worn over the top. [PPE]
- Wear safety glasses or goggles to stop splashes. [PPE]
	Medium
	

	3
	Frame and roof with edge protection
	Falling from height
Falling from a roof edge
Nail gun injuries
	Critical
	- Do the work from the ground where you can, for example pre-assemble on the ground or use extension poles. [Elimination]
- Install guardrails or edge protection on all open edges before work starts. [Engineering (guarding)]
- Use a scaffold, mobile work platform or aerial work platform instead of working off a ladder. [Engineering]
- Where edge protection is not practical, use a fall restraint or fall arrest system on a rated anchor point. [Engineering]
- Fall protection plan in place where required. Workers trained in fall protection (Working at Heights training in Ontario). [Administrative]
- Have a rescue plan so a worker hanging in a harness can be brought down within minutes. [Administrative]
- Do what you can from the ground or from a scaffold at the gutter line, for example pre-assemble parts on the ground. [Elimination]
- Install edge protection or guardrails on all open roof edges before work starts. [Engineering (guarding)]
- Use a perimeter scaffold with handrails and toe boards along the eaves where practical. [Engineering]
- Where guardrails cannot be fitted, use fall restraint on certified roof anchors so workers cannot reach the edge. [Engineering]
- Use one safe, controlled access point and keep others off the roof. [Administrative]
- Use a nail gun with a sequential (single shot) trigger, not a contact or bump trigger. [Substitution]
- Disconnect the air or battery before clearing jams, adjusting or moving between work areas. [Engineering]
- Keep your free hand at least 30 cm from the nailing point. [Administrative]
- Never point the gun at anyone or carry it with your finger on the trigger. [Administrative]
- Train new users before they use a nail gun, and check for pipes, cables and metal behind the surface. [Administrative]
	Medium
	

	4
	Connect services by licensed trades
	Electric shock from live wiring
Gas and fuel lines
Trench or excavation collapse
	Critical
	- Isolate the power before any work. Do not work live. [Elimination]
- Lock out and tag the isolation point with your own personal lock and danger tag. [Engineering (guarding)]
- Test before you touch: prove dead at the point of work with a tested voltage tester. [Engineering]
- Only licensed electricians do electrical work, to the Canadian Electrical Code and provincial rules. [Administrative]
- Check for back feeds from solar, batteries and generators that can keep a circuit live after the main switch is off. [Administrative]
- Isolate and purge the line before work, with the owner's approval. [Elimination]
- Lock off and tag the isolation valve. [Engineering (guarding)]
- Check for leaks with a gas detector before and during work, and ventilate the area. [Engineering]
- Only licensed gas fitters work on gas lines. [Administrative]
- Remove ignition sources: no smoking, no hot work and no sparking tools near the line. [Administrative]
- Use methods that keep people out of the trench, such as directional boring or working from the surface. [Elimination]
- Barricade or cover the excavation so people and equipment cannot fall in. [Engineering (guarding)]
- Shore, slope or use a trench box in any trench deeper than 1.2 metres (1.5 metres in Alberta and Manitoba). [Engineering]
- Keep spoil, materials and equipment at least 1 metre back from the edge. [Engineering]
- Provide a safe way in and out, such as a ladder near where people work. [Engineering]
- Inspect the excavation at the start of each shift and after rain or anything that could weaken it. Record it. [Administrative]
	Medium
	

	5
	Fit out and clean up
	General dust
Poor housekeeping and waste
	Medium
	- Use low-dust products, such as dust-reduced or pre-mixed compounds. [Substitution]
- Seal off the work area with plastic sheeting in occupied buildings. [Engineering (guarding)]
- Use tools with dust extraction and a vacuum for clean up. [Engineering]
- Lightly mist the area with water to keep dust down, away from anything electrical. [Engineering]
- Never dry sweep or blow dust off with compressed air. [Administrative]
- Wear a dust mask and safety glasses. [PPE]
- Order materials to size and send packaging back where you can. [Elimination]
- Put waste bins and chutes close to the work. [Engineering]
- Clean as you go, and do a full clean up at the end of each day. [Administrative]
- Keep exits, stairs and walkways clear at all times. [Administrative]
- Stack materials neatly on level ground, away from edges. [Administrative]
- Wear gloves when handling waste. [PPE]
	Low
	


3. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	CSA green triangle safety boots (CSA Z195)
High-visibility vest (CSA Z96)
Hard hat (CSA Z94.1)
Safety glasses (CSA Z94.3)
Hearing protection
Full body harness (fall arrest)
N95 respirator
Chemical-resistant gloves
Safety goggles
Knee pads
Sun protection (sunscreen, hat, long sleeves)
Work gloves
	Excavator (Provincial operator training)
Concrete pump truck
Frame scaffold (Provincial scaffold erector training)
Nail gun
Circular saw
	Roof access permit
Fall protection plan


4. EMERGENCY ARRANGEMENTS
	Emergency number: 911
	

	Nearest hospital
	

	Muster point
	

	First aid attendant
	

	First aid kit location
	

	Fire extinguisher location
	


5. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Provincial occupational health and safety law (e.g. Ontario OHSA and O. Reg. 213/91, BC OHS Regulation, Alberta OHS Code).
Keep completed hazard assessments for at least 3 years (COR auditors sample the last 12 months). Review this FLHA and re-sign whenever the task, crew or conditions change.
6. END OF SHIFT REVIEW
	Area cleaned up and safe (yes / no)
	

	Permits closed
	

	Incidents or near misses
	

	Hazards remaining
	


7. SIGN-OFF
By signing below, each person confirms they have read and understood this FLHA and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/ca/flha/general-building/granny-flat-construction/
