FIELD LEVEL HAZARD ASSESSMENT (FLHA)
Shed and garage construction · General contracting · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client / general contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by
	

	Document number and revision
	

	Review date
	


2. JOB STEPS, HAZARDS AND CONTROLS
	#
	Job step
	Hazards
	Risk before
	Controls
	Risk after
	Responsible

	1
	Get utility locates and pour the slab or footings
	Hitting underground services
Wet concrete and cement burns
	Critical
	- Keep machine buckets well clear of marked services and use a spotter. [Engineering (guarding)]
- Scan the area with a cable locator before digging and mark services on the ground. [Engineering]
- Hand expose or hydrovac services before machine digging inside the locate tolerance zone. [Engineering]
- Click Before You Dig: lodge a locate request with your provincial one-call service and wait for the locates. [Administrative]
- Follow your province's ground disturbance rules and keep locate sheets on site. [Administrative]
- Keep plans or locate tickets on site and check them again if the work area grows. [Administrative]
- If you hit a service, stop, get everyone clear, and call the owner and emergency services. [Administrative]
- Wear safety boots, gloves and hi-vis when digging. [PPE]
- Use long-handled tools and pumps to cut down contact. [Engineering]
- Wash concrete off skin straight away with clean water. [Administrative]
- Have clean water and eye wash at the pour. [Administrative]
- Wear waterproof gloves, long sleeves and rubber boots with pants worn over the top. [PPE]
- Wear safety glasses or goggles to stop splashes. [PPE]
	Medium
	

	2
	Stand the frame and brace it straight away
	Structural collapse during alterations
Strong wind and storms
Lifting and carrying heavy loads
	High
	- Get an engineer to check before removing any wall, beam, post or bracing that may be load-bearing. [Elimination]
- Keep everyone clear of the area under and next to the work. [Engineering (guarding)]
- Install temporary props, needles or shoring as designed before removing any support. [Engineering]
- Follow the engineer's sequence. Do not change it without approval. [Administrative]
- Check props daily. Do not remove them until the permanent support is in and approved. [Administrative]
- Check the forecast each morning and plan work at height and lifting around the weather. [Elimination]
- Tie down or weigh down loose sheets, panels, boards and rubbish at the end of each shift. [Engineering]
- Set wind limits for roof work, platforms and cranes, using the manufacturer's limits, and stop when they are reached. [Administrative]
- Stop work and get down in lightning. Wait 30 minutes after the last thunder before going back up. [Administrative]
- Check scaffold, fencing and edge protection after strong wind before anyone uses them. [Administrative]
- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Elimination]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Substitution]
- Use trolleys, pallet jacks, hoists, vacuum lifters or equipment instead of carrying by hand. [Engineering]
- Use a two-person lift for anything heavy, long or awkward. Plan the route first and clear it. [Administrative]
- Keep the load close, back straight and no twisting. Turn with your feet. [Administrative]
	Medium
	

	3
	Fix wall and roof sheets, working from a secured ladder or scaffold
	Falling from a ladder
Falling from a roof edge
Cuts from sharp edges
	Critical
	- Use a platform ladder, mobile scaffold or aerial work platform for longer jobs instead of a straight ladder. [Substitution]
- Use CSA Grade 1, 1A or 1AA ladders in good condition. Remove any damaged ladder from site. [Engineering]
- Set extension ladders at a 4 to 1 angle on firm, level ground, tied or footed, and reaching 1 metre above the landing. [Engineering]
- Use ladders only for short, light work. Do not carry heavy or awkward loads up a ladder. [Administrative]
- Keep three points of contact and your belt buckle between the side rails. Do not overreach. [Administrative]
- Do what you can from the ground or from a scaffold at the gutter line, for example pre-assemble parts on the ground. [Elimination]
- Install edge protection or guardrails on all open roof edges before work starts. [Engineering (guarding)]
- Use a perimeter scaffold with handrails and toe boards along the eaves where practical. [Engineering]
- Where guardrails cannot be fitted, use fall restraint on certified roof anchors so workers cannot reach the edge. [Engineering]
- Use one safe, controlled access point and keep others off the roof. [Administrative]
- Deburr or cover sharp edges, and fit edge protectors on exposed sheet metal. [Engineering]
- Use knives with retractable or self-retracting blades. [Engineering]
- Cut away from your body and keep your other hand clear. [Administrative]
- Put used blades in a blade bin or sharps container. [Administrative]
- Use two people to handle large sheets of metal or glass. [Administrative]
	Medium
	

	4
	Cut sheets with shears or nibblers rather than a grinder
	Angle grinder injuries
Fire from hot works
Loud noise
	Critical
	- Use a guarded saw or a different tool where you can. [Substitution]
- Keep the guard on and use the side handle. Never remove the guard. [Engineering]
- Use the right disc for the job, rated for the grinder's speed. Check it for cracks first. [Administrative]
- Only trained people change discs, with the grinder unplugged or the battery out. [Administrative]
- Keep both hands on the grinder and let the disc stop before putting it down. [Administrative]
- Use cold work methods where you can, such as bolting, press fittings or cutting with a saw instead of a torch. [Elimination]
- Move anything that can burn at least 10 metres away, or cover it with fire blankets. [Engineering (guarding)]
- Use fire-resistant screens to stop sparks reaching people or gaps in walls and floors. [Engineering]
- Get a hot work permit before starting. [Administrative]
- Keep a charged fire extinguisher and fire blanket at the work spot. [Administrative]
- Use quieter tools and methods, such as cut-to-size materials, low-noise machines and battery tools. [Substitution]
- Keep noisy equipment away from work areas, and use screens or distance between the noise and people. [Engineering (guarding)]
- Keep tools maintained and use mufflers on compressors and generators. [Engineering]
- Limit time on noisy tools and rotate workers. [Administrative]
- If you have to shout to be heard 1 metre away, wear hearing protection. [Administrative]
	Medium
	

	5
	Fit doors, flashings and clean up
	Poor housekeeping and waste
	Medium
	- Order materials to size and send packaging back where you can. [Elimination]
- Put waste bins and chutes close to the work. [Engineering]
- Clean as you go, and do a full clean up at the end of each day. [Administrative]
- Keep exits, stairs and walkways clear at all times. [Administrative]
- Stack materials neatly on level ground, away from edges. [Administrative]
- Wear gloves when handling waste. [PPE]
	Low
	


3. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	CSA green triangle safety boots (CSA Z195)
Cut-resistant gloves
Safety glasses (CSA Z94.3)
Hearing protection
Full body harness (fall arrest)
Sun protection (sunscreen, hat, long sleeves)
Chemical-resistant gloves
Safety goggles
Knee pads
Hard hat (CSA Z94.1)
Work gloves
Face shield
Welding gloves
Coveralls
	Cement mixer
Power drill
Angle grinder
Extension ladder
Hand tools
	Roof access permit
Fall protection plan
Hot work permit


4. EMERGENCY ARRANGEMENTS
	Emergency number: 911
	

	Nearest hospital
	

	Muster point
	

	First aid attendant
	

	First aid kit location
	

	Fire extinguisher location
	


5. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Provincial occupational health and safety law (e.g. Ontario OHSA and O. Reg. 213/91, BC OHS Regulation, Alberta OHS Code).
Keep completed hazard assessments for at least 3 years (COR auditors sample the last 12 months). Review this FLHA and re-sign whenever the task, crew or conditions change.
6. END OF SHIFT REVIEW
	Area cleaned up and safe (yes / no)
	

	Permits closed
	

	Incidents or near misses
	

	Hazards remaining
	


7. SIGN-OFF
By signing below, each person confirms they have read and understood this FLHA and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/ca/flha/general-building/shed-garage-construction/
