FIELD LEVEL HAZARD ASSESSMENT (FLHA)
Shopfront and commercial glazing · Glazing · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client / general contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by
	

	Document number and revision
	

	Review date
	


2. JOB STEPS, HAZARDS AND CONTROLS
	#
	Job step
	Hazards
	Risk before
	Controls
	Risk after
	Responsible

	1
	Set up pedestrian control on the sidewalk
	Public entering the work area
Road traffic
	Critical
	- Fence off the site with secure temporary fencing and lock the gates when you leave. [Engineering (guarding)]
- Give pedestrians a safe, marked path around the work, with ramps for strollers and wheelchairs. [Engineering (guarding)]
- Use hoarding, covered walkways or catch fans where work is above public areas. [Engineering]
- Put signs at each entry: site name, contact number and "No unauthorised entry". [Administrative]
- Make the site safe at the end of each day: cover holes, lower buckets and booms, remove ladders and lock tools away. [Administrative]
- Use a spotter when moving equipment or materials across public paths. [Administrative]
- Do the work at low-traffic times, or close the road or lane with approval. [Elimination]
- Put solid barriers between the work and traffic where speeds are high, not just cones. [Engineering (guarding)]
- Use a truck-mounted attenuator or buffer vehicle on high speed roads. [Engineering]
- Set up signs and cones to your provincial traffic control manual, with trained traffic control persons. [Administrative]
- Get a road occupancy permit from the municipality or road authority before you start. [Administrative]
- Park work vehicles to shield the work zone, with beacons on. [Administrative]
- Wear high-visibility clothing to CSA Z96. [PPE]
	Medium
	

	2
	Plan large lifts with vacuum lifters or crane
	Crane and lifting failure
Glass handling and breakage
	High
	- Barricade the lift zone and keep everyone out from under the load. [Engineering (guarding)]
- Use a crane rated for the load at the radius, set up on firm ground with outrigger pads. [Engineering]
- Check slings, chains, shackles and hooks before use. Remove anything damaged or not tagged. [Engineering]
- Plan the lift: weight, radius, ground, path and landing area. Use a written lift plan for complex lifts. [Administrative]
- Use certified crane operators and trained riggers and signallers, as your province requires. [Administrative]
- Use tag lines to control loads and agree on clear radio or hand signals. [Administrative]
- Stop lifting in high wind or when the operator cannot see the signaller. [Administrative]
- Never ride on a load or hook. [Administrative]
- Wear a hard hat, hi-vis, gloves and safety boots. [PPE]
- Use suction lifters, glass trolleys or a glazing robot for large panes. [Engineering]
- Store glass upright on racks and secure it. Never lay it flat or lean it loosely. [Engineering]
- Use two or more people for large panes, and clear the carry route first. [Administrative]
- Mark new glass with tape or stickers so nobody walks into it. [Administrative]
- Clean up broken glass straight away into a marked container. [Administrative]
- Wear cut-resistant gloves, arm guards, safety glasses and safety boots. [PPE]
	Medium
	

	3
	Work from a aerial work platform for high panes
	Aerial work platform tip-over or crush
Falling from height
	Critical
	- Check the ground before setting up. Use outriggers and spreader pads, and keep clear of trenches, pits and slopes. [Engineering]
- Use a platform with tilt alarm and secondary guarding (anti-entrapment) where there is an overhead crush risk. [Engineering]
- Operators are trained to CSA B354.8 and the manufacturer's instructions, and the platform is inspected to CSA B354.7. [Administrative]
- Do a pre-start check each day. Keep a trained person on the ground who can lower the platform in an emergency. [Administrative]
- Never exceed the safe working load, climb on the rails or use a ladder in the basket. [Administrative]
- In boom-type platforms, wear a harness clipped to the basket anchor point. [PPE]
- Do the work from the ground where you can, for example pre-assemble on the ground or use extension poles. [Elimination]
- Install guardrails or edge protection on all open edges before work starts. [Engineering (guarding)]
- Use a scaffold, mobile work platform or aerial work platform instead of working off a ladder. [Engineering]
- Where edge protection is not practical, use a fall restraint or fall arrest system on a rated anchor point. [Engineering]
- Fall protection plan in place where required. Workers trained in fall protection (Working at Heights training in Ontario). [Administrative]
- Have a rescue plan so a worker hanging in a harness can be brought down within minutes. [Administrative]
- Wear a full body harness with a shock-absorbing lanyard, clipped on at all times when using fall arrest. [PPE]
	Medium
	

	4
	Install frames and glass, keeping everyone out from under the load
	Falling tools and materials
Lifting and carrying heavy loads
	High
	- Barricade and sign the drop zone under overhead work so nobody walks beneath. [Engineering (guarding)]
- Fit toe boards, kick plates and mesh screens on scaffolds and edges. [Engineering]
- Use catch fans, debris netting or covered walkways where people pass below. [Engineering]
- Tether hand tools when working at height. [Engineering]
- Keep platforms tidy. Do not stack materials near edges or above toe board height. [Administrative]
- Lower materials with a hoist, chute or rope. Never throw or drop anything down. [Administrative]
- Wear a hard hat anywhere objects could fall. [PPE]
- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Elimination]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Substitution]
- Use trolleys, pallet jacks, hoists, vacuum lifters or equipment instead of carrying by hand. [Engineering]
- Use a two-person lift for anything heavy, long or awkward. Plan the route first and clear it. [Administrative]
- Keep the load close, back straight and no twisting. Turn with your feet. [Administrative]
- Rotate tasks and take breaks on long lifting jobs. [Administrative]
- Wear gloves for grip and safety boots to protect your feet. [PPE]
	Medium
	

	5
	Seal, clean up and reopen the sidewalk
	Hazardous chemicals
Poor housekeeping and waste
	Medium
	- Choose the least harmful product that does the job, for example water-based instead of solvent-based. [Substitution]
- Use chemicals in well-ventilated areas, or use fans and extraction in closed rooms. [Engineering]
- Read the Safety Data Sheet (SDS) and WHMIS labels before use. Workers have WHMIS training. [Administrative]
- Keep chemicals in labelled containers. Never decant into drink bottles. [Administrative]
- Store chemicals away from heat, food and drink, and keep products that react with each other apart. [Administrative]
- Have eye wash and a spill kit nearby, and wash hands before eating. [Administrative]
- Wear chemical-resistant gloves and safety glasses or goggles as listed on the SDS. [PPE]
- Use a respirator with the right cartridge if the SDS calls for one. [PPE]
- Order materials to size and send packaging back where you can. [Elimination]
- Put waste bins and chutes close to the work. [Engineering]
- Clean as you go, and do a full clean up at the end of each day. [Administrative]
- Keep exits, stairs and walkways clear at all times. [Administrative]
- Stack materials neatly on level ground, away from edges. [Administrative]
- Wear gloves when handling waste. [PPE]
	Medium
	


3. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	CSA green triangle safety boots (CSA Z195)
Hard hat (CSA Z94.1)
High-visibility vest (CSA Z96)
Cut-resistant gloves
Safety glasses (CSA Z94.3)
Full body harness (fall arrest)
Work gloves
Chemical-resistant gloves
Safety goggles
Respirator fit tested to CSA Z94.4 (P100 for dust, or the type the air test calls for)
Coveralls
	Mobile crane (Provincial crane operator certification, qualified rigger)
Boom lift (Provincial aerial work platform operator training (CSA B354.8))
Telehandler (Provincial lift truck or telehandler operator training)
Power drill
Hand tools
	Lift plan
Fall protection plan


4. EMERGENCY ARRANGEMENTS
	Emergency number: 911
	

	Nearest hospital
	

	Muster point
	

	First aid attendant
	

	First aid kit location
	

	Fire extinguisher location
	


5. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Provincial occupational health and safety law (e.g. Ontario OHSA and O. Reg. 213/91, BC OHS Regulation, Alberta OHS Code).
Keep completed hazard assessments for at least 3 years (COR auditors sample the last 12 months). Review this FLHA and re-sign whenever the task, crew or conditions change.
6. END OF SHIFT REVIEW
	Area cleaned up and safe (yes / no)
	

	Permits closed
	

	Incidents or near misses
	

	Hazards remaining
	


7. SIGN-OFF
By signing below, each person confirms they have read and understood this FLHA and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/ca/flha/glazing/shopfront-glazing/
