FIELD LEVEL HAZARD ASSESSMENT (FLHA)
Sliding glass door installation · Glazing · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client / general contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by
	

	Document number and revision
	

	Review date
	


2. JOB STEPS, HAZARDS AND CONTROLS
	#
	Job step
	Hazards
	Risk before
	Controls
	Risk after
	Responsible

	1
	Remove the old door, wearing cut gloves
	Glass handling and breakage
Cuts from sharp edges
	High
	- Use suction lifters, glass trolleys or a glazing robot for large panes. [Engineering]
- Store glass upright on racks and secure it. Never lay it flat or lean it loosely. [Engineering]
- Use two or more people for large panes, and clear the carry route first. [Administrative]
- Mark new glass with tape or stickers so nobody walks into it. [Administrative]
- Clean up broken glass straight away into a marked container. [Administrative]
- Wear cut-resistant gloves, arm guards, safety glasses and safety boots. [PPE]
- Deburr or cover sharp edges, and fit edge protectors on exposed sheet metal. [Engineering]
- Use knives with retractable or self-retracting blades. [Engineering]
- Cut away from your body and keep your other hand clear. [Administrative]
- Put used blades in a blade bin or sharps container. [Administrative]
- Use two people to handle large sheets of metal or glass. [Administrative]
- Wear cut-resistant gloves and long sleeves. [PPE]
	Medium
	

	2
	Carry panels with enough people or a glass trolley
	Lifting and carrying heavy loads
	High
	- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Elimination]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Substitution]
- Use trolleys, pallet jacks, hoists, vacuum lifters or equipment instead of carrying by hand. [Engineering]
- Use a two-person lift for anything heavy, long or awkward. Plan the route first and clear it. [Administrative]
- Keep the load close, back straight and no twisting. Turn with your feet. [Administrative]
- Rotate tasks and take breaks on long lifting jobs. [Administrative]
- Wear gloves for grip and safety boots to protect your feet. [PPE]
	Medium
	

	3
	Fit and level the frame
	Injury from power tools
Repetitive work and awkward postures
	Medium
	- Keep all guards fitted and working. Never tie back or remove a guard. [Engineering]
- Clamp or secure the work piece. Do not hold it by hand. [Engineering]
- Only trained, competent people use power tools, following the maker's instructions. [Administrative]
- Check tools before use. Unplug or remove the battery before changing blades or bits. [Administrative]
- No loose clothing, jewellery or long hair near spinning parts. [Administrative]
- Wear safety glasses and hearing protection. Do not wear loose gloves on drills or other rotating tools. [PPE]
- Use tools that cut the effort: powered screwdrivers, long-handled tools and extension poles for overhead work. [Substitution]
- Set work up at waist height on benches or trestles where you can. [Engineering]
- Use light tools with good grips, and keep blades and bits sharp. [Engineering]
- Rotate tasks and take short breaks every hour on repetitive work. [Administrative]
- Warm up before heavy physical work and report aches and pains early. [Administrative]
- Wear knee pads for kneeling work and gloves for grip. [PPE]
	Medium
	

	4
	Install panels and test the door
	Glass handling and breakage
Lifting and carrying heavy loads
	High
	- Glass handling and breakage: see step 1 for the full controls [Administrative]
- Lifting and carrying heavy loads: see step 2 for the full controls [Administrative]
	Medium
	

	5
	Clean up
	Poor housekeeping and waste
	Medium
	- Order materials to size and send packaging back where you can. [Elimination]
- Put waste bins and chutes close to the work. [Engineering]
- Clean as you go, and do a full clean up at the end of each day. [Administrative]
- Keep exits, stairs and walkways clear at all times. [Administrative]
- Stack materials neatly on level ground, away from edges. [Administrative]
- Wear gloves when handling waste. [PPE]
	Low
	


3. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Cut-resistant gloves
Safety glasses (CSA Z94.3)
CSA green triangle safety boots (CSA Z195)
Work gloves
Hearing protection
Knee pads
	Power drill
Hand tools
	None required


4. EMERGENCY ARRANGEMENTS
	Emergency number: 911
	

	Nearest hospital
	

	Muster point
	

	First aid attendant
	

	First aid kit location
	

	Fire extinguisher location
	


5. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Provincial occupational health and safety law (e.g. Ontario OHSA and O. Reg. 213/91, BC OHS Regulation, Alberta OHS Code).
Keep completed hazard assessments for at least 3 years (COR auditors sample the last 12 months). Review this FLHA and re-sign whenever the task, crew or conditions change.
6. END OF SHIFT REVIEW
	Area cleaned up and safe (yes / no)
	

	Permits closed
	

	Incidents or near misses
	

	Hazards remaining
	


7. SIGN-OFF
By signing below, each person confirms they have read and understood this FLHA and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/ca/flha/glazing/sliding-door-installation/
