FIELD LEVEL HAZARD ASSESSMENT (FLHA)
Airless spray painting · Painting · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client / general contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by
	

	Document number and revision
	

	Review date
	


2. JOB STEPS, HAZARDS AND CONTROLS
	#
	Job step
	Hazards
	Risk before
	Controls
	Risk after
	Responsible

	1
	Mask off and ventilate the area, and remove ignition sources
	Flammable liquids and gases
Fire and emergencies
	High
	- Use non-flammable or water-based products where you can. [Substitution]
- Keep ignition sources away: no smoking, no hot work and no running engines near flammables. [Engineering (guarding)]
- Store fuels and solvents in approved, closed containers in a ventilated area away from the work. [Engineering]
- Refuel equipment outdoors with the engine off and cool. [Administrative]
- Keep only what you need for the day on site. [Administrative]
- Store gas cylinders upright, secured and outdoors. [Administrative]
- Keep a suitable fire extinguisher where flammables are used or stored. [Administrative]
- Wear chemical gloves and safety glasses when pouring or mixing. [PPE]
- Provide fire extinguishers suited to the site, checked and easy to reach. [Engineering]
- Keep exits and escape routes clear and signed. [Engineering]
- Have a site emergency plan: alarm, exits, assembly point and emergency contacts. [Administrative]
- Keep a stocked first aid kit and at least one trained first aider on site. [Administrative]
- Know the site address and how emergency services get in. Call 911. [Administrative]
- Go through the emergency plan with every worker and visitor at induction. [Administrative]
- Keep flammable materials and rubbish away from exits and escape routes. [Administrative]
	Medium
	

	2
	Check hoses and tip guard, and lock the trigger when not spraying
	Stored energy
Hazardous chemicals
	Medium
	- Release or block all stored energy before work: release the pressure in pipes, tanks and hoses, bleed hydraulics, release springs, lower loads. [Elimination]
- Lock out and tag all energy sources with personal locks. [Engineering (guarding)]
- Stored energy: see step 5 for the full controls [Administrative]
- Choose the least harmful product that does the job, for example water-based instead of solvent-based. [Substitution]
- Use chemicals in well-ventilated areas, or use fans and extraction in closed rooms. [Engineering]
- Hazardous chemicals: see step 4 for the full controls [Administrative]
	Medium
	

	3
	Never point the gun at anyone or put a hand near the tip
	Stored energy
Cuts from sharp edges
	Medium
	- Put mechanical blocks or props under raised parts like buckets, tipper bodies and doors. [Engineering]
- Test that the system is dead and nothing can move before you start. [Administrative]
- Stored energy: see step 5 for the full controls [Administrative]
- Deburr or cover sharp edges, and fit edge protectors on exposed sheet metal. [Engineering]
- Use knives with retractable or self-retracting blades. [Engineering]
- Cut away from your body and keep your other hand clear. [Administrative]
- Put used blades in a blade bin or sharps container. [Administrative]
- Use two people to handle large sheets of metal or glass. [Administrative]
- Wear cut-resistant gloves and long sleeves. [PPE]
	Low
	

	4
	Spray with a respirator and goggles, keeping others out
	Hazardous chemicals
Eye injuries
	Medium
	- Choose the least harmful product that does the job, for example water-based instead of solvent-based. [Substitution]
- Use chemicals in well-ventilated areas, or use fans and extraction in closed rooms. [Engineering]
- Read the Safety Data Sheet (SDS) and WHMIS labels before use. Workers have WHMIS training. [Administrative]
- Keep chemicals in labelled containers. Never decant into drink bottles. [Administrative]
- Store chemicals away from heat, food and drink, and keep products that react with each other apart. [Administrative]
- Have eye wash and a spill kit nearby, and wash hands before eating. [Administrative]
- Wear chemical-resistant gloves and safety glasses or goggles as listed on the SDS. [PPE]
- Use a respirator with the right cartridge if the SDS calls for one. [PPE]
- Use tool guards and screens to stop flying particles. [Engineering]
- Use dust extraction and water to keep dust out of the air. [Engineering]
- Keep others out of the area when cutting, grinding or chipping. [Administrative]
- Keep an eye wash station or eye wash bottles on site. [Administrative]
- Wear safety glasses at all times, goggles for dust and chemicals, and a face shield for grinding. [PPE]
	Medium
	

	5
	Release pressure before cleaning or changing tips
	Stored energy
	Medium
	- Release or block all stored energy before work: release the pressure in pipes, tanks and hoses, bleed hydraulics, release springs, lower loads. [Elimination]
- Lock out and tag all energy sources with personal locks. [Engineering (guarding)]
- Put mechanical blocks or props under raised parts like buckets, tipper bodies and doors. [Engineering]
- Test that the system is dead and nothing can move before you start. [Administrative]
- Follow the maker's procedure, for example for garage door and roller door springs. [Administrative]
- Wear safety glasses and gloves. [PPE]
	Low
	

	6
	Clean the pump and dispose of solvent waste properly
	Flammable liquids and gases
Poor housekeeping and waste
	High
	- Flammable liquids and gases: see step 1 for the full controls [Administrative]
- Order materials to size and send packaging back where you can. [Elimination]
- Put waste bins and chutes close to the work. [Engineering]
- Clean as you go, and do a full clean up at the end of each day. [Administrative]
- Keep exits, stairs and walkways clear at all times. [Administrative]
- Stack materials neatly on level ground, away from edges. [Administrative]
- Wear gloves when handling waste. [PPE]
	Medium
	


3. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Respirator fit tested to CSA Z94.4 (P100 for dust, or the type the air test calls for)
Safety goggles
Coveralls
Chemical-resistant gloves
CSA green triangle safety boots (CSA Z195)
Safety glasses (CSA Z94.3)
Work gloves
Cut-resistant gloves
Face shield
	Airless paint sprayer
Air compressor
Rolling scaffold (Provincial scaffold training)
Scissor lift (Provincial aerial work platform operator training (CSA B354.8))
	Lockout permit


4. EMERGENCY ARRANGEMENTS
	Emergency number: 911
	

	Nearest hospital
	

	Muster point
	

	First aid attendant
	

	First aid kit location
	

	Fire extinguisher location
	


5. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Provincial occupational health and safety law (e.g. Ontario OHSA and O. Reg. 213/91, BC OHS Regulation, Alberta OHS Code).
Keep completed hazard assessments for at least 3 years (COR auditors sample the last 12 months). Review this FLHA and re-sign whenever the task, crew or conditions change.
6. END OF SHIFT REVIEW
	Area cleaned up and safe (yes / no)
	

	Permits closed
	

	Incidents or near misses
	

	Hazards remaining
	


7. SIGN-OFF
By signing below, each person confirms they have read and understood this FLHA and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/ca/flha/painting/airless-spray-painting/
