FIELD LEVEL HAZARD ASSESSMENT (FLHA)
Replace fascia and soffits · Roofing · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client / general contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by
	

	Document number and revision
	

	Review date
	


2. JOB STEPS, HAZARDS AND CONTROLS
	#
	Job step
	Hazards
	Risk before
	Controls
	Risk after
	Responsible

	1
	Barricade below and set up a mobile scaffold or secured ladder
	Public entering the work area
Falling from a ladder
Falling from height
	Critical
	- Fence off the site with secure temporary fencing and lock the gates when you leave. [Engineering (guarding)]
- Give pedestrians a safe, marked path around the work, with ramps for strollers and wheelchairs. [Engineering (guarding)]
- Use hoarding, covered walkways or catch fans where work is above public areas. [Engineering]
- Put signs at each entry: site name, contact number and "No unauthorised entry". [Administrative]
- Make the site safe at the end of each day: cover holes, lower buckets and booms, remove ladders and lock tools away. [Administrative]
- Use a platform ladder, mobile scaffold or aerial work platform for longer jobs instead of a straight ladder. [Substitution]
- Use CSA Grade 1, 1A or 1AA ladders in good condition. Remove any damaged ladder from site. [Engineering]
- Set extension ladders at a 4 to 1 angle on firm, level ground, tied or footed, and reaching 1 metre above the landing. [Engineering]
- Use ladders only for short, light work. Do not carry heavy or awkward loads up a ladder. [Administrative]
- Keep three points of contact and your belt buckle between the side rails. Do not overreach. [Administrative]
- Do the work from the ground where you can, for example pre-assemble on the ground or use extension poles. [Elimination]
- Install guardrails or edge protection on all open edges before work starts. [Engineering (guarding)]
- Use a scaffold, mobile work platform or aerial work platform instead of working off a ladder. [Engineering]
- Where edge protection is not practical, use a fall restraint or fall arrest system on a rated anchor point. [Engineering]
- Fall protection plan in place where required. Workers trained in fall protection (Working at Heights training in Ontario). [Administrative]
- Have a rescue plan so a worker hanging in a harness can be brought down within minutes. [Administrative]
	Medium
	

	2
	Check soffit sheets for asbestos and old paint for lead before removing
	Disturbing asbestos
Lead paint dust and fumes
	Critical
	- Get an asbestos survey before work on buildings built before 1990. [Elimination]
- Seal off the work area and keep everyone else out. [Engineering (guarding)]
- If asbestos must be disturbed, keep it wet, use hand tools not power tools, and clean up with a HEPA vacuum. [Engineering]
- Follow your province's asbestos rules, including notification and trained or certified workers where required. [Administrative]
- In BC, a qualified person must inspect and write a hazardous materials report before demolition or renovation, and asbestos abatement must be done by a WorkSafeBC licensed contractor (since 1 January 2024). [Administrative]
- Stop work straight away if you find suspect asbestos. Do not touch it and tell your supervisor. [Administrative]
- Wear a fit-tested respirator suited to the work, and disposable coveralls. [PPE]
- Test old paint for lead before you sand, scrape, cut or heat it. [Elimination]
- Use wet scraping, chemical strippers or shrouded tools with extraction instead of dry sanding. Never burn off lead paint with an open flame. [Substitution]
- Seal off the work area with plastic sheeting and keep residents, children and pets out. [Engineering (guarding)]
- Clean up with a HEPA vacuum and wet wipes. Never dry sweep. [Engineering]
- Wash hands and face before eating, drinking or smoking. Change out of dusty clothes before going home. [Administrative]
- Wear a fit-tested respirator with P100 filters, disposable coveralls and gloves. [PPE]
	Medium
	

	3
	Remove gutters and old fascia boards, lowering them by hand
	Lifting and carrying heavy loads
Falling tools and materials
Cuts from sharp edges
	High
	- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Elimination]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Substitution]
- Use trolleys, pallet jacks, hoists, vacuum lifters or equipment instead of carrying by hand. [Engineering]
- Use a two-person lift for anything heavy, long or awkward. Plan the route first and clear it. [Administrative]
- Keep the load close, back straight and no twisting. Turn with your feet. [Administrative]
- Barricade and sign the drop zone under overhead work so nobody walks beneath. [Engineering (guarding)]
- Fit toe boards, kick plates and mesh screens on scaffolds and edges. [Engineering]
- Use catch fans, debris netting or covered walkways where people pass below. [Engineering]
- Tether hand tools when working at height. [Engineering]
- Keep platforms tidy. Do not stack materials near edges or above toe board height. [Administrative]
- Deburr or cover sharp edges, and fit edge protectors on exposed sheet metal. [Engineering]
- Use knives with retractable or self-retracting blades. [Engineering]
- Cut away from your body and keep your other hand clear. [Administrative]
- Put used blades in a blade bin or sharps container. [Administrative]
- Use two people to handle large sheets of metal or glass. [Administrative]
	Medium
	

	4
	Cut and fix new boards and soffit lining
	Saw cuts and kickback
Nail gun injuries
Wood and MDF dust
Loud noise
	High
	- Keep blade guards fitted and working, and use the riving knife on table saws. [Engineering]
- Use push sticks and clamps, and support long pieces so they do not pinch the blade. [Engineering]
- Use a sharp, undamaged blade made for the material. [Administrative]
- Stand to one side of the blade line, out of the kickback path. [Administrative]
- Use a nail gun with a sequential (single shot) trigger, not a contact or bump trigger. [Substitution]
- Disconnect the air or battery before clearing jams, adjusting or moving between work areas. [Engineering]
- Keep your free hand at least 30 cm from the nailing point. [Administrative]
- Never point the gun at anyone or carry it with your finger on the trigger. [Administrative]
- Buy pre-cut or pre-finished timber where you can. [Substitution]
- Cut outdoors or in a well-ventilated area away from others. [Engineering (guarding)]
- Use saws and sanders with dust collection connected to a HEPA vacuum. [Engineering]
- Clean up with a vacuum, not a broom or compressed air. [Administrative]
- Use quieter tools and methods, such as cut-to-size materials, low-noise machines and battery tools. [Substitution]
- Keep noisy equipment away from work areas, and use screens or distance between the noise and people. [Engineering (guarding)]
- Keep tools maintained and use mufflers on compressors and generators. [Engineering]
- Limit time on noisy tools and rotate workers. [Administrative]
	Medium
	

	5
	Refit gutters, clean up and remove access
	Poor housekeeping and waste
Falling from a ladder
	High
	- Order materials to size and send packaging back where you can. [Elimination]
- Put waste bins and chutes close to the work. [Engineering]
- Clean as you go, and do a full clean up at the end of each day. [Administrative]
- Keep exits, stairs and walkways clear at all times. [Administrative]
- Stack materials neatly on level ground, away from edges. [Administrative]
- Wear gloves when handling waste. [PPE]
- Do not stand on the top three rungs of an extension ladder or the top step of a stepladder. [Administrative]
- Check the ladder before each use: feet, rungs, side rails and locks. [Administrative]
- Wear non-slip safety boots with clean soles. [PPE]
- Falling from a ladder: see step 1 for the full controls [Administrative]
	Medium
	


3. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	CSA green triangle safety boots (CSA Z195)
Safety glasses (CSA Z94.3)
Work gloves
N95 respirator
Hearing protection
High-visibility vest (CSA Z96)
Hard hat (CSA Z94.1)
Respirator fit tested to CSA Z94.4 (P100 for dust, or the type the air test calls for)
Coveralls
Cut-resistant gloves
	Rolling scaffold (Provincial scaffold training)
Extension ladder
Circular saw
Nail gun
Hand tools
	None required


4. EMERGENCY ARRANGEMENTS
	Emergency number: 911
	

	Nearest hospital
	

	Muster point
	

	First aid attendant
	

	First aid kit location
	

	Fire extinguisher location
	


5. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Provincial occupational health and safety law (e.g. Ontario OHSA and O. Reg. 213/91, BC OHS Regulation, Alberta OHS Code).
Keep completed hazard assessments for at least 3 years (COR auditors sample the last 12 months). Review this FLHA and re-sign whenever the task, crew or conditions change.
6. END OF SHIFT REVIEW
	Area cleaned up and safe (yes / no)
	

	Permits closed
	

	Incidents or near misses
	

	Hazards remaining
	


7. SIGN-OFF
By signing below, each person confirms they have read and understood this FLHA and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/ca/flha/roofing/fascia-soffit-replacement/
