FIELD LEVEL HAZARD ASSESSMENT (FLHA)
Hot cutting with oxy-acetylene · Welding and fabrication · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client / general contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by
	

	Document number and revision
	

	Review date
	


2. JOB STEPS, HAZARDS AND CONTROLS
	#
	Job step
	Hazards
	Risk before
	Controls
	Risk after
	Responsible

	1
	Get a hot work permit and clear combustibles
	Fire from hot works
Flammable liquids and gases
	Critical
	- Use cold work methods where you can, such as bolting, press fittings or cutting with a saw instead of a torch. [Elimination]
- Move anything that can burn at least 10 metres away, or cover it with fire blankets. [Engineering (guarding)]
- Fire from hot works: see step 5 for the full controls [Administrative]
- Use non-flammable or water-based products where you can. [Substitution]
- Keep ignition sources away: no smoking, no hot work and no running engines near flammables. [Engineering (guarding)]
- Store fuels and solvents in approved, closed containers in a ventilated area away from the work. [Engineering]
- Refuel equipment outdoors with the engine off and cool. [Administrative]
- Keep only what you need for the day on site. [Administrative]
- Store gas cylinders upright, secured and outdoors. [Administrative]
- Keep a suitable fire extinguisher where flammables are used or stored. [Administrative]
- Wear chemical gloves and safety glasses when pouring or mixing. [PPE]
	Medium
	

	2
	Check hoses, regulators and flashback arrestors
	Flammable liquids and gases
Compressed air
	High
	- Flammable liquids and gases: see step 1 for the full controls [Administrative]
- Fit whip checks (safety cables) on hose joints and check hoses before use. [Engineering]
- Fit a pressure regulator and keep pressure to the tool's rating. [Engineering]
- Turn off and bleed the line before disconnecting. [Administrative]
- Never use compressed air to clean clothes or skin, or point it at anyone. [Administrative]
- Wear safety glasses and hearing protection. [PPE]
	Medium
	

	3
	Cut with goggles, keeping sparks away from others
	Burns from hot surfaces
Eye injuries
Welding and cutting fumes
	Critical
	- Isolate heating systems and let parts cool before you touch them. [Elimination]
- Fit guards or insulation on hot pipes and equipment. [Engineering]
- Mark hot items with chalk or a "HOT" sign so others know. [Administrative]
- Keep a first aid kit and cool running water nearby for burns. [Administrative]
- Wear heat-resistant gloves and long sleeves. [PPE]
- Use tool guards and screens to stop flying particles. [Engineering]
- Use dust extraction and water to keep dust out of the air. [Engineering]
- Keep others out of the area when cutting, grinding or chipping. [Administrative]
- Keep an eye wash station or eye wash bottles on site. [Administrative]
- Wear safety glasses at all times, goggles for dust and chemicals, and a face shield for grinding. [PPE]
- Remove paint, galvanising and coatings from the weld area first, or use a process that makes less fume. [Substitution]
- Use fume extraction (local exhaust ventilation) close to the weld. [Engineering]
- Weld outdoors or in a well-ventilated area, and keep your head out of the fume plume. [Engineering]
- Never weld or cut in a confined space without testing the air and using forced ventilation. [Administrative]
- Wear a powered air respirator or fitted respirator when extraction is not enough. [PPE]
	Medium
	

	4
	Never cut drums or tanks that held fuel
	Flammable liquids and gases
Fire and emergencies
	High
	- Flammable liquids and gases: see step 1 for the full controls [Administrative]
- Provide fire extinguishers suited to the site, checked and easy to reach. [Engineering]
- Keep exits and escape routes clear and signed. [Engineering]
- Have a site emergency plan: alarm, exits, assembly point and emergency contacts. [Administrative]
- Keep a stocked first aid kit and at least one trained first aider on site. [Administrative]
- Know the site address and how emergency services get in. Call 911. [Administrative]
- Go through the emergency plan with every worker and visitor at induction. [Administrative]
- Keep flammable materials and rubbish away from exits and escape routes. [Administrative]
	Medium
	

	5
	Shut down bottles and fire watch after
	Fire from hot works
	Critical
	- Use cold work methods where you can, such as bolting, press fittings or cutting with a saw instead of a torch. [Elimination]
- Move anything that can burn at least 10 metres away, or cover it with fire blankets. [Engineering (guarding)]
- Use fire-resistant screens to stop sparks reaching people or gaps in walls and floors. [Engineering]
- Get a hot work permit before starting. [Administrative]
- Keep a charged fire extinguisher and fire blanket at the work spot. [Administrative]
- Keep a fire watch during the work and for at least 60 minutes after you finish. [Administrative]
- Check for smouldering behind walls, in ceilings and under floors before you leave. [Administrative]
- Wear flame-resistant clothing, welding gloves and eye or face protection. [PPE]
	Medium
	


3. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Welding gloves
Safety goggles
CSA green triangle safety boots (CSA Z195)
Coveralls
Respirator fit tested to CSA Z94.4 (P100 for dust, or the type the air test calls for)
Face shield
Safety glasses (CSA Z94.3)
Hearing protection
Welding helmet (CSA Z94.3)
	Oxy-acetylene torch
Hand tools
	Hot work permit


4. EMERGENCY ARRANGEMENTS
	Emergency number: 911
	

	Nearest hospital
	

	Muster point
	

	First aid attendant
	

	First aid kit location
	

	Fire extinguisher location
	


5. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Provincial occupational health and safety law (e.g. Ontario OHSA and O. Reg. 213/91, BC OHS Regulation, Alberta OHS Code).
Keep completed hazard assessments for at least 3 years (COR auditors sample the last 12 months). Review this FLHA and re-sign whenever the task, crew or conditions change.
6. END OF SHIFT REVIEW
	Area cleaned up and safe (yes / no)
	

	Permits closed
	

	Incidents or near misses
	

	Hazards remaining
	


7. SIGN-OFF
By signing below, each person confirms they have read and understood this FLHA and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/ca/flha/welding-fabrication/oxy-cutting/
