RISK ASSESSMENT AND METHOD STATEMENT (RAMS)
Concrete driveway · Concreting · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company name and number
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client and principal contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by / approved by
	

	Document reference and revision
	

	Review date
	


2. RISK ASSESSMENT
	#
	Activity
	Hazards
	Who might be harmed
	Risk before
	Controls
	Risk after
	Responsible

	1
	Set up traffic and pedestrian control at the street
	Road traffic
Public entering the work area
	Workers, Road users, Public, Children
	Very high (15)
	- Do the work at low-traffic times, or close the road or lane with approval. [Eliminate]
- Put solid barriers between the work and traffic where speeds are high, not just cones. [Isolate]
- Use a truck-mounted attenuator or buffer vehicle on high speed roads. [Control (engineering)]
- Set up signs and cones to Chapter 8 (Traffic Signs Manual) by trained operatives. [Control (procedures)]
- Get a street works permit or licence from the highway authority before you start. [Control (procedures)]
- Park work vehicles to shield the work zone, with beacons on. [Control (procedures)]
- Wear Class 2 or 3 hi-vis clothing (EN ISO 20471). [PPE]
- Fence off the site with secure temporary fencing and lock the gates when you leave. [Isolate]
- Give pedestrians a safe, marked path around the work, with ramps for prams and wheelchairs. [Isolate]
- Public entering the work area: see step 6 for the full controls [Control (procedures)]
	Medium (5)
	

	2
	Locate services, then excavate and level the base with the skid steer
	Hitting underground services
Being hit by mobile plant
	Workers, Public, Visitors
	Very high (15)
	- Keep machine buckets well clear of marked services and use a spotter. [Isolate]
- Do a CAT and Genny scan before digging and mark services on the ground. [Control (engineering)]
- Hand dig trial holes to find services before machine digging (safe digging practice). [Control (engineering)]
- Get utility plans before digging and check them against what you see on site. [Control (procedures)]
- Keep plans or locate tickets on site and check them again if the work area grows. [Control (procedures)]
- If you hit a service, stop, get everyone clear, and call the owner and emergency services. [Control (procedures)]
- Wear safety boots, gloves and hi-vis when digging. [PPE]
- Separate people and plant with barriers, exclusion zones and marked walkways. [Isolate]
- Use plant with working reversing alarms, cameras and lights. [Control (engineering)]
- Have a traffic management plan showing plant routes, loading areas and pedestrian paths. [Control (procedures)]
- Use a spotter when reversing or working near people. [Control (procedures)]
- Make eye contact with the operator before going near. Stay out of the swing radius. [Control (procedures)]
- Operators hold a CPCS, NPORS or equal card for the plant they use. [Control (procedures)]
- Do a pre-start check on each machine every day and record it. [Control (procedures)]
- Wear hi-vis clothing and a hard hat. [PPE]
	Medium (5)
	

	3
	Compact base, set forms and rebar
	Hand-arm and whole-body vibration
Loud noise
Impalement on rebar
Lifting and carrying heavy loads
	Workers, People nearby
	High (12)
	- Use low-vibration tools and methods, such as a breaker on an excavator instead of a hand jackhammer. [Reduce / substitute]
- Keep tools sharp and well maintained, and use anti-vibration handles and seats. [Control (engineering)]
- Limit trigger time using the HSE vibration calculator to stay below the exposure action value, and rotate workers. [Control (procedures)]
- Keep hands warm and dry, and take regular breaks. [Control (procedures)]
- Use quieter tools and methods, such as cut-to-size materials, low-noise machines and battery tools. [Reduce / substitute]
- Keep noisy plant away from work areas, and use screens or distance between the noise and people. [Isolate]
- Keep tools maintained and use mufflers on compressors and generators. [Control (engineering)]
- Limit time on noisy tools and rotate workers. [Control (procedures)]
- Assess noise. At 85 dB(A) or more, hearing protection is required and the zone must be marked. [Control (procedures)]
- Cover or cap all exposed bar ends with approved caps or covers. [Control (engineering)]
- Bend bars over where the design allows. [Control (engineering)]
- Use edge protection near starter bars so nobody can fall onto them. [Control (engineering)]
- Keep walkways clear of exposed bars and mark the hazard. [Control (procedures)]
- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Eliminate]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Reduce / substitute]
- Use trolleys, pallet jacks, hoists, vacuum lifters or plant instead of carrying by hand. [Control (engineering)]
- Use a two-person lift for anything heavy, long or awkward. Plan the route first and clear it. [Control (procedures)]
	Medium (6)
	

	4
	Pour and finish the concrete
	Wet concrete and cement burns
Heat stress
Sun exposure (UV)
	Workers
	High (12)
	- Use long-handled tools and pumps to cut down contact. [Control (engineering)]
- Wash concrete off skin straight away with clean water. [Control (procedures)]
- Have clean water and eye wash where concrete or mortar is mixed and used. [Control (procedures)]
- Do a COSHH assessment for cement, lime and mortar, and check hands regularly for early signs of dermatitis. [Control (procedures)]
- Wear waterproof gloves, long sleeves and waterproof boots with trousers worn over the top. [PPE]
- Wear safety glasses or goggles to stop splashes. [PPE]
- Schedule heavy work for the cooler part of the day. [Eliminate]
- Provide shade over work and rest areas, and fans or cooling in roof spaces. [Control (engineering)]
- Supply cool drinking water close by and drink a cup every 15 to 20 minutes. [Control (procedures)]
- Take regular rest breaks in the shade, more often as it gets hotter. [Control (procedures)]
- Let new and returning workers build up to full work in the heat over about a week. [Control (procedures)]
- Plan outdoor work for early morning or late afternoon when UV is lower. [Eliminate]
- Put shade covers over fixed work areas. [Control (engineering)]
- Check the UV index each day. Use sun protection when it is 3 or higher. [Control (procedures)]
- Check your skin regularly and see a doctor about any new or changing spots. [Control (procedures)]
- Wear a broad-brim hat or hard hat brim, long sleeves, sunglasses and SPF 30 or higher sunscreen, reapplied every 2 hours. [PPE]
	Medium (8)
	

	5
	Saw cut control joints with water suppression
	Silica dust from concrete, brick, stone and tiles
Saw cuts and kickback
Loud noise
	Workers, People nearby
	Very high (20)
	- Order materials cut to size, or use low-dust methods such as score and snap or a block splitter. [Reduce / substitute]
- Cut outdoors or in a separate area, with other people well away and upwind. [Isolate]
- Use water on the blade or on-tool dust extraction connected to an H-class vacuum. [Control (engineering)]
- Clean up with a vacuum or wet methods. Never dry sweep or use compressed air. [Control (procedures)]
- Do a COSHH assessment and keep exposure below the workplace exposure limit (0.1 mg/m3 respirable crystalline silica, 8 hours). [Control (procedures)]
- Workers regularly exposed to silica dust get health surveillance (COSHH reg 11, HSE G404). [Control (procedures)]
- Wear a fit-tested FFP3 mask. [PPE]
- Keep blade guards fitted and working, and use the riving knife on table saws. [Control (engineering)]
- Use push sticks and clamps, and support long pieces so they do not pinch the blade. [Control (engineering)]
- Use a sharp, undamaged blade made for the material. [Control (procedures)]
- Stand to one side of the blade line, out of the kickback path. [Control (procedures)]
- Let the blade stop fully before reaching in or putting the saw down. [Control (procedures)]
- If you have to shout to be heard by someone 2 metres away, the noise is probably 85 dB(A) or more: wear hearing protection. [Control (procedures)]
- Wear earplugs or earmuffs rated for the noise. [PPE]
- Loud noise: see step 3 for the full controls [Control (procedures)]
	Medium (8)
	

	6
	Clean up, wash out away from drains and barricade until cured
	Poor housekeeping and waste
Public entering the work area
	Workers, Visitors, Public, Children
	High (12)
	- Order materials to size and send packaging back where you can. [Eliminate]
- Put skips and waste chutes close to the work. [Control (engineering)]
- Clean as you go, and do a full clean up at the end of each day. [Control (procedures)]
- Keep exits, stairs and walkways clear at all times. [Control (procedures)]
- Stack materials neatly on level ground, away from edges. [Control (procedures)]
- Use a registered waste carrier and keep waste transfer notes for at least 2 years. Keep hazardous waste such as asbestos separate, with consignment notes (special waste in Scotland). [Control (procedures)]
- Wear gloves when handling waste. [PPE]
- Fence off the site with secure temporary fencing and lock the gates when you leave. [Isolate]
- Give pedestrians a safe, marked path around the work, with ramps for prams and wheelchairs. [Isolate]
- Use hoarding, covered walkways or catch fans where work is above public areas. [Control (engineering)]
- Put signs at each entry: site name, contact number and "No unauthorised entry". [Control (procedures)]
- Make the site safe at the end of each day: cover holes, lower plant, remove ladders and lock tools away. [Control (procedures)]
- Use a spotter when moving plant or materials across public paths. [Control (procedures)]
	Low (4)
	


3. METHOD STATEMENT: SEQUENCE OF WORK
1. Set up traffic and pedestrian control at the street
2. Locate services, then excavate and level the base with the skid steer
3. Compact base, set forms and rebar
4. Pour and finish the concrete
5. Saw cut control joints with water suppression
6. Clean up, wash out away from drains and barricade until cured
4. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Safety boots
Hi-vis vest
Chemical-resistant gloves
Safety glasses
Ear defenders
Sun protection (sunscreen and neck cover)
Safety helmet
Rigger gloves
Safety goggles
Knee pads
Half-mask respirator (P3 filters)
FFP3 dust mask
	Skid steer loader (CPCS or NPORS skid steer card)
Wacker plate
Cut-off saw (Stihl saw)
Hand tools
Concrete pump
	None required


5. EMERGENCY ARRANGEMENTS
	Emergency number: 999
	

	Nearest A&E
	

	Assembly point
	

	First aider
	

	First aid kit location
	

	Fire extinguisher location
	


6. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Management of Health and Safety at Work Regulations 1999 and the Construction (Design and Management) Regulations 2015.
Keep this RAMS, every revision and the signed briefing register with the site file for the length of the job, and keep a copy in your records afterwards.
7. BRIEFING REGISTER
By signing below, each person confirms they have read and understood this RAMS and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/uk/rams/concreting/driveway-concreting/
