RISK ASSESSMENT AND METHOD STATEMENT (RAMS)
Build a garden annexe · General building · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company name and number
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client and principal contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by / approved by
	

	Document reference and revision
	

	Review date
	


2. RISK ASSESSMENT
	#
	Activity
	Hazards
	Who might be harmed
	Risk before
	Controls
	Risk after
	Responsible

	1
	Set up fencing and keep the main house occupants away from the work
	Public entering the work area
Working in an occupied home or building
	Public, Children, Workers, Residents, Staff
	High (12)
	- Fence off the site with secure temporary fencing and lock the gates when you leave. [Isolate]
- Give pedestrians a safe, marked path around the work, with ramps for prams and wheelchairs. [Isolate]
- Use hoarding, covered walkways or catch fans where work is above public areas. [Control (engineering)]
- Put signs at each entry: site name, contact number and "No unauthorised entry". [Control (procedures)]
- Make the site safe at the end of each day: cover holes, lower plant, remove ladders and lock tools away. [Control (procedures)]
- Use a spotter when moving plant or materials across public paths. [Control (procedures)]
- Plan noisy, dusty or risky work for when the building is empty. [Eliminate]
- Close off the work area with barriers, plastic sheeting or locked doors, and put up signs. [Isolate]
- Keep fire exits and paths clear at all times. [Control (procedures)]
- Tell occupants before you turn off power, water or gas, and before noisy or dusty work. [Control (procedures)]
- Lock away tools, chemicals and materials each day, out of reach of children. [Control (procedures)]
- Clean up dust and debris at the end of each day. [Control (procedures)]
	Low (4)
	

	2
	Excavate and pour the slab
	Hitting underground services
Being hit by mobile plant
Wet concrete and cement burns
	Workers, Public, Visitors
	Very high (15)
	- Keep machine buckets well clear of marked services and use a spotter. [Isolate]
- Do a CAT and Genny scan before digging and mark services on the ground. [Control (engineering)]
- Hand dig trial holes to find services before machine digging (safe digging practice). [Control (engineering)]
- Get utility plans before digging and check them against what you see on site. [Control (procedures)]
- Keep plans or locate tickets on site and check them again if the work area grows. [Control (procedures)]
- Separate people and plant with barriers, exclusion zones and marked walkways. [Isolate]
- Use plant with working reversing alarms, cameras and lights. [Control (engineering)]
- Have a traffic management plan showing plant routes, loading areas and pedestrian paths. [Control (procedures)]
- Use a spotter when reversing or working near people. [Control (procedures)]
- Make eye contact with the operator before going near. Stay out of the swing radius. [Control (procedures)]
- Use long-handled tools and pumps to cut down contact. [Control (engineering)]
- Wash concrete off skin straight away with clean water. [Control (procedures)]
- Have clean water and eye wash where concrete or mortar is mixed and used. [Control (procedures)]
- Do a COSHH assessment for cement, lime and mortar, and check hands regularly for early signs of dermatitis. [Control (procedures)]
- Wear waterproof gloves, long sleeves and waterproof boots with trousers worn over the top. [PPE]
- Wear safety glasses or goggles to stop splashes. [PPE]
	Medium (5)
	

	3
	Frame and roof with edge protection
	Falling from height
Falling from a roof edge
Nail gun injuries
	Workers, People below, People nearby
	Very high (20)
	- Do the work from the ground where you can, for example pre-assemble on the ground or use extension poles. [Eliminate]
- Install guardrails or edge protection on all open edges before work starts. [Isolate]
- Use a scaffold, mobile tower or MEWP instead of working off a ladder. [Control (engineering)]
- Where edge protection is not practical, use a fall restraint or fall arrest system on a rated anchor point. [Control (engineering)]
- Have a rescue plan so a worker hanging in a harness can be brought down within minutes. [Control (procedures)]
- Do what you can from the ground or from a scaffold at the gutter line, for example pre-assemble parts on the ground. [Eliminate]
- Install edge protection or guardrails on all open roof edges before work starts. [Isolate]
- Use a perimeter scaffold with handrails and toe boards along the eaves where practical. [Control (engineering)]
- Where guardrails cannot be fitted, use fall restraint on certified roof anchors so workers cannot reach the edge. [Control (engineering)]
- Use one safe, controlled access point and keep others off the roof. [Control (procedures)]
- Use a nail gun with a sequential (single shot) trigger, not a contact or bump trigger. [Reduce / substitute]
- Disconnect the air or battery before clearing jams, adjusting or moving between work areas. [Control (engineering)]
- Keep your free hand at least 30 cm from the nailing point. [Control (procedures)]
- Never point the gun at anyone or carry it with your finger on the trigger. [Control (procedures)]
- Train new users before they use a nail gun, and check for pipes, cables and metal behind the surface. [Control (procedures)]
	Medium (8)
	

	4
	Connect services by competent trades: a Gas Safe registered engineer for gas and a qualified electrician for electrics
	Electric shock from live wiring
Gas and fuel lines
Trench or excavation collapse
	Workers, Occupants, Public
	Very high (15)
	- Isolate the power before any work. Do not work live. [Eliminate]
- Lock out and tag the isolation point with your own personal lock and danger tag. [Isolate]
- Prove dead at the point of work with an approved voltage indicator (GS38), and prove the tester before and after. [Control (engineering)]
- Only competent, qualified electricians do electrical work, following a safe isolation procedure. [Control (procedures)]
- Check for back feeds from solar, batteries and generators that can keep a circuit live after the main switch is off. [Control (procedures)]
- Isolate and purge the line before work, with the owner's approval. [Eliminate]
- Lock off and tag the isolation valve. [Isolate]
- Check for leaks with a gas detector before and during work, and ventilate the area. [Control (engineering)]
- Only Gas Safe registered engineers work on gas fittings. [Control (procedures)]
- Remove ignition sources: no smoking, no hot work and no sparking tools near the line. [Control (procedures)]
- Use methods that keep people out of the trench, such as directional boring or working from the surface. [Eliminate]
- Barricade or cover the excavation so people and plant cannot fall in. [Isolate]
- Support or batter back the sides of any excavation where collapse could happen. Use trench boxes or sheet piling for deeper trenches. [Control (engineering)]
- Keep spoil, materials and plant at least 1 metre back from the edge. [Control (engineering)]
- Provide a safe way in and out, such as a ladder near where people work. [Control (engineering)]
- Inspect the excavation at the start of each shift and after rain or anything that could weaken it. Record it. [Control (procedures)]
	Medium (5)
	

	5
	Fit out and clean up
	General dust
Poor housekeeping and waste
	Workers, Occupants, Visitors
	Medium (8)
	- Use low-dust products, such as dust-reduced or pre-mixed compounds. [Reduce / substitute]
- Seal off the work area with plastic sheeting in occupied buildings. [Isolate]
- Use tools with dust extraction and a vacuum for clean up. [Control (engineering)]
- Lightly mist the area with water to keep dust down, away from anything electrical. [Control (engineering)]
- Never dry sweep or blow dust off with compressed air. [Control (procedures)]
- Wear a dust mask and safety glasses. [PPE]
- Order materials to size and send packaging back where you can. [Eliminate]
- Put skips and waste chutes close to the work. [Control (engineering)]
- Clean as you go, and do a full clean up at the end of each day. [Control (procedures)]
- Keep exits, stairs and walkways clear at all times. [Control (procedures)]
- Stack materials neatly on level ground, away from edges. [Control (procedures)]
- Use a registered waste carrier and keep waste transfer notes for at least 2 years. Keep hazardous waste such as asbestos separate, with consignment notes (special waste in Scotland). [Control (procedures)]
- Wear gloves when handling waste. [PPE]
	Low (4)
	


3. METHOD STATEMENT: SEQUENCE OF WORK
1. Set up fencing and keep the main house occupants away from the work
2. Excavate and pour the slab
3. Frame and roof with edge protection
4. Connect services by competent trades: a Gas Safe registered engineer for gas and a qualified electrician for electrics
5. Fit out and clean up
4. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Safety boots
Hi-vis vest
Safety helmet
Safety glasses
Ear defenders
Full body harness and lanyard
FFP3 dust mask
Chemical-resistant gloves
Safety goggles
Knee pads
Sun protection (sunscreen and neck cover)
Rigger gloves
	Excavator (360) (CPCS or NPORS excavator card)
Concrete pump
Tube and fitting or system scaffold (CISRS scaffolder card to erect, alter or dismantle)
Nail gun
Circular saw
	Roof access permit
Work at height permit


5. EMERGENCY ARRANGEMENTS
	Emergency number: 999
	

	Nearest A&E
	

	Assembly point
	

	First aider
	

	First aid kit location
	

	Fire extinguisher location
	


6. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Management of Health and Safety at Work Regulations 1999 and the Construction (Design and Management) Regulations 2015.
Keep this RAMS, every revision and the signed briefing register with the site file for the length of the job, and keep a copy in your records afterwards.
7. BRIEFING REGISTER
By signing below, each person confirms they have read and understood this RAMS and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/uk/rams/general-building/granny-flat-construction/
