RISK ASSESSMENT AND METHOD STATEMENT (RAMS)
Kitchen renovation · General building · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company name and number
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client and principal contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by / approved by
	

	Document reference and revision
	

	Review date
	


2. RISK ASSESSMENT
	#
	Activity
	Hazards
	Who might be harmed
	Risk before
	Controls
	Risk after
	Responsible

	1
	Check for asbestos and isolate power, gas and water
	Disturbing asbestos
Electric shock from live wiring
Gas and fuel lines
	Workers, Occupants, Public
	Very high (15)
	- Before work on any building built before 2000, check the refurbishment and demolition asbestos survey for the work area (HSE HSG264). If there is none, presume asbestos is present or have it sampled before you start. [Eliminate]
- Seal off the work area and keep everyone else out. [Isolate]
- If asbestos must be disturbed, keep it wet, use hand tools not power tools, and clean up with an H-class vacuum. [Control (engineering)]
- Most asbestos insulation, coatings and insulating board need a licensed contractor. Notifiable non-licensed work is notified to HSE before it starts. Other work needs trained workers and controls. [Control (procedures)]
- Stop work straight away if you find suspect asbestos. Do not touch it and tell your supervisor. [Control (procedures)]
- Wear a fit-tested FFP3 mask (or better) and disposable type 5 coveralls. [PPE]
- Isolate the power before any work. Do not work live. [Eliminate]
- Lock out and tag the isolation point with your own personal lock and danger tag. [Isolate]
- Prove dead at the point of work with an approved voltage indicator (GS38), and prove the tester before and after. [Control (engineering)]
- Only competent, qualified electricians do electrical work, following a safe isolation procedure. [Control (procedures)]
- Check for back feeds from solar, batteries and generators that can keep a circuit live after the main switch is off. [Control (procedures)]
- Isolate and purge the line before work, with the owner's approval. [Eliminate]
- Lock off and tag the isolation valve. [Isolate]
- Check for leaks with a gas detector before and during work, and ventilate the area. [Control (engineering)]
- Only Gas Safe registered engineers work on gas fittings. [Control (procedures)]
- Remove ignition sources: no smoking, no hot work and no sparking tools near the line. [Control (procedures)]
	Medium (5)
	

	2
	Remove old cabinets and appliances with two people
	Lifting and carrying heavy loads
Cuts from sharp edges
	Workers
	High (12)
	- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Eliminate]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Reduce / substitute]
- Use trolleys, pallet jacks, hoists, vacuum lifters or plant instead of carrying by hand. [Control (engineering)]
- Use a two-person lift for anything heavy, long or awkward. Plan the route first and clear it. [Control (procedures)]
- Keep the load close, back straight and no twisting. Turn with your feet. [Control (procedures)]
- Rotate tasks and take breaks on long lifting jobs. [Control (procedures)]
- Wear gloves for grip and safety boots to protect your feet. [PPE]
- Deburr or cover sharp edges, and fit edge protectors on exposed sheet metal. [Control (engineering)]
- Use knives with retractable or self-retracting blades. [Control (engineering)]
- Cut away from your body and keep your other hand clear. [Control (procedures)]
- Put used blades in a blade bin or sharps container. [Control (procedures)]
- Use two people to handle large sheets of metal or glass. [Control (procedures)]
- Wear cut-resistant gloves and long sleeves. [PPE]
	Medium (6)
	

	3
	Patch walls and run new services
	General dust
Electric shock from live wiring
	Workers, Occupants
	Very high (15)
	- Use low-dust products, such as dust-reduced or pre-mixed compounds. [Reduce / substitute]
- Seal off the work area with plastic sheeting in occupied buildings. [Isolate]
- Use tools with dust extraction and a vacuum for clean up. [Control (engineering)]
- Lightly mist the area with water to keep dust down, away from anything electrical. [Control (engineering)]
- Never dry sweep or blow dust off with compressed air. [Control (procedures)]
- Wear a dust mask and safety glasses. [PPE]
- If live work cannot be avoided, use a permit, a safety observer and insulated tools. [Control (procedures)]
- Wear insulated gloves, arc-rated clothing and a face shield when testing or working near live parts. [PPE]
- Electric shock from live wiring: see step 1 for the full controls [Control (procedures)]
	Medium (5)
	

	4
	Install cabinets and benchtops, wet cutting stone
	Silica dust from concrete, brick, stone and tiles
Lifting and carrying heavy loads
Saw cuts and kickback
	Workers, People nearby
	Very high (20)
	- Order materials cut to size, or use low-dust methods such as score and snap or a block splitter. [Reduce / substitute]
- Cut outdoors or in a separate area, with other people well away and upwind. [Isolate]
- Use water on the blade or on-tool dust extraction connected to an H-class vacuum. [Control (engineering)]
- Clean up with a vacuum or wet methods. Never dry sweep or use compressed air. [Control (procedures)]
- Do a COSHH assessment and keep exposure below the workplace exposure limit (0.1 mg/m3 respirable crystalline silica, 8 hours). [Control (procedures)]
- Workers regularly exposed to silica dust get health surveillance (COSHH reg 11, HSE G404). [Control (procedures)]
- Wear a fit-tested FFP3 mask. [PPE]
- Lifting and carrying heavy loads: see step 2 for the full controls [Control (procedures)]
- Keep blade guards fitted and working, and use the riving knife on table saws. [Control (engineering)]
- Use push sticks and clamps, and support long pieces so they do not pinch the blade. [Control (engineering)]
- Use a sharp, undamaged blade made for the material. [Control (procedures)]
- Stand to one side of the blade line, out of the kickback path. [Control (procedures)]
- Let the blade stop fully before reaching in or putting the saw down. [Control (procedures)]
	Medium (8)
	

	5
	Fit off, test gas and power, and clean up
	Gas and fuel lines
Electric shock from live wiring
Poor housekeeping and waste
	Workers, Occupants, Public, Visitors
	Very high (15)
	- Know where the shut-off valve is and what to do if a leak happens. [Control (procedures)]
- Wear safety glasses and gloves, and keep a fire extinguisher close by. [PPE]
- Gas and fuel lines: see step 1 for the full controls [Control (procedures)]
- Electric shock from live wiring: see step 1 for the full controls [Control (procedures)]
- Order materials to size and send packaging back where you can. [Eliminate]
- Put skips and waste chutes close to the work. [Control (engineering)]
- Clean as you go, and do a full clean up at the end of each day. [Control (procedures)]
- Keep exits, stairs and walkways clear at all times. [Control (procedures)]
- Stack materials neatly on level ground, away from edges. [Control (procedures)]
- Use a registered waste carrier and keep waste transfer notes for at least 2 years. Keep hazardous waste such as asbestos separate, with consignment notes (special waste in Scotland). [Control (procedures)]
	Medium (5)
	


3. METHOD STATEMENT: SEQUENCE OF WORK
1. Check for asbestos and isolate power, gas and water
2. Remove old cabinets and appliances with two people
3. Patch walls and run new services
4. Install cabinets and benchtops, wet cutting stone
5. Fit off, test gas and power, and clean up
4. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Safety boots
Safety glasses
FFP3 dust mask
Ear defenders
Rigger gloves
Half-mask respirator (P3 filters)
Coveralls
Cut-resistant gloves
	Power drill
Circular saw
SDS drill
H-class dust extractor
Hand tools
	None required


5. EMERGENCY ARRANGEMENTS
	Emergency number: 999
	

	Nearest A&E
	

	Assembly point
	

	First aider
	

	First aid kit location
	

	Fire extinguisher location
	


6. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Management of Health and Safety at Work Regulations 1999 and the Construction (Design and Management) Regulations 2015.
Keep this RAMS, every revision and the signed briefing register with the site file for the length of the job, and keep a copy in your records afterwards.
7. BRIEFING REGISTER
By signing below, each person confirms they have read and understood this RAMS and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/uk/rams/general-building/kitchen-renovation/
