RISK ASSESSMENT AND METHOD STATEMENT (RAMS)
Minor maintenance and repairs · General building · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company name and number
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client and principal contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by / approved by
	

	Document reference and revision
	

	Review date
	


2. RISK ASSESSMENT
	#
	Activity
	Hazards
	Who might be harmed
	Risk before
	Controls
	Risk after
	Responsible

	1
	Talk to the occupants and set up a tidy work area
	Working in an occupied home or building
Slips and trips
	Residents, Children, Staff, Workers, Visitors, Public
	Medium (9)
	- Plan noisy, dusty or risky work for when the building is empty. [Eliminate]
- Close off the work area with barriers, plastic sheeting or locked doors, and put up signs. [Isolate]
- Keep fire exits and paths clear at all times. [Control (procedures)]
- Tell occupants before you turn off power, water or gas, and before noisy or dusty work. [Control (procedures)]
- Lock away tools, chemicals and materials each day, out of reach of children. [Control (procedures)]
- Clean up dust and debris at the end of each day. [Control (procedures)]
- Plan walkways and keep them clear of materials, hoses and leads. [Eliminate]
- Run leads and hoses overhead on hooks or stands, or along walls, not across walkways. [Control (engineering)]
- Fill or cover holes, and lay boards or mats on muddy access paths. [Control (engineering)]
- Clean up offcuts, packaging and spills as you go, not at the end of the day. [Control (procedures)]
- Keep work areas, stairs and access paths well lit. [Control (procedures)]
- Wear safety boots with good grip, laced up. [PPE]
	Low (4)
	

	2
	Check for asbestos and lead paint before drilling or cutting older buildings
	Disturbing asbestos
Lead paint dust and fumes
	Workers, Occupants, Public, Residents, Children
	Very high (15)
	- Before work on any building built before 2000, check the refurbishment and demolition asbestos survey for the work area (HSE HSG264). If there is none, presume asbestos is present or have it sampled before you start. [Eliminate]
- Seal off the work area and keep everyone else out. [Isolate]
- If asbestos must be disturbed, keep it wet, use hand tools not power tools, and clean up with an H-class vacuum. [Control (engineering)]
- Most asbestos insulation, coatings and insulating board need a licensed contractor. Notifiable non-licensed work is notified to HSE before it starts. Other work needs trained workers and controls. [Control (procedures)]
- Stop work straight away if you find suspect asbestos. Do not touch it and tell your supervisor. [Control (procedures)]
- Wear a fit-tested FFP3 mask (or better) and disposable type 5 coveralls. [PPE]
- Test old paint for lead before you sand, scrape, cut or heat it. [Eliminate]
- Use wet scraping, chemical strippers or shrouded tools with extraction instead of dry sanding. Never burn off lead paint with an open flame. [Reduce / substitute]
- Seal off the work area with plastic sheeting and keep residents, children and pets out. [Isolate]
- Clean up with an H-class vacuum and wet wipes. Never dry sweep. [Control (engineering)]
- Wash hands and face before eating, drinking or smoking. Change out of dusty clothes before going home. [Control (procedures)]
- Wear an FFP3 mask, disposable coveralls and gloves. [PPE]
	Medium (5)
	

	3
	Isolate any services you will work near
	Electric shock from live wiring
Gas and fuel lines
	Workers, Occupants, Public
	Very high (15)
	- Isolate the power before any work. Do not work live. [Eliminate]
- Lock out and tag the isolation point with your own personal lock and danger tag. [Isolate]
- Prove dead at the point of work with an approved voltage indicator (GS38), and prove the tester before and after. [Control (engineering)]
- Only competent, qualified electricians do electrical work, following a safe isolation procedure. [Control (procedures)]
- Check for back feeds from solar, batteries and generators that can keep a circuit live after the main switch is off. [Control (procedures)]
- If live work cannot be avoided, use a permit, a safety observer and insulated tools. [Control (procedures)]
- Wear insulated gloves, arc-rated clothing and a face shield when testing or working near live parts. [PPE]
- Isolate and purge the line before work, with the owner's approval. [Eliminate]
- Lock off and tag the isolation valve. [Isolate]
- Check for leaks with a gas detector before and during work, and ventilate the area. [Control (engineering)]
- Only Gas Safe registered engineers work on gas fittings. [Control (procedures)]
- Remove ignition sources: no smoking, no hot work and no sparking tools near the line. [Control (procedures)]
- Know where the shut-off valve is and what to do if a leak happens. [Control (procedures)]
- Wear safety glasses and gloves, and keep a fire extinguisher close by. [PPE]
	Medium (5)
	

	4
	Use the right ladder and keep three points of contact
	Falling from a ladder
	Workers
	High (12)
	- Use a podium step, mobile tower or MEWP for longer jobs instead of a straight ladder. [Reduce / substitute]
- Use EN 131 professional ladders in good condition. Remove any damaged ladder from site. [Control (engineering)]
- Set extension ladders at a 4 to 1 angle on firm, level ground, tied or footed, and reaching 1 metre above the landing. [Control (engineering)]
- Use ladders only for short, light work (about 30 minutes in one spot). Do not carry heavy or awkward loads up a ladder. [Control (procedures)]
- Keep three points of contact and your belt buckle between the stiles. Do not overreach. [Control (procedures)]
- Do not work off the top three rungs of a leaning ladder. On a stepladder, do not stand on the top two steps (top three on swing-back or double-sided steps) unless there is a suitable handhold. [Control (procedures)]
- Check the ladder before each use: feet, rungs, stiles and locks. [Control (procedures)]
- Wear non-slip safety boots with clean soles. [PPE]
	Medium (8)
	

	5
	Do the repair with guards and PPE on tools
	Injury from power tools
Saw cuts and kickback
General dust
	Workers, People nearby, Occupants
	High (12)
	- Keep all guards fitted and working. Never tie back or remove a guard. [Control (engineering)]
- Clamp or secure the work piece. Do not hold it by hand. [Control (engineering)]
- Only trained, competent people use power tools, following the maker's instructions. [Control (procedures)]
- Check tools before use. Unplug or remove the battery before changing blades or bits. [Control (procedures)]
- No loose clothing, jewellery or long hair near spinning parts. [Control (procedures)]
- Keep blade guards fitted and working, and use the riving knife on table saws. [Control (engineering)]
- Use push sticks and clamps, and support long pieces so they do not pinch the blade. [Control (engineering)]
- Use a sharp, undamaged blade made for the material. [Control (procedures)]
- Stand to one side of the blade line, out of the kickback path. [Control (procedures)]
- Let the blade stop fully before reaching in or putting the saw down. [Control (procedures)]
- Use low-dust products, such as dust-reduced or pre-mixed compounds. [Reduce / substitute]
- Seal off the work area with plastic sheeting in occupied buildings. [Isolate]
- Use tools with dust extraction and a vacuum for clean up. [Control (engineering)]
- Lightly mist the area with water to keep dust down, away from anything electrical. [Control (engineering)]
- Never dry sweep or blow dust off with compressed air. [Control (procedures)]
	Medium (8)
	

	6
	Tell someone where you are if working alone, then clean up
	Working alone
Poor housekeeping and waste
	Workers, Visitors
	Medium (8)
	- Do not do high risk work alone: work at height, confined spaces, live electrical or trenches. [Eliminate]
- Set a check-in system: call or text at set times, and someone follows up if there is no reply. [Control (procedures)]
- Tell someone where you are working and when you expect to finish. [Control (procedures)]
- Carry a charged phone. Use a personal alarm or GPS device where there is no signal. [Control (procedures)]
- Keep a first aid kit on hand and know the site address for emergency services. [Control (procedures)]
- Order materials to size and send packaging back where you can. [Eliminate]
- Put skips and waste chutes close to the work. [Control (engineering)]
- Clean as you go, and do a full clean up at the end of each day. [Control (procedures)]
- Keep exits, stairs and walkways clear at all times. [Control (procedures)]
- Stack materials neatly on level ground, away from edges. [Control (procedures)]
- Use a registered waste carrier and keep waste transfer notes for at least 2 years. Keep hazardous waste such as asbestos separate, with consignment notes (special waste in Scotland). [Control (procedures)]
- Wear gloves when handling waste. [PPE]
	Low (4)
	


3. METHOD STATEMENT: SEQUENCE OF WORK
1. Talk to the occupants and set up a tidy work area
2. Check for asbestos and lead paint before drilling or cutting older buildings
3. Isolate any services you will work near
4. Use the right ladder and keep three points of contact
5. Do the repair with guards and PPE on tools
6. Tell someone where you are if working alone, then clean up
4. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Safety boots
Safety glasses
Rigger gloves
FFP3 dust mask
Half-mask respirator (P3 filters)
Coveralls
Safety helmet
Ear defenders
	Hand tools
Power drill
Stepladder
Circular saw
	None required


5. EMERGENCY ARRANGEMENTS
	Emergency number: 999
	

	Nearest A&E
	

	Assembly point
	

	First aider
	

	First aid kit location
	

	Fire extinguisher location
	


6. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Management of Health and Safety at Work Regulations 1999 and the Construction (Design and Management) Regulations 2015.
Keep this RAMS, every revision and the signed briefing register with the site file for the length of the job, and keep a copy in your records afterwards.
7. BRIEFING REGISTER
By signing below, each person confirms they have read and understood this RAMS and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/uk/rams/general-building/minor-maintenance-repairs/
