RISK ASSESSMENT AND METHOD STATEMENT (RAMS)
Lay turf · Landscaping · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company name and number
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client and principal contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by / approved by
	

	Document reference and revision
	

	Review date
	


2. RISK ASSESSMENT
	#
	Activity
	Hazards
	Who might be harmed
	Risk before
	Controls
	Risk after
	Responsible

	1
	Locate irrigation and services before levelling
	Hitting underground services
	Workers, Public
	Very high (15)
	- Keep machine buckets well clear of marked services and use a spotter. [Isolate]
- Do a CAT and Genny scan before digging and mark services on the ground. [Control (engineering)]
- Hand dig trial holes to find services before machine digging (safe digging practice). [Control (engineering)]
- Get utility plans before digging and check them against what you see on site. [Control (procedures)]
- Keep plans or locate tickets on site and check them again if the work area grows. [Control (procedures)]
- If you hit a service, stop, get everyone clear, and call the owner and emergency services. [Control (procedures)]
- Wear safety boots, gloves and hi-vis when digging. [PPE]
	Medium (5)
	

	2
	Level and prepare soil with the skid steer
	Being hit by mobile plant
General dust
	Workers, Visitors, Public, Occupants
	Very high (15)
	- Separate people and plant with barriers, exclusion zones and marked walkways. [Isolate]
- Use plant with working reversing alarms, cameras and lights. [Control (engineering)]
- Have a traffic management plan showing plant routes, loading areas and pedestrian paths. [Control (procedures)]
- Use a spotter when reversing or working near people. [Control (procedures)]
- Make eye contact with the operator before going near. Stay out of the swing radius. [Control (procedures)]
- Operators hold a CPCS, NPORS or equal card for the plant they use. [Control (procedures)]
- Do a pre-start check on each machine every day and record it. [Control (procedures)]
- Wear hi-vis clothing and a hard hat. [PPE]
- Use low-dust products, such as dust-reduced or pre-mixed compounds. [Reduce / substitute]
- Seal off the work area with plastic sheeting in occupied buildings. [Isolate]
- Use tools with dust extraction and a vacuum for clean up. [Control (engineering)]
- Lightly mist the area with water to keep dust down, away from anything electrical. [Control (engineering)]
- Never dry sweep or blow dust off with compressed air. [Control (procedures)]
- Wear a dust mask and safety glasses. [PPE]
	Medium (5)
	

	3
	Lay rolls, lifting with your legs and swapping tasks
	Lifting and carrying heavy loads
Repetitive work and awkward postures
	Workers
	High (12)
	- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Eliminate]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Reduce / substitute]
- Use trolleys, pallet jacks, hoists, vacuum lifters or plant instead of carrying by hand. [Control (engineering)]
- Use a two-person lift for anything heavy, long or awkward. Plan the route first and clear it. [Control (procedures)]
- Keep the load close, back straight and no twisting. Turn with your feet. [Control (procedures)]
- Rotate tasks and take breaks on long lifting jobs. [Control (procedures)]
- Wear gloves for grip and safety boots to protect your feet. [PPE]
- Use tools that cut the effort: powered screwdrivers, long-handled tools and extension poles for overhead work. [Reduce / substitute]
- Set work up at waist height on benches or trestles where you can. [Control (engineering)]
- Use light tools with good grips, and keep blades and bits sharp. [Control (engineering)]
- Rotate tasks and take short breaks every hour on repetitive work. [Control (procedures)]
- Warm up before heavy physical work and report aches and pains early. [Control (procedures)]
- Wear knee pads for kneeling work and gloves for grip. [PPE]
	Medium (6)
	

	4
	Apply fertiliser with gloves
	Hazardous chemicals
	Workers, Occupants
	Medium (9)
	- Choose the least harmful product that does the job, for example water-based instead of solvent-based. [Reduce / substitute]
- Use chemicals in well-ventilated areas, or use fans and extraction in closed rooms. [Control (engineering)]
- Do a COSHH assessment and read the Safety Data Sheet (SDS) before use. [Control (procedures)]
- Keep chemicals in labelled containers. Never decant into drink bottles. [Control (procedures)]
- Store chemicals away from heat, food and drink, and keep products that react with each other apart. [Control (procedures)]
- Have eye wash and a spill kit nearby, and wash hands before eating. [Control (procedures)]
- Wear chemical-resistant gloves and safety glasses or goggles as listed on the SDS. [PPE]
- Use a respirator with the right cartridge if the SDS calls for one. [PPE]
	Medium (6)
	

	5
	Water in, drink plenty and clean up
	Heat stress
Sun exposure (UV)
Poor housekeeping and waste
	Workers, Visitors
	High (12)
	- Schedule heavy work for the cooler part of the day. [Eliminate]
- Provide shade over work and rest areas, and fans or cooling in roof spaces. [Control (engineering)]
- Supply cool drinking water close by and drink a cup every 15 to 20 minutes. [Control (procedures)]
- Take regular rest breaks in the shade, more often as it gets hotter. [Control (procedures)]
- Let new and returning workers build up to full work in the heat over about a week. [Control (procedures)]
- Plan outdoor work for early morning or late afternoon when UV is lower. [Eliminate]
- Put shade covers over fixed work areas. [Control (engineering)]
- Check the UV index each day. Use sun protection when it is 3 or higher. [Control (procedures)]
- Check your skin regularly and see a doctor about any new or changing spots. [Control (procedures)]
- Wear a broad-brim hat or hard hat brim, long sleeves, sunglasses and SPF 30 or higher sunscreen, reapplied every 2 hours. [PPE]
- Order materials to size and send packaging back where you can. [Eliminate]
- Put skips and waste chutes close to the work. [Control (engineering)]
- Clean as you go, and do a full clean up at the end of each day. [Control (procedures)]
- Keep exits, stairs and walkways clear at all times. [Control (procedures)]
- Stack materials neatly on level ground, away from edges. [Control (procedures)]
- Use a registered waste carrier and keep waste transfer notes for at least 2 years. Keep hazardous waste such as asbestos separate, with consignment notes (special waste in Scotland). [Control (procedures)]
	Medium (8)
	


3. METHOD STATEMENT: SEQUENCE OF WORK
1. Locate irrigation and services before levelling
2. Level and prepare soil with the skid steer
3. Lay rolls, lifting with your legs and swapping tasks
4. Apply fertiliser with gloves
5. Water in, drink plenty and clean up
4. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Safety boots
Rigger gloves
Sun protection (sunscreen and neck cover)
Knee pads
Hi-vis vest
Safety helmet
FFP3 dust mask
Safety glasses
Chemical-resistant gloves
Safety goggles
Half-mask respirator (P3 filters)
Coveralls
	Skid steer loader (CPCS or NPORS skid steer card)
Wacker plate
Hand tools
Trailer
	None required


5. EMERGENCY ARRANGEMENTS
	Emergency number: 999
	

	Nearest A&E
	

	Assembly point
	

	First aider
	

	First aid kit location
	

	Fire extinguisher location
	


6. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Management of Health and Safety at Work Regulations 1999 and the Construction (Design and Management) Regulations 2015.
Keep this RAMS, every revision and the signed briefing register with the site file for the length of the job, and keep a copy in your records afterwards.
7. BRIEFING REGISTER
By signing below, each person confirms they have read and understood this RAMS and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/uk/rams/landscaping/turf-laying/
