RISK ASSESSMENT AND METHOD STATEMENT (RAMS)
Plasterboard patching and repairs · Plastering and dry lining · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company name and number
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client and principal contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by / approved by
	

	Document reference and revision
	

	Review date
	


2. RISK ASSESSMENT
	#
	Activity
	Hazards
	Who might be harmed
	Risk before
	Controls
	Risk after
	Responsible

	1
	Check for asbestos in older linings before cutting
	Disturbing asbestos
	Workers, Occupants, Public
	Very high (15)
	- Before work on any building built before 2000, check the refurbishment and demolition asbestos survey for the work area (HSE HSG264). If there is none, presume asbestos is present or have it sampled before you start. [Eliminate]
- Seal off the work area and keep everyone else out. [Isolate]
- If asbestos must be disturbed, keep it wet, use hand tools not power tools, and clean up with an H-class vacuum. [Control (engineering)]
- Most asbestos insulation, coatings and insulating board need a licensed contractor. Notifiable non-licensed work is notified to HSE before it starts. Other work needs trained workers and controls. [Control (procedures)]
- Stop work straight away if you find suspect asbestos. Do not touch it and tell your supervisor. [Control (procedures)]
- Wear a fit-tested FFP3 mask (or better) and disposable type 5 coveralls. [PPE]
	Medium (5)
	

	2
	Check for cables and pipes behind the wall
	Electric shock from live wiring
	Workers, Occupants
	Very high (15)
	- Isolate the power before any work. Do not work live. [Eliminate]
- Lock out and tag the isolation point with your own personal lock and danger tag. [Isolate]
- Prove dead at the point of work with an approved voltage indicator (GS38), and prove the tester before and after. [Control (engineering)]
- Only competent, qualified electricians do electrical work, following a safe isolation procedure. [Control (procedures)]
- Check for back feeds from solar, batteries and generators that can keep a circuit live after the main switch is off. [Control (procedures)]
- If live work cannot be avoided, use a permit, a safety observer and insulated tools. [Control (procedures)]
- Wear insulated gloves, arc-rated clothing and a face shield when testing or working near live parts. [PPE]
	Medium (5)
	

	3
	Cut out damage and fit a patch
	Cuts from sharp edges
General dust
	Workers, Occupants
	Medium (8)
	- Deburr or cover sharp edges, and fit edge protectors on exposed sheet metal. [Control (engineering)]
- Use knives with retractable or self-retracting blades. [Control (engineering)]
- Cut away from your body and keep your other hand clear. [Control (procedures)]
- Put used blades in a blade bin or sharps container. [Control (procedures)]
- Use two people to handle large sheets of metal or glass. [Control (procedures)]
- Wear cut-resistant gloves and long sleeves. [PPE]
- Use low-dust products, such as dust-reduced or pre-mixed compounds. [Reduce / substitute]
- Seal off the work area with plastic sheeting in occupied buildings. [Isolate]
- Use tools with dust extraction and a vacuum for clean up. [Control (engineering)]
- Lightly mist the area with water to keep dust down, away from anything electrical. [Control (engineering)]
- Never dry sweep or blow dust off with compressed air. [Control (procedures)]
- Wear a dust mask and safety glasses. [PPE]
	Low (4)
	

	4
	Set, sand and finish
	General dust
Falling from a ladder
	Workers, Occupants
	High (12)
	- General dust: see step 3 for the full controls [Control (procedures)]
- Use a podium step, mobile tower or MEWP for longer jobs instead of a straight ladder. [Reduce / substitute]
- Use EN 131 professional ladders in good condition. Remove any damaged ladder from site. [Control (engineering)]
- Set extension ladders at a 4 to 1 angle on firm, level ground, tied or footed, and reaching 1 metre above the landing. [Control (engineering)]
- Use ladders only for short, light work (about 30 minutes in one spot). Do not carry heavy or awkward loads up a ladder. [Control (procedures)]
- Keep three points of contact and your belt buckle between the stiles. Do not overreach. [Control (procedures)]
- Do not work off the top three rungs of a leaning ladder. On a stepladder, do not stand on the top two steps (top three on swing-back or double-sided steps) unless there is a suitable handhold. [Control (procedures)]
- Check the ladder before each use: feet, rungs, stiles and locks. [Control (procedures)]
- Wear non-slip safety boots with clean soles. [PPE]
	Medium (8)
	

	5
	Clean up
	Poor housekeeping and waste
	Workers, Visitors
	Medium (8)
	- Order materials to size and send packaging back where you can. [Eliminate]
- Put skips and waste chutes close to the work. [Control (engineering)]
- Clean as you go, and do a full clean up at the end of each day. [Control (procedures)]
- Keep exits, stairs and walkways clear at all times. [Control (procedures)]
- Stack materials neatly on level ground, away from edges. [Control (procedures)]
- Use a registered waste carrier and keep waste transfer notes for at least 2 years. Keep hazardous waste such as asbestos separate, with consignment notes (special waste in Scotland). [Control (procedures)]
- Wear gloves when handling waste. [PPE]
	Low (4)
	


3. METHOD STATEMENT: SEQUENCE OF WORK
1. Check for asbestos in older linings before cutting
2. Check for cables and pipes behind the wall
3. Cut out damage and fit a patch
4. Set, sand and finish
5. Clean up
4. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	FFP3 dust mask
Safety glasses
Safety boots
Half-mask respirator (P3 filters)
Coveralls
Rigger gloves
Cut-resistant gloves
Safety helmet
	Hand tools
Power sander
Stepladder
	None required


5. EMERGENCY ARRANGEMENTS
	Emergency number: 999
	

	Nearest A&E
	

	Assembly point
	

	First aider
	

	First aid kit location
	

	Fire extinguisher location
	


6. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Management of Health and Safety at Work Regulations 1999 and the Construction (Design and Management) Regulations 2015.
Keep this RAMS, every revision and the signed briefing register with the site file for the length of the job, and keep a copy in your records afterwards.
7. BRIEFING REGISTER
By signing below, each person confirms they have read and understood this RAMS and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/uk/rams/plastering/drywall-patching-repair/
