RISK ASSESSMENT AND METHOD STATEMENT (RAMS)
Drain unblocking and jetting · Plumbing · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company name and number
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client and principal contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by / approved by
	

	Document reference and revision
	

	Review date
	


2. RISK ASSESSMENT
	#
	Activity
	Hazards
	Who might be harmed
	Risk before
	Controls
	Risk after
	Responsible

	1
	Set up cones around open pits and keep the public and pets away
	Public entering the work area
Falling through a floor opening or void
	Public, Children, Workers, Visitors
	Very high (15)
	- Fence off the site with secure temporary fencing and lock the gates when you leave. [Isolate]
- Give pedestrians a safe, marked path around the work, with ramps for prams and wheelchairs. [Isolate]
- Use hoarding, covered walkways or catch fans where work is above public areas. [Control (engineering)]
- Put signs at each entry: site name, contact number and "No unauthorised entry". [Control (procedures)]
- Make the site safe at the end of each day: cover holes, lower plant, remove ladders and lock tools away. [Control (procedures)]
- Use a spotter when moving plant or materials across public paths. [Control (procedures)]
- Cover every hole and penetration with a fixed, secured cover marked "HOLE" or "DANGER". [Isolate]
- Put guardrails with toe boards around stairwells, lift shafts, voids and open edges. [Isolate]
- Install stairs early and fit temporary handrails as soon as they go in. [Control (engineering)]
- Never remove a cover or guardrail without approval. Put it back straight away. [Control (procedures)]
- Inspect covers and barriers daily and after other trades have been through. [Control (procedures)]
- Keep lighting good enough to see openings, especially on lower floors and in the evening. [Control (procedures)]
- Use a harness clipped to a rated anchor when working right next to an open void. [PPE]
	Medium (5)
	

	2
	Open the inspection point, never enter pits or manholes without a confined space permit
	Confined space entry
Lifting and carrying heavy loads
	Workers, Rescuers
	High (12)
	- Do the work from outside the space where you can, using cameras or long-reach tools. [Eliminate]
- Isolate and lock out all pipes, power and moving parts going into the space. [Isolate]
- Test the air for oxygen, flammable and toxic gases before entry, and keep testing during the work. [Control (engineering)]
- Use forced ventilation to keep the air clean. [Control (engineering)]
- Issue a confined space entry permit before anyone goes in. Only trained workers enter. [Control (procedures)]
- Keep a trained standby person outside at all times, in contact with those inside. [Control (procedures)]
- Set up a rescue plan and rescue gear before entry. Never go in to rescue without the right gear. [Control (procedures)]
- Wear a harness for retrieval and the respirator the air test calls for. [PPE]
- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Eliminate]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Reduce / substitute]
- Use trolleys, pallet jacks, hoists, vacuum lifters or plant instead of carrying by hand. [Control (engineering)]
- Use a two-person lift for anything heavy, long or awkward. Plan the route first and clear it. [Control (procedures)]
- Keep the load close, back straight and no twisting. Turn with your feet. [Control (procedures)]
- Rotate tasks and take breaks on long lifting jobs. [Control (procedures)]
- Wear gloves for grip and safety boots to protect your feet. [PPE]
	Medium (6)
	

	3
	Check the jetter hose and fittings, then jet with the nozzle well inside the pipe before starting
	High pressure water jetting
Stored energy
Loud noise
	Workers, People nearby
	High (12)
	- Set an exclusion zone around the jetting area. [Isolate]
- Use a dead man's trigger that stops the jet when released, and check hoses and fittings before use. [Control (engineering)]
- Only trained operators use high pressure jetting gear. [Control (procedures)]
- Never point the lance at anyone or put a hand in front of it. [Control (procedures)]
- Treat any jetting injury as serious and go to hospital, even if it looks small. [Control (procedures)]
- Release or block all stored energy before work: release the pressure in pipes, tanks and hoses, bleed hydraulics, release springs, lower loads. [Eliminate]
- Lock out and tag all energy sources with personal locks. [Isolate]
- Put mechanical blocks or props under raised parts like buckets, tipper bodies and doors. [Control (engineering)]
- Test that the system is dead and nothing can move before you start. [Control (procedures)]
- Follow the maker's procedure, for example for garage door and roller door springs. [Control (procedures)]
- Use quieter tools and methods, such as cut-to-size materials, low-noise machines and battery tools. [Reduce / substitute]
- Keep noisy plant away from work areas, and use screens or distance between the noise and people. [Isolate]
- Keep tools maintained and use mufflers on compressors and generators. [Control (engineering)]
- Limit time on noisy tools and rotate workers. [Control (procedures)]
- If you have to shout to be heard by someone 2 metres away, the noise is probably 85 dB(A) or more: wear hearing protection. [Control (procedures)]
- Assess noise. At 85 dB(A) or more, hearing protection is required and the zone must be marked. [Control (procedures)]
	Medium (6)
	

	4
	Clear the blockage, keeping face and hands away from splashback
	Sewage and wastewater
Eye injuries
Slips and trips
	Workers, People nearby, Visitors, Public
	Medium (9)
	- Flush and drain the line before opening it, and plan the job to avoid contact. [Eliminate]
- Use drain cameras, jetters and long-handled tools to keep hands out. [Control (engineering)]
- Sewage and wastewater: see step 6 for the full controls [Control (procedures)]
- Use tool guards and screens to stop flying particles. [Control (engineering)]
- Use dust extraction and water to keep dust out of the air. [Control (engineering)]
- Keep others out of the area when cutting, grinding or chipping. [Control (procedures)]
- Keep an eye wash station or eye wash bottles on site. [Control (procedures)]
- Wear safety glasses at all times, goggles for dust and chemicals, and a face shield for grinding. [PPE]
- Plan walkways and keep them clear of materials, hoses and leads. [Eliminate]
- Run leads and hoses overhead on hooks or stands, or along walls, not across walkways. [Control (engineering)]
- Fill or cover holes, and lay boards or mats on muddy access paths. [Control (engineering)]
- Clean up offcuts, packaging and spills as you go, not at the end of the day. [Control (procedures)]
- Keep work areas, stairs and access paths well lit. [Control (procedures)]
	Low (4)
	

	5
	Run a CCTV camera to confirm the line is clear
	Sewage and wastewater
	Workers
	Medium (9)
	- Cover cuts with waterproof dressings. Never eat, drink or smoke before washing. [Control (procedures)]
- Wash hands well and clean tools and boots after the job. [Control (procedures)]
- Sewage and wastewater: see step 6 for the full controls [Control (procedures)]
	Low (3)
	

	6
	Close pits, wash down, and wash hands before eating
	Sewage and wastewater
Poor housekeeping and waste
	Workers, Visitors
	Medium (9)
	- Flush and drain the line before opening it, and plan the job to avoid contact. [Eliminate]
- Use drain cameras, jetters and long-handled tools to keep hands out. [Control (engineering)]
- Cover cuts with waterproof dressings. Never eat, drink or smoke before washing. [Control (procedures)]
- Wash hands well and clean tools and boots after the job. [Control (procedures)]
- Keep vaccinations such as tetanus and hepatitis A up to date, on medical advice. [Control (procedures)]
- Wear waterproof gloves, goggles or a face shield, and coveralls. [PPE]
- Order materials to size and send packaging back where you can. [Eliminate]
- Put skips and waste chutes close to the work. [Control (engineering)]
- Clean as you go, and do a full clean up at the end of each day. [Control (procedures)]
- Keep exits, stairs and walkways clear at all times. [Control (procedures)]
- Stack materials neatly on level ground, away from edges. [Control (procedures)]
- Use a registered waste carrier and keep waste transfer notes for at least 2 years. Keep hazardous waste such as asbestos separate, with consignment notes (special waste in Scotland). [Control (procedures)]
- Wear gloves when handling waste. [PPE]
	Low (4)
	


3. METHOD STATEMENT: SEQUENCE OF WORK
1. Set up cones around open pits and keep the public and pets away
2. Open the inspection point, never enter pits or manholes without a confined space permit
3. Check the jetter hose and fittings, then jet with the nozzle well inside the pipe before starting
4. Clear the blockage, keeping face and hands away from splashback
5. Run a CCTV camera to confirm the line is clear
6. Close pits, wash down, and wash hands before eating
4. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Safety boots
Chemical-resistant gloves
Safety goggles
Face shield
Coveralls
Hi-vis vest
Rigger gloves
Ear defenders
Safety glasses
	Drain jetting unit
Hand tools
	Permit to work (electrical isolation)


5. EMERGENCY ARRANGEMENTS
	Emergency number: 999
	

	Nearest A&E
	

	Assembly point
	

	First aider
	

	First aid kit location
	

	Fire extinguisher location
	


6. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Management of Health and Safety at Work Regulations 1999 and the Construction (Design and Management) Regulations 2015.
Keep this RAMS, every revision and the signed briefing register with the site file for the length of the job, and keep a copy in your records afterwards.
7. BRIEFING REGISTER
By signing below, each person confirms they have read and understood this RAMS and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/uk/rams/plumbing/drain-unblocking-jetting/
