RISK ASSESSMENT AND METHOD STATEMENT (RAMS)
Install a toilet, taps or basin · Plumbing · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company name and number
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client and principal contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by / approved by
	

	Document reference and revision
	

	Review date
	


2. RISK ASSESSMENT
	#
	Activity
	Hazards
	Who might be harmed
	Risk before
	Controls
	Risk after
	Responsible

	1
	Isolate water to the fixture and drain the lines
	Stored energy
Slips and trips
	Workers, Visitors, Public
	Medium (8)
	- Release or block all stored energy before work: release the pressure in pipes, tanks and hoses, bleed hydraulics, release springs, lower loads. [Eliminate]
- Lock out and tag all energy sources with personal locks. [Isolate]
- Put mechanical blocks or props under raised parts like buckets, tipper bodies and doors. [Control (engineering)]
- Test that the system is dead and nothing can move before you start. [Control (procedures)]
- Follow the maker's procedure, for example for garage door and roller door springs. [Control (procedures)]
- Wear safety glasses and gloves. [PPE]
- Plan walkways and keep them clear of materials, hoses and leads. [Eliminate]
- Run leads and hoses overhead on hooks or stands, or along walls, not across walkways. [Control (engineering)]
- Slips and trips: see step 5 for the full controls [Control (procedures)]
	Low (4)
	

	2
	Remove the old fixture, wearing gloves for waste contamination
	Sewage and wastewater
Lifting and carrying heavy loads
Cuts from sharp edges
	Workers
	High (12)
	- Flush and drain the line before opening it, and plan the job to avoid contact. [Eliminate]
- Use drain cameras, jetters and long-handled tools to keep hands out. [Control (engineering)]
- Cover cuts with waterproof dressings. Never eat, drink or smoke before washing. [Control (procedures)]
- Wash hands well and clean tools and boots after the job. [Control (procedures)]
- Keep vaccinations such as tetanus and hepatitis A up to date, on medical advice. [Control (procedures)]
- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Eliminate]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Reduce / substitute]
- Use trolleys, pallet jacks, hoists, vacuum lifters or plant instead of carrying by hand. [Control (engineering)]
- Use a two-person lift for anything heavy, long or awkward. Plan the route first and clear it. [Control (procedures)]
- Keep the load close, back straight and no twisting. Turn with your feet. [Control (procedures)]
- Deburr or cover sharp edges, and fit edge protectors on exposed sheet metal. [Control (engineering)]
- Use knives with retractable or self-retracting blades. [Control (engineering)]
- Cut away from your body and keep your other hand clear. [Control (procedures)]
- Put used blades in a blade bin or sharps container. [Control (procedures)]
- Use two people to handle large sheets of metal or glass. [Control (procedures)]
	Medium (6)
	

	3
	Drill fixings into tiles with the right bit and glasses on
	Injury from power tools
Eye injuries
Glass handling and breakage
	Workers, People nearby, Occupants
	High (12)
	- Keep all guards fitted and working. Never tie back or remove a guard. [Control (engineering)]
- Clamp or secure the work piece. Do not hold it by hand. [Control (engineering)]
- Only trained, competent people use power tools, following the maker's instructions. [Control (procedures)]
- Check tools before use. Unplug or remove the battery before changing blades or bits. [Control (procedures)]
- No loose clothing, jewellery or long hair near spinning parts. [Control (procedures)]
- Use tool guards and screens to stop flying particles. [Control (engineering)]
- Use dust extraction and water to keep dust out of the air. [Control (engineering)]
- Keep others out of the area when cutting, grinding or chipping. [Control (procedures)]
- Keep an eye wash station or eye wash bottles on site. [Control (procedures)]
- Wear safety glasses at all times, goggles for dust and chemicals, and a face shield for grinding. [PPE]
- Use suction lifters, glass trolleys or a glazing robot for large panes. [Control (engineering)]
- Store glass upright on racks and secure it. Never lay it flat or lean it loosely. [Control (engineering)]
- Use two or more people for large panes, and clear the carry route first. [Control (procedures)]
- Mark new glass with tape or stickers so nobody walks into it. [Control (procedures)]
- Clean up broken glass straight away into a marked container. [Control (procedures)]
	Medium (8)
	

	4
	Fit and connect the new fixture, kneeling on pads
	Lifting and carrying heavy loads
Repetitive work and awkward postures
	Workers
	High (12)
	- Rotate tasks and take breaks on long lifting jobs. [Control (procedures)]
- Wear gloves for grip and safety boots to protect your feet. [PPE]
- Lifting and carrying heavy loads: see step 2 for the full controls [Control (procedures)]
- Use tools that cut the effort: powered screwdrivers, long-handled tools and extension poles for overhead work. [Reduce / substitute]
- Set work up at waist height on benches or trestles where you can. [Control (engineering)]
- Use light tools with good grips, and keep blades and bits sharp. [Control (engineering)]
- Rotate tasks and take short breaks every hour on repetitive work. [Control (procedures)]
- Warm up before heavy physical work and report aches and pains early. [Control (procedures)]
- Wear knee pads for kneeling work and gloves for grip. [PPE]
	Medium (6)
	

	5
	Turn water on, check for leaks and clean up
	Slips and trips
Poor housekeeping and waste
	Workers, Visitors, Public
	Medium (8)
	- Plan walkways and keep them clear of materials, hoses and leads. [Eliminate]
- Run leads and hoses overhead on hooks or stands, or along walls, not across walkways. [Control (engineering)]
- Fill or cover holes, and lay boards or mats on muddy access paths. [Control (engineering)]
- Clean up offcuts, packaging and spills as you go, not at the end of the day. [Control (procedures)]
- Keep work areas, stairs and access paths well lit. [Control (procedures)]
- Wear safety boots with good grip, laced up. [PPE]
- Order materials to size and send packaging back where you can. [Eliminate]
- Put skips and waste chutes close to the work. [Control (engineering)]
- Clean as you go, and do a full clean up at the end of each day. [Control (procedures)]
- Keep exits, stairs and walkways clear at all times. [Control (procedures)]
- Stack materials neatly on level ground, away from edges. [Control (procedures)]
- Use a registered waste carrier and keep waste transfer notes for at least 2 years. Keep hazardous waste such as asbestos separate, with consignment notes (special waste in Scotland). [Control (procedures)]
- Wear gloves when handling waste. [PPE]
	Low (4)
	


3. METHOD STATEMENT: SEQUENCE OF WORK
1. Isolate water to the fixture and drain the lines
2. Remove the old fixture, wearing gloves for waste contamination
3. Drill fixings into tiles with the right bit and glasses on
4. Fit and connect the new fixture, kneeling on pads
5. Turn water on, check for leaks and clean up
4. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Safety boots
Rigger gloves
Safety glasses
Knee pads
Chemical-resistant gloves
Safety goggles
Face shield
Coveralls
Cut-resistant gloves
Ear defenders
	Hand tools
Power drill
	Permit to work (electrical isolation)


5. EMERGENCY ARRANGEMENTS
	Emergency number: 999
	

	Nearest A&E
	

	Assembly point
	

	First aider
	

	First aid kit location
	

	Fire extinguisher location
	


6. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Management of Health and Safety at Work Regulations 1999 and the Construction (Design and Management) Regulations 2015.
Keep this RAMS, every revision and the signed briefing register with the site file for the length of the job, and keep a copy in your records afterwards.
7. BRIEFING REGISTER
By signing below, each person confirms they have read and understood this RAMS and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/uk/rams/plumbing/toilet-tap-installation/
