RISK ASSESSMENT AND METHOD STATEMENT (RAMS)
Mobile scaffold tower set up and use · Scaffolding · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company name and number
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client and principal contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by / approved by
	

	Document reference and revision
	

	Review date
	


2. RISK ASSESSMENT
	#
	Activity
	Hazards
	Who might be harmed
	Risk before
	Controls
	Risk after
	Responsible

	1
	Check all parts and the ground, and look up for power lines
	Contact with overhead power lines
Scaffold collapse or fall from scaffold
	Workers, Plant operators, Public, People below
	Very high (15)
	- Ask the distribution network operator (DNO) to turn off, move or insulate the lines before work starts. [Eliminate]
- Use non-conductive (fibreglass) ladders near any power lines. [Reduce / substitute]
- Mark the safe distance with flags, tape or goal posts and keep all plant and people outside it. [Isolate]
- Follow HSE GS6: barriers, goal posts under the lines and a permit for work near them. [Control (procedures)]
- Use a dedicated spotter whenever plant moves or raises anything near lines. [Control (procedures)]
- Treat all lines as live. If plant touches a line, stay in the cab and keep everyone well away. [Control (procedures)]
- Scaffold is built, altered and taken down only by CISRS-carded scaffolders, to TG20 or a specific design. [Control (engineering)]
- Fit guardrails, mid rails and toe boards on every working platform. [Control (engineering)]
- Scaffold collapse or fall from scaffold: see step 4 for the full controls [Control (procedures)]
	Medium (5)
	

	2
	Build to the instructions with outriggers and guardrails
	Scaffold collapse or fall from scaffold
Falling from height
	Workers, Public, People below
	Very high (20)
	- Use mobile scaffolds only on firm, level ground with castors locked and outriggers fitted. Never move one with anyone on it. [Control (engineering)]
- Mobile towers are built by PASMA-trained workers. [Control (procedures)]
- Scaffold collapse or fall from scaffold: see step 4 for the full controls [Control (procedures)]
- Do the work from the ground where you can, for example pre-assemble on the ground or use extension poles. [Eliminate]
- Install guardrails or edge protection on all open edges before work starts. [Isolate]
- Use a scaffold, mobile tower or MEWP instead of working off a ladder. [Control (engineering)]
- Where edge protection is not practical, use a fall restraint or fall arrest system on a rated anchor point. [Control (engineering)]
- Have a rescue plan so a worker hanging in a harness can be brought down within minutes. [Control (procedures)]
- Wear a full body harness with a shock-absorbing lanyard, clipped on at all times when using fall arrest. [PPE]
	Medium (5)
	

	3
	Lock the wheels before climbing, climb only on the inside
	Scaffold collapse or fall from scaffold
Falling from height
	Workers, Public, People below
	Very high (20)
	- Inspect the scaffold before first use, after any change or bad weather, and at least every 7 days. Record it on the tag and register. [Control (procedures)]
- Do not overload platforms. Know the duty rating and keep material stacks over the standards. [Control (procedures)]
- Scaffold collapse or fall from scaffold: see step 4 for the full controls [Control (procedures)]
- Falling from height: see step 2 for the full controls [Control (procedures)]
	Medium (5)
	

	4
	Never move it with anyone or anything on it
	Scaffold collapse or fall from scaffold
Falling tools and materials
	Workers, Public, People below
	Very high (15)
	- Scaffold is built, altered and taken down only by CISRS-carded scaffolders, to TG20 or a specific design. [Control (engineering)]
- Fit guardrails, mid rails and toe boards on every working platform. [Control (engineering)]
- Use mobile scaffolds only on firm, level ground with castors locked and outriggers fitted. Never move one with anyone on it. [Control (engineering)]
- Mobile towers are built by PASMA-trained workers. [Control (procedures)]
- Inspect the scaffold before first use, after any change or bad weather, and at least every 7 days. Record it on the tag and register. [Control (procedures)]
- Do not overload platforms. Know the duty rating and keep material stacks over the standards. [Control (procedures)]
- Never remove ties, braces, guardrails or boards. Only the scaffolder alters the scaffold. [Control (procedures)]
- Wear a hard hat and safety boots on and around the scaffold. [PPE]
- Barricade and sign the drop zone under overhead work so nobody walks beneath. [Isolate]
- Fit toe boards, kick plates and mesh screens on scaffolds and edges. [Control (engineering)]
- Use catch fans, debris netting or covered walkways where people pass below. [Control (engineering)]
- Tether hand tools when working at height. [Control (engineering)]
- Keep platforms tidy. Do not stack materials near edges or above toe board height. [Control (procedures)]
- Lower materials with a hoist, chute or rope. Never throw or drop anything down. [Control (procedures)]
- Wear a hard hat anywhere objects could fall. [PPE]
	Medium (8)
	

	5
	Dismantle in reverse order and store parts
	Lifting and carrying heavy loads
	Workers
	High (12)
	- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Eliminate]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Reduce / substitute]
- Use trolleys, pallet jacks, hoists, vacuum lifters or plant instead of carrying by hand. [Control (engineering)]
- Use a two-person lift for anything heavy, long or awkward. Plan the route first and clear it. [Control (procedures)]
- Keep the load close, back straight and no twisting. Turn with your feet. [Control (procedures)]
- Rotate tasks and take breaks on long lifting jobs. [Control (procedures)]
- Wear gloves for grip and safety boots to protect your feet. [PPE]
	Medium (6)
	


3. METHOD STATEMENT: SEQUENCE OF WORK
1. Check all parts and the ground, and look up for power lines
2. Build to the instructions with outriggers and guardrails
3. Lock the wheels before climbing, climb only on the inside
4. Never move it with anyone or anything on it
5. Dismantle in reverse order and store parts
4. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Safety boots
Safety helmet
Rigger gloves
Hi-vis vest
Safety glasses
	Mobile access tower (PASMA certificate)
Hand tools
	Work at height permit


5. EMERGENCY ARRANGEMENTS
	Emergency number: 999
	

	Nearest A&E
	

	Assembly point
	

	First aider
	

	First aid kit location
	

	Fire extinguisher location
	


6. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Management of Health and Safety at Work Regulations 1999 and the Construction (Design and Management) Regulations 2015.
Keep this RAMS, every revision and the signed briefing register with the site file for the length of the job, and keep a copy in your records afterwards.
7. BRIEFING REGISTER
By signing below, each person confirms they have read and understood this RAMS and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/uk/rams/scaffolding/mobile-tower-erection/
