RISK ASSESSMENT AND METHOD STATEMENT (RAMS)
Install roof edge protection · Scaffolding · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company name and number
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client and principal contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by / approved by
	

	Document reference and revision
	

	Review date
	


2. RISK ASSESSMENT
	#
	Activity
	Hazards
	Who might be harmed
	Risk before
	Controls
	Risk after
	Responsible

	1
	Plan the system to suit the roof pitch and gutter height
	Falling from a roof edge
	Workers, People below
	Very high (20)
	- Do what you can from the ground or from a scaffold at the gutter line, for example pre-assemble parts on the ground. [Eliminate]
- Install edge protection or guardrails on all open roof edges before work starts. [Isolate]
- Falling from a roof edge: see step 2 for the full controls [Control (procedures)]
	Medium (5)
	

	2
	Install from a MEWP or scaffold, or harnessed to an anchor
	Falling from a roof edge
MEWP tip-over or crush
Falling from height
	Workers, People below, People nearby
	Very high (20)
	- Do what you can from the ground or from a scaffold at the gutter line, for example pre-assemble parts on the ground. [Eliminate]
- Install edge protection or guardrails on all open roof edges before work starts. [Isolate]
- Use a perimeter scaffold with handrails and toe boards along the eaves where practical. [Control (engineering)]
- Where guardrails cannot be fitted, use fall restraint on certified roof anchors so workers cannot reach the edge. [Control (engineering)]
- Use one safe, controlled access point and keep others off the roof. [Control (procedures)]
- Check the ground before setting up. Use outriggers and spreader pads, and keep clear of trenches, pits and slopes. [Control (engineering)]
- Use a platform with tilt alarm and secondary guarding (anti-entrapment) where there is an overhead crush risk. [Control (engineering)]
- Use IPAF-trained operators for MEWPs, carrying their PAL card. [Control (procedures)]
- Do a pre-start check each day. Keep a trained person on the ground who can lower the platform in an emergency. [Control (procedures)]
- Never exceed the safe working load, climb on the rails or use a ladder in the basket. [Control (procedures)]
- In boom-type platforms, wear a harness clipped to the basket anchor point. [PPE]
- Do the work from the ground where you can, for example pre-assemble on the ground or use extension poles. [Eliminate]
- Install guardrails or edge protection on all open edges before work starts. [Isolate]
- Use a scaffold, mobile tower or MEWP instead of working off a ladder. [Control (engineering)]
- Where edge protection is not practical, use a fall restraint or fall arrest system on a rated anchor point. [Control (engineering)]
- Have a rescue plan so a worker hanging in a harness can be brought down within minutes. [Control (procedures)]
	Medium (5)
	

	3
	Fix brackets into sound structure
	Structural collapse during alterations
Injury from power tools
	Workers, Occupants, People nearby
	High (10)
	- Get an engineer to check before removing any wall, beam, post or bracing that may be load-bearing. [Eliminate]
- Keep everyone clear of the area under and next to the work. [Isolate]
- Install temporary props, needles or shoring as designed before removing any support. [Control (engineering)]
- Follow the engineer's sequence. Do not change it without approval. [Control (procedures)]
- Check props daily. Do not remove them until the permanent support is in and approved. [Control (procedures)]
- Wear a hard hat and safety boots. [PPE]
- Keep all guards fitted and working. Never tie back or remove a guard. [Control (engineering)]
- Clamp or secure the work piece. Do not hold it by hand. [Control (engineering)]
- Only trained, competent people use power tools, following the maker's instructions. [Control (procedures)]
- Check tools before use. Unplug or remove the battery before changing blades or bits. [Control (procedures)]
- No loose clothing, jewellery or long hair near spinning parts. [Control (procedures)]
- Wear safety glasses and hearing protection. Do not wear loose gloves on drills or other rotating tools. [PPE]
	Medium (6)
	

	4
	Fit rails and mesh, keeping tools tethered
	Falling tools and materials
Lifting and carrying heavy loads
	Workers, Public, People below
	High (12)
	- Barricade and sign the drop zone under overhead work so nobody walks beneath. [Isolate]
- Fit toe boards, kick plates and mesh screens on scaffolds and edges. [Control (engineering)]
- Use catch fans, debris netting or covered walkways where people pass below. [Control (engineering)]
- Tether hand tools when working at height. [Control (engineering)]
- Keep platforms tidy. Do not stack materials near edges or above toe board height. [Control (procedures)]
- Lower materials with a hoist, chute or rope. Never throw or drop anything down. [Control (procedures)]
- Wear a hard hat anywhere objects could fall. [PPE]
- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Eliminate]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Reduce / substitute]
- Use trolleys, pallet jacks, hoists, vacuum lifters or plant instead of carrying by hand. [Control (engineering)]
- Use a two-person lift for anything heavy, long or awkward. Plan the route first and clear it. [Control (procedures)]
- Keep the load close, back straight and no twisting. Turn with your feet. [Control (procedures)]
- Rotate tasks and take breaks on long lifting jobs. [Control (procedures)]
- Wear gloves for grip and safety boots to protect your feet. [PPE]
	Medium (8)
	

	5
	Inspect and hand over before roof work starts
	Falling from a roof edge
	Workers, People below
	Very high (20)
	- Stop roof work in strong wind or rain, and when the roof is wet, icy or covered in dust or frost. [Control (procedures)]
- Wear a harness clipped to a rated anchor when using restraint or fall arrest, and soft-soled non-slip boots. [PPE]
- Falling from a roof edge: see step 2 for the full controls [Control (procedures)]
	Medium (5)
	


3. METHOD STATEMENT: SEQUENCE OF WORK
1. Plan the system to suit the roof pitch and gutter height
2. Install from a MEWP or scaffold, or harnessed to an anchor
3. Fix brackets into sound structure
4. Fit rails and mesh, keeping tools tethered
5. Inspect and hand over before roof work starts
4. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Safety boots
Full body harness and lanyard
Safety helmet
Rigger gloves
Sun protection (sunscreen and neck cover)
Hi-vis vest
Safety glasses
Ear defenders
	Tube and fitting or system scaffold (CISRS scaffolder card to erect, alter or dismantle)
Boom MEWP (IPAF PAL card (3b))
Hand tools
Power drill
	Roof access permit
Work at height permit


5. EMERGENCY ARRANGEMENTS
	Emergency number: 999
	

	Nearest A&E
	

	Assembly point
	

	First aider
	

	First aid kit location
	

	Fire extinguisher location
	


6. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Management of Health and Safety at Work Regulations 1999 and the Construction (Design and Management) Regulations 2015.
Keep this RAMS, every revision and the signed briefing register with the site file for the length of the job, and keep a copy in your records afterwards.
7. BRIEFING REGISTER
By signing below, each person confirms they have read and understood this RAMS and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/uk/rams/scaffolding/roof-edge-protection-install/
