RISK ASSESSMENT AND METHOD STATEMENT (RAMS)
Wet area waterproofing · Tiling · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company name and number
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client and principal contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by / approved by
	

	Document reference and revision
	

	Review date
	


2. RISK ASSESSMENT
	#
	Activity
	Hazards
	Who might be harmed
	Risk before
	Controls
	Risk after
	Responsible

	1
	Check the substrate is sheeted, clean, dry and cured, and keep occupants out of the room
	Working in an occupied home or building
Slips and trips
	Residents, Children, Staff, Workers, Visitors, Public
	Medium (9)
	- Plan noisy, dusty or risky work for when the building is empty. [Eliminate]
- Close off the work area with barriers, plastic sheeting or locked doors, and put up signs. [Isolate]
- Keep fire exits and paths clear at all times. [Control (procedures)]
- Tell occupants before you turn off power, water or gas, and before noisy or dusty work. [Control (procedures)]
- Lock away tools, chemicals and materials each day, out of reach of children. [Control (procedures)]
- Clean up dust and debris at the end of each day. [Control (procedures)]
- Plan walkways and keep them clear of materials, hoses and leads. [Eliminate]
- Run leads and hoses overhead on hooks or stands, or along walls, not across walkways. [Control (engineering)]
- Fill or cover holes, and lay boards or mats on muddy access paths. [Control (engineering)]
- Clean up offcuts, packaging and spills as you go, not at the end of the day. [Control (procedures)]
- Keep work areas, stairs and access paths well lit. [Control (procedures)]
- Wear safety boots with good grip, laced up. [PPE]
	Low (4)
	

	2
	Read the safety data sheets and set up fans or open windows, as solvent membranes give off fumes
	Hazardous chemicals
	Workers, Occupants
	Medium (9)
	- Choose the least harmful product that does the job, for example water-based instead of solvent-based. [Reduce / substitute]
- Use chemicals in well-ventilated areas, or use fans and extraction in closed rooms. [Control (engineering)]
- Hazardous chemicals: see step 7 for the full controls [Control (procedures)]
	Medium (6)
	

	3
	Have a qualified electrician isolate or make safe sockets and lights in the room if they will get wet, and run tools through RCD protection
	Electric shock from leads and power tools
	Workers
	High (12)
	- Use battery-powered tools where you can. [Reduce / substitute]
- Use 110V tools through a centre-tapped transformer, or battery tools. Use an RCD on any 230V supply. [Control (engineering)]
- Keep leads off the ground and out of water, using lead stands or hooks. [Control (engineering)]
- Check leads, plugs and tools before every use. Tag out and remove anything damaged. [Control (procedures)]
- Keep tools and leads inspected and PAT tested on a regular schedule. [Control (procedures)]
- Do not use tools in rain or wet areas unless they are rated for it. [Control (procedures)]
- Wear safety boots and dry gloves. [PPE]
	Low (4)
	

	4
	Prepare the surface, grinding with extraction
	Silica dust from concrete, brick, stone and tiles
General dust
Loud noise
	Workers, People nearby, Occupants
	Very high (20)
	- Order materials cut to size, or use low-dust methods such as score and snap or a block splitter. [Reduce / substitute]
- Cut outdoors or in a separate area, with other people well away and upwind. [Isolate]
- Use water on the blade or on-tool dust extraction connected to an H-class vacuum. [Control (engineering)]
- Clean up with a vacuum or wet methods. Never dry sweep or use compressed air. [Control (procedures)]
- Do a COSHH assessment and keep exposure below the workplace exposure limit (0.1 mg/m3 respirable crystalline silica, 8 hours). [Control (procedures)]
- Workers regularly exposed to silica dust get health surveillance (COSHH reg 11, HSE G404). [Control (procedures)]
- Wear a fit-tested FFP3 mask. [PPE]
- Use low-dust products, such as dust-reduced or pre-mixed compounds. [Reduce / substitute]
- Seal off the work area with plastic sheeting in occupied buildings. [Isolate]
- Use tools with dust extraction and a vacuum for clean up. [Control (engineering)]
- Lightly mist the area with water to keep dust down, away from anything electrical. [Control (engineering)]
- Never dry sweep or blow dust off with compressed air. [Control (procedures)]
- Use quieter tools and methods, such as cut-to-size materials, low-noise machines and battery tools. [Reduce / substitute]
- Keep noisy plant away from work areas, and use screens or distance between the noise and people. [Isolate]
- Keep tools maintained and use mufflers on compressors and generators. [Control (engineering)]
- Limit time on noisy tools and rotate workers. [Control (procedures)]
- If you have to shout to be heard by someone 2 metres away, the noise is probably 85 dB(A) or more: wear hearing protection. [Control (procedures)]
- Assess noise. At 85 dB(A) or more, hearing protection is required and the zone must be marked. [Control (procedures)]
	Medium (6)
	

	5
	Fit bond breakers, puddle flanges and angles
	Hazardous chemicals
Cuts from sharp edges
	Workers, Occupants
	Medium (9)
	- Do a COSHH assessment and read the Safety Data Sheet (SDS) before use. [Control (procedures)]
- Keep chemicals in labelled containers. Never decant into drink bottles. [Control (procedures)]
- Hazardous chemicals: see step 7 for the full controls [Control (procedures)]
- Deburr or cover sharp edges, and fit edge protectors on exposed sheet metal. [Control (engineering)]
- Use knives with retractable or self-retracting blades. [Control (engineering)]
- Cut away from your body and keep your other hand clear. [Control (procedures)]
- Put used blades in a blade bin or sharps container. [Control (procedures)]
- Use two people to handle large sheets of metal or glass. [Control (procedures)]
- Wear cut-resistant gloves and long sleeves. [PPE]
	Medium (6)
	

	6
	Prime the surface, keeping all ignition sources away until it is dry
	Flammable liquids and gases
Hazardous chemicals
Fire and emergencies
	Workers, Occupants, Public, Visitors
	High (10)
	- Use non-flammable or water-based products where you can. [Reduce / substitute]
- Keep ignition sources away: no smoking, no hot work and no running engines near flammables. [Isolate]
- Store fuels and solvents in approved, closed containers in a ventilated area away from the work. [Control (engineering)]
- Refuel equipment outdoors with the engine off and cool. [Control (procedures)]
- Keep only what you need for the day on site. [Control (procedures)]
- Store chemicals away from heat, food and drink, and keep products that react with each other apart. [Control (procedures)]
- Have eye wash and a spill kit nearby, and wash hands before eating. [Control (procedures)]
- Hazardous chemicals: see step 7 for the full controls [Control (procedures)]
- Provide fire extinguishers suited to the site, checked and easy to reach. [Control (engineering)]
- Keep exits and escape routes clear and signed. [Control (engineering)]
- Have a site emergency plan: alarm, exits, assembly point and emergency contacts. [Control (procedures)]
- Keep a stocked first aid kit and at least one trained first aider on site. [Control (procedures)]
- Know the site address and how emergency services get in. Call 999. [Control (procedures)]
	Medium (6)
	

	7
	Apply the membrane in coats with nitrile gloves and the respirator the SDS lists (an organic vapour cartridge for solvent or polyurethane products), kneeling on pads
	Hazardous chemicals
Repetitive work and awkward postures
	Workers, Occupants
	Medium (9)
	- Choose the least harmful product that does the job, for example water-based instead of solvent-based. [Reduce / substitute]
- Use chemicals in well-ventilated areas, or use fans and extraction in closed rooms. [Control (engineering)]
- Do a COSHH assessment and read the Safety Data Sheet (SDS) before use. [Control (procedures)]
- Keep chemicals in labelled containers. Never decant into drink bottles. [Control (procedures)]
- Store chemicals away from heat, food and drink, and keep products that react with each other apart. [Control (procedures)]
- Have eye wash and a spill kit nearby, and wash hands before eating. [Control (procedures)]
- Wear chemical-resistant gloves and safety glasses or goggles as listed on the SDS. [PPE]
- Use a respirator with the right cartridge if the SDS calls for one. [PPE]
- Use tools that cut the effort: powered screwdrivers, long-handled tools and extension poles for overhead work. [Reduce / substitute]
- Set work up at waist height on benches or trestles where you can. [Control (engineering)]
- Use light tools with good grips, and keep blades and bits sharp. [Control (engineering)]
- Rotate tasks and take short breaks every hour on repetitive work. [Control (procedures)]
- Warm up before heavy physical work and report aches and pains early. [Control (procedures)]
- Wear knee pads for kneeling work and gloves for grip. [PPE]
	Medium (6)
	

	8
	Let it cure, then flood test
	Slips and trips
	Workers, Visitors, Public
	Medium (8)
	- Slips and trips: see step 1 for the full controls [Control (procedures)]
	Low (4)
	

	9
	Clean tools and dispose of waste membrane and tins properly
	Hazardous chemicals
Poor housekeeping and waste
	Workers, Occupants, Visitors
	Medium (9)
	- Hazardous chemicals: see step 7 for the full controls [Control (procedures)]
- Order materials to size and send packaging back where you can. [Eliminate]
- Put skips and waste chutes close to the work. [Control (engineering)]
- Clean as you go, and do a full clean up at the end of each day. [Control (procedures)]
- Keep exits, stairs and walkways clear at all times. [Control (procedures)]
- Stack materials neatly on level ground, away from edges. [Control (procedures)]
- Use a registered waste carrier and keep waste transfer notes for at least 2 years. Keep hazardous waste such as asbestos separate, with consignment notes (special waste in Scotland). [Control (procedures)]
- Wear gloves when handling waste. [PPE]
	Medium (6)
	


3. METHOD STATEMENT: SEQUENCE OF WORK
1. Check the substrate is sheeted, clean, dry and cured, and keep occupants out of the room
2. Read the safety data sheets and set up fans or open windows, as solvent membranes give off fumes
3. Have a qualified electrician isolate or make safe sockets and lights in the room if they will get wet, and run tools through RCD protection
4. Prepare the surface, grinding with extraction
5. Fit bond breakers, puddle flanges and angles
6. Prime the surface, keeping all ignition sources away until it is dry
7. Apply the membrane in coats with nitrile gloves and the respirator the SDS lists (an organic vapour cartridge for solvent or polyurethane products), kneeling on pads
8. Let it cure, then flood test
9. Clean tools and dispose of waste membrane and tins properly
4. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Chemical-resistant gloves
Safety glasses
Half-mask respirator (P3 filters)
Knee pads
FFP3 dust mask
Safety boots
Safety goggles
Coveralls
Rigger gloves
Ear defenders
Cut-resistant gloves
	Hand tools
Angle grinder (disc cutter)
H-class dust extractor
	None required


5. EMERGENCY ARRANGEMENTS
	Emergency number: 999
	

	Nearest A&E
	

	Assembly point
	

	First aider
	

	First aid kit location
	

	Fire extinguisher location
	


6. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Management of Health and Safety at Work Regulations 1999 and the Construction (Design and Management) Regulations 2015.
Keep this RAMS, every revision and the signed briefing register with the site file for the length of the job, and keep a copy in your records afterwards.
7. BRIEFING REGISTER
By signing below, each person confirms they have read and understood this RAMS and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/uk/rams/tiling/waterproofing/
