JOB HAZARD ANALYSIS (JHA)
Bonded (non-friable) asbestos removal · Demolition · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client / general contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by
	

	Document number and revision
	

	Competent person
	

	Review date
	


2. JOB STEPS, HAZARDS AND CONTROLS
	#
	Job step
	Hazards
	Risk before
	Controls
	Risk after
	Responsible

	1
	Confirm the licence needed, notify the regulator if required, and tell neighbours
	Disturbing asbestos
Public entering the work area
	Critical
	- Treat insulation, surfacing and resilient flooring in buildings built before 1981 as asbestos unless testing shows otherwise, and get the owner's asbestos survey before you start. [Elimination]
- Seal off the work area and keep everyone else out. [Engineering (guarding)]
- Disturbing asbestos: see step 6 for the full controls [Administrative]
- Fence off the site with secure temporary fencing and lock the gates when you leave. [Engineering (guarding)]
- Give pedestrians a safe, marked path around the work, with ramps for strollers and wheelchairs. [Engineering (guarding)]
- Public entering the work area: see step 2 for the full controls [Administrative]
	Medium
	

	2
	Set up the work area with barriers, signs and plastic sheeting, and close nearby windows
	Disturbing asbestos
Public entering the work area
	Critical
	- If asbestos must be disturbed, keep it wet, use hand tools not power tools, and clean up with a HEPA vacuum. [Engineering]
- Follow 29 CFR 1926.1101: competent person, work class, regulated area and exposure monitoring. [Administrative]
- Disturbing asbestos: see step 6 for the full controls [Administrative]
- Fence off the site with secure temporary fencing and lock the gates when you leave. [Engineering (guarding)]
- Give pedestrians a safe, marked path around the work, with ramps for strollers and wheelchairs. [Engineering (guarding)]
- Use hoarding, covered walkways or catch fans where work is above public areas. [Engineering]
- Put signs at each entry: site name, contact number and "No unauthorized entry". [Administrative]
- Make the site safe at the end of each day: cover holes, lower plant, remove ladders and lock tools away. [Administrative]
- Use a spotter when moving plant or materials across public paths. [Administrative]
	Medium
	

	3
	Set up a decontamination point and put on disposable coveralls and a fitted respirator
	Disturbing asbestos
	Critical
	- Commercial renovation and any demolition need a NESHAP asbestos inspection first, and demolition needs written notice to the state or EPA 10 working days before work starts (40 CFR 61 Subpart M). [Administrative]
- Roofing felts, cement shingles and siding, roof coatings and old panel backboards can also contain asbestos. Test them or treat them as asbestos; asbestos roofing is removed intact with hand tools by trained workers (29 CFR 1926.1101(g)(8)). [Administrative]
- Disturbing asbestos: see step 6 for the full controls [Administrative]
	Medium
	

	4
	Have a licensed electrician isolate and disconnect power to anything fixed to the sheets, and check where the service line is attached
	Electric shock from live wiring
	Critical
	- Isolate the power before any work. Do not work live. [Elimination]
- Lock out and tag the disconnecting means with your own personal lock and tag so the circuit cannot be energized (29 CFR 1926.417). [Engineering (guarding)]
- Test before you touch: prove dead at the point of work with a tested voltage tester. [Engineering]
- Only qualified persons work on or near exposed energized parts. [Administrative]
- Check for back feeds from solar, batteries and generators that can keep a circuit live after the main switch is off. [Administrative]
- If energized work cannot be avoided, use an energized work permit, a safety observer and insulated tools, following NFPA 70E. [Administrative]
- Wear insulated gloves, arc-rated clothing and a face shield when testing or working near live parts. [PPE]
	Medium
	

	5
	Use fall protection when removing from roofs, as sheets are fragile
	Falling through a fragile roof or skylight
Falling from a roof edge
	Critical
	- Work from underneath or from an aerial lift so nobody stands on the fragile roof. [Elimination]
- Cover every skylight with a fixed, marked cover that can hold at least twice the weight it may carry, or guard it with a guardrail. [Engineering (guarding)]
- Use crawl boards or staging to spread the load on fragile or rotten decking, and cover or guard any hole left where decking is removed (29 CFR 1926.501(b)(4)). [Engineering]
- Use fall arrest on rated anchors when working near fragile areas. [Engineering]
- Treat all roof sheets as fragile until a competent person confirms they are not. Old fiber cement and plastic sheets are fragile. [Administrative]
- Put "Fragile roof" signs at every roof access point. [Administrative]
- Never walk on sheets between purlins or along skylights. Stay on boards or staging. [Administrative]
- Wear a full body harness clipped to a rated anchor. [PPE]
- Do what you can from the ground or from a scaffold at the gutter line, for example pre-assemble parts on the ground. [Elimination]
- Install edge protection or guardrails on all open roof edges before work starts. [Engineering (guarding)]
- Use a perimeter scaffold with handrails and toe boards along the eaves where practical. [Engineering]
- Where guardrails cannot be fitted, use fall restraint on certified roof anchors so workers cannot reach the edge. [Engineering]
- Low-slope roofs: guardrails, safety nets, personal fall arrest, or a warning line combined with one of these or with a safety monitor (a safety monitor alone only on roofs 50 feet wide or less). Steep roofs: guardrails with toe boards, safety nets or personal fall arrest (29 CFR 1926.501(b)(10), (11)). [Administrative]
- Use one safe, controlled access point and keep others off the roof. [Administrative]
- Stop roof work in strong wind or rain, and when the roof is wet, icy or covered in dust or frost. [Administrative]
- Wear a harness clipped to a rated anchor when using restraint or fall arrest, and soft-soled non-slip boots. [PPE]
	Medium
	

	6
	Wet the sheets and undo fixings by hand, removing sheets whole with no power tools or breaking
	Disturbing asbestos
Lifting and carrying heavy loads
Heat stress
	Critical
	- Treat insulation, surfacing and resilient flooring in buildings built before 1981 as asbestos unless testing shows otherwise, and get the owner's asbestos survey before you start. [Elimination]
- Seal off the work area and keep everyone else out. [Engineering (guarding)]
- If asbestos must be disturbed, keep it wet, use hand tools not power tools, and clean up with a HEPA vacuum. [Engineering]
- Follow 29 CFR 1926.1101: competent person, work class, regulated area and exposure monitoring. [Administrative]
- Commercial renovation and any demolition need a NESHAP asbestos inspection first, and demolition needs written notice to the state or EPA 10 working days before work starts (40 CFR 61 Subpart M). [Administrative]
- Roofing felts, cement shingles and siding, roof coatings and old panel backboards can also contain asbestos. Test them or treat them as asbestos; asbestos roofing is removed intact with hand tools by trained workers (29 CFR 1926.1101(g)(8)). [Administrative]
- Stop work straight away if you find suspect asbestos. Do not touch it and tell your supervisor. [Administrative]
- Wear a fit-tested NIOSH-approved respirator suited to the work class, and disposable coveralls. [PPE]
- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Elimination]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Substitution]
- Use trolleys, pallet jacks, hoists, vacuum lifters or plant instead of carrying by hand. [Engineering]
- Use a two-person lift for anything heavy, long or awkward. Plan the route first and clear it. [Administrative]
- Keep the load close, back straight and no twisting. Turn with your feet. [Administrative]
- Schedule heavy work for the cooler part of the day. [Elimination]
- Provide shade over work and rest areas, and fans or cooling in attics. [Engineering]
- Supply cool drinking water close by and drink a cup every 15 to 20 minutes. [Administrative]
- Take regular rest breaks in the shade, more often as it gets hotter. [Administrative]
- Let new and returning workers build up to full work in the heat over about a week. [Administrative]
- In California, Washington, Oregon and Maryland, follow the state heat illness rule: written plan, shade, water, rest and high-heat procedures. [Administrative]
	Medium
	

	7
	Lower sheets carefully; never drop or slide them
	Disturbing asbestos
Falling tools and materials
Lifting and carrying heavy loads
	Critical
	- Disturbing asbestos: see step 6 for the full controls [Administrative]
- Barricade and sign the drop zone under overhead work so nobody walks beneath. [Engineering (guarding)]
- Fit toe boards, kick plates and mesh screens on scaffolds and edges. [Engineering]
- Use catch fans, debris netting or covered walkways where people pass below. [Engineering]
- Tether hand tools when working at height. [Engineering]
- Keep platforms tidy. Do not stack materials near edges or above toe board height. [Administrative]
- Rotate tasks and take breaks on long lifting jobs. [Administrative]
- Wear gloves for grip and safety boots to protect your feet. [PPE]
- Lifting and carrying heavy loads: see step 6 for the full controls [Administrative]
	Medium
	

	8
	Wrap sheets in heavy plastic, label as asbestos waste and take to an approved disposal site
	Disturbing asbestos
Poor housekeeping and waste
	Critical
	- Disturbing asbestos: see step 6 for the full controls [Administrative]
- Order materials to size and send packaging back where you can. [Elimination]
- Put dumpsters and waste chutes close to the work. [Engineering]
- Clean as you go, and do a full clean up at the end of each day. [Administrative]
- Keep exits, stairs and walkways clear at all times. [Administrative]
- Stack materials neatly on level ground, away from edges. [Administrative]
- Wear gloves when handling waste. [PPE]
	Medium
	

	9
	Clean up with an H-class vacuum and wet wipes, then decontaminate
	Disturbing asbestos
	Critical
	- Disturbing asbestos: see step 6 for the full controls [Administrative]
	Medium
	

	10
	Get a clearance inspection before others enter
	Disturbing asbestos
	Critical
	- Disturbing asbestos: see step 6 for the full controls [Administrative]
	Medium
	


3. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Half-face respirator (P100 cartridges)
Coveralls
Chemical-resistant gloves
Safety-toe boots (ASTM F2413)
Safety glasses (ANSI Z87.1)
Work gloves
High-visibility safety apparel, ANSI/ISEA 107 Class 2 or 3 (Type R near roadways)
Personal fall arrest system (harness)
Hard hat (ANSI Z89.1)
Sun protection (sunscreen, hat, long sleeves)
	Hand tools
HEPA vacuum
Extension ladder
Trailer
	Asbestos abatement permit / NESHAP notice (10 working days before demolition)
Written fall protection plan (only where guardrails, nets or personal fall arrest are not feasible, 1926.502(k))


4. EMERGENCY ARRANGEMENTS
	Emergency number: 911
	

	Nearest hospital
	

	Assembly point
	

	First aid / CPR person
	

	First aid kit location
	

	Fire extinguisher location
	


5. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: OSH Act Section 5(a)(1) and 29 CFR 1926, Safety and Health Regulations for Construction (incl. 1926.20 and 1926.21).
Keep this JHA on site during the job, and keep it with the training and inspection records for at least 1 year after the job (longer if your state plan or general contractor requires it). OSHA does not set a retention period for JHAs themselves.
6. SIGN-OFF
By signing below, each person confirms they have read and understood this JHA and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/us/jha/demolition/bonded-asbestos-removal/
