JOB HAZARD ANALYSIS (JHA)
Site cut and levelling · Excavation and earthworks · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client / general contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by
	

	Document number and revision
	

	Competent person
	

	Review date
	


2. JOB STEPS, HAZARDS AND CONTROLS
	#
	Job step
	Hazards
	Risk before
	Controls
	Risk after
	Responsible

	1
	Get 811 locates, check for overhead power lines and plan truck movements
	Hitting underground services
Contact with overhead power lines
Road traffic
	Critical
	- Keep machine buckets well clear of marked services and use a spotter. [Engineering (guarding)]
- Scan the area with a cable locator before digging and mark services on the ground. [Engineering]
- Hand dig or vacuum excavate to expose services before using a machine near them. [Engineering]
- Call 811 before you dig and wait until all utilities have marked their lines. [Administrative]
- Keep plans or locate tickets on site and check them again if the work area grows. [Administrative]
- Support or protect exposed utilities so they cannot sag or break while the excavation is open (29 CFR 1926.651(b)(4)). [Administrative]
- Ask the utility to de-energize, move or insulate the lines before work starts. [Elimination]
- Use non-conductive (fiberglass) ladders near any power lines. [Substitution]
- Mark the safe distance with flags, tape or warning lines and keep all equipment and people outside it. [Engineering (guarding)]
- Keep equipment at least 10 feet from lines up to 50 kV once the utility confirms the voltage, more for higher voltages, and 20 feet when the voltage is unknown (29 CFR 1926.1408). [Administrative]
- Use a dedicated spotter whenever equipment moves or raises anything near lines. [Administrative]
- Treat all lines as energized. If equipment touches a line, the operator stays in the cab and everyone else keeps well away. [Administrative]
- Do the work at low-traffic times, or close the road or lane with approval. [Elimination]
- Put solid barriers between the work and traffic where speeds are high, not just cones. [Engineering (guarding)]
- Use a truck-mounted attenuator or buffer vehicle on high speed roads. [Engineering]
- Set up work zone signs and cones to MUTCD Part 6, with trained flaggers. [Administrative]
- Get any permit needed from the city, county or state DOT before you start. [Administrative]
	Medium
	

	2
	Set up a spotter and exclusion zones for machines
	Being hit by heavy equipment
	Critical
	- Separate people and equipment with barriers, exclusion zones and marked walkways. [Engineering (guarding)]
- Use equipment with working backup alarms, cameras and lights. [Engineering]
- Have a site traffic plan showing equipment routes, loading areas and pedestrian paths. [Administrative]
- Use a spotter when backing up or working near people. [Administrative]
- Make eye contact with the operator before going near. Stay out of the swing radius. [Administrative]
- Operators are trained and authorized for each machine. Forklift and telehandler operators are trained, evaluated and certified by the employer (29 CFR 1910.178(l), via 1926.602(d)). [Administrative]
- Do a pre-start check on each machine every day and record it. [Administrative]
- Wear hi-vis clothing and a hard hat. [PPE]
	Medium
	

	3
	Cut the site, battering or retaining cut faces
	Trench or excavation collapse
Structural collapse during alterations
	Critical
	- Use methods that keep people out of the trench, such as directional boring or working from the surface. [Elimination]
- Barricade or cover the excavation so people and equipment cannot fall in. Use guardrails on walkways that cross it (29 CFR 1926.651(l)). [Engineering (guarding)]
- Use a protective system (sloping, shoring or a trench box) in any trench 5 feet or deeper, or shallower if the competent person sees signs of a possible cave-in (29 CFR 1926.652). [Engineering]
- Protective systems for trenches over 20 feet deep are designed by a registered professional engineer (29 CFR 1926.652(b), (c)). [Engineering]
- Keep spoil, materials and equipment at least 2 feet back from the edge. [Engineering]
- Provide a ladder, stairway or ramp within 25 feet of workers in trenches 4 feet or deeper. [Engineering]
- Competent person inspects the trench daily, after rain and as conditions change, and tests the air before entry in trenches over 4 feet deep where a hazardous atmosphere could exist (29 CFR 1926.651(g), (k)). [Administrative]
- Nobody works in a trench where water is collecting unless the competent person has controls in place, such as pumping or special support (29 CFR 1926.651(h)). [Administrative]
- Nobody stands under a loaded bucket or near a truck being loaded (29 CFR 1926.651(e)). [Administrative]
- Never work alone in a trench. Watch for water, cracks and bulging walls, and get out if you see them. [Administrative]
- Wear a hard hat, hi-vis and safety boots. [PPE]
- Get an engineer to check before removing any wall, beam, post or bracing that may be load-bearing. [Elimination]
- Keep everyone clear of the area under and next to the work. [Engineering (guarding)]
- Install temporary props, needles or shoring as designed before removing any support. [Engineering]
- Follow the engineer's sequence. Do not change it without approval. [Administrative]
- Check props daily. Do not remove them until the permanent support is in and approved. [Administrative]
- Wear a hard hat and safety boots. [PPE]
	Medium
	

	4
	Watch neighbouring fences and footings near the cut
	Structural collapse during alterations
Public entering the work area
	High
	- Structural collapse during alterations: see step 3 for the full controls [Administrative]
- Fence off the site with secure temporary fencing and lock the gates when you leave. [Engineering (guarding)]
- Give pedestrians a safe, marked path around the work, with ramps for strollers and wheelchairs. [Engineering (guarding)]
- Use hoarding, covered walkways or catch fans where work is above public areas. [Engineering]
- Put signs at each entry: site name, contact number and "No unauthorized entry". [Administrative]
- Make the site safe at the end of each day: cover holes, lower plant, remove ladders and lock tools away. [Administrative]
- Use a spotter when moving plant or materials across public paths. [Administrative]
	Medium
	

	5
	Control dust with water
	General dust
Silica dust from concrete, brick, stone and tiles
	Critical
	- Use low-dust products, such as dust-reduced or pre-mixed compounds. [Substitution]
- Seal off the work area with plastic sheeting in occupied buildings. [Engineering (guarding)]
- Use tools with dust extraction and a vacuum for clean up. [Engineering]
- Lightly mist the area with water to keep dust down, away from anything electrical. [Engineering]
- Never dry sweep or blow dust off with compressed air. [Administrative]
- Wear a dust mask and safety glasses. [PPE]
- Order materials cut to size, or use low-dust methods such as score and snap or a block splitter. [Substitution]
- Cut outdoors or in a separate area, with other people well away and upwind. [Engineering (guarding)]
- Use wet cutting or on-tool dust collection with a HEPA vacuum, as set out in Table 1 of 29 CFR 1926.1153. [Engineering]
- Clean up with a vacuum or wet methods. Never dry sweep or use compressed air. [Administrative]
- Have a written exposure control plan and a competent person for silica (29 CFR 1926.1153). [Administrative]
- Workers who must wear a respirator 30 or more days a year get a free medical exam every 3 years (29 CFR 1926.1153(h)). [Administrative]
- Wear the respirator Table 1 lists for the task: APF 10 (a fit-tested N95 or half mask) for most tasks, APF 25 (such as a loose-fitting PAPR) for tuckpointing with a handheld grinder for more than 4 hours a shift. [PPE]
	Medium
	

	6
	Load trucks and clean the street
	Road traffic
Poor housekeeping and waste
	Critical
	- Park work vehicles to shield the work zone, with beacons on. [Administrative]
- Wear ANSI/ISEA 107 Class 2 or 3 high-visibility clothing. [PPE]
- Road traffic: see step 1 for the full controls [Administrative]
- Order materials to size and send packaging back where you can. [Elimination]
- Put dumpsters and waste chutes close to the work. [Engineering]
- Clean as you go, and do a full clean up at the end of each day. [Administrative]
- Keep exits, stairs and walkways clear at all times. [Administrative]
- Stack materials neatly on level ground, away from edges. [Administrative]
- Wear gloves when handling waste. [PPE]
	Medium
	


3. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Safety-toe boots (ASTM F2413)
High-visibility safety apparel, ANSI/ISEA 107 Class 2 or 3 (Type R near roadways)
Hard hat (ANSI Z89.1)
Hearing protection (earmuffs or plugs)
N95 respirator
Safety glasses (ANSI Z87.1)
Half-face respirator (P100 cartridges)
Work gloves
	Excavator
Skid steer
Dump truck (CDL if the truck's GVWR, or the combination's GCWR, is 26,001 lb or more (49 CFR 383.5), or if it carries placarded hazmat)
Plate compactor
	811 locate ticket / excavation permit


4. EMERGENCY ARRANGEMENTS
	Emergency number: 911
	

	Nearest hospital
	

	Assembly point
	

	First aid / CPR person
	

	First aid kit location
	

	Fire extinguisher location
	


5. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: OSH Act Section 5(a)(1) and 29 CFR 1926, Safety and Health Regulations for Construction (incl. 1926.20 and 1926.21).
Keep this JHA on site during the job, and keep it with the training and inspection records for at least 1 year after the job (longer if your state plan or general contractor requires it). OSHA does not set a retention period for JHAs themselves.
6. SIGN-OFF
By signing below, each person confirms they have read and understood this JHA and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/us/jha/excavation/site-cut-levelling/
