JOB HAZARD ANALYSIS (JHA)
Shower screen installation · Glazing · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client / general contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by
	

	Document number and revision
	

	Competent person
	

	Review date
	


2. JOB STEPS, HAZARDS AND CONTROLS
	#
	Job step
	Hazards
	Risk before
	Controls
	Risk after
	Responsible

	1
	Check walls for pipes and cables before drilling
	Electric shock from live wiring
	Critical
	- Isolate the power before any work. Do not work live. [Elimination]
- Lock out and tag the disconnecting means with your own personal lock and tag so the circuit cannot be energized (29 CFR 1926.417). [Engineering (guarding)]
- Test before you touch: prove dead at the point of work with a tested voltage tester. [Engineering]
- Only qualified persons work on or near exposed energized parts. [Administrative]
- Check for back feeds from solar, batteries and generators that can keep a circuit live after the main switch is off. [Administrative]
- If energized work cannot be avoided, use an energized work permit, a safety observer and insulated tools, following NFPA 70E. [Administrative]
- Wear insulated gloves, arc-rated clothing and a face shield when testing or working near live parts. [PPE]
	Medium
	

	2
	Carry glass panels with two people
	Lifting and carrying heavy loads
Glass handling and breakage
	High
	- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Elimination]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Substitution]
- Use trolleys, pallet jacks, hoists, vacuum lifters or plant instead of carrying by hand. [Engineering]
- Use a two-person lift for anything heavy, long or awkward. Plan the route first and clear it. [Administrative]
- Keep the load close, back straight and no twisting. Turn with your feet. [Administrative]
- Rotate tasks and take breaks on long lifting jobs. [Administrative]
- Wear gloves for grip and safety boots to protect your feet. [PPE]
- Use suction lifters, glass trolleys or a glazing robot for large panes. [Engineering]
- Store glass upright on racks and secure it. Never lay it flat or lean it loosely. [Engineering]
- Use two or more people for large panes, and clear the carry route first. [Administrative]
- Mark new glass with tape or stickers so nobody walks into it. [Administrative]
- Clean up broken glass straight away into a marked container. [Administrative]
- Wear cut-resistant gloves, arm guards, safety glasses and safety boots. [PPE]
	Medium
	

	3
	Drill tiles with the right bit and glasses on
	Injury from power tools
Eye injuries
	Medium
	- Keep all guards fitted and working. Never tie back or remove a guard. [Engineering]
- Clamp or secure the work piece. Do not hold it by hand. [Engineering]
- Only trained, competent people use power tools, following the maker's instructions. [Administrative]
- Check tools before use. Unplug or remove the battery before changing blades or bits. [Administrative]
- No loose clothing, jewelry or long hair near spinning parts. [Administrative]
- Wear safety glasses and hearing protection. Do not wear loose gloves on drills or other rotating tools. [PPE]
- Use tool guards and screens to stop flying particles. [Engineering]
- Use dust extraction and water to keep dust out of the air. [Engineering]
- Keep others out of the area when cutting, grinding or chipping. [Administrative]
- Keep an eye wash station or eye wash bottles on site. [Administrative]
- Wear safety glasses at all times, goggles for dust and chemicals, and a face shield for grinding. [PPE]
	Medium
	

	4
	Fit and silicone the screen with ventilation
	Hazardous chemicals
	Medium
	- Choose the least harmful product that does the job, for example water-based instead of solvent-based. [Substitution]
- Use chemicals in well-ventilated areas, or use fans and extraction in closed rooms. [Engineering]
- Read the Safety Data Sheet (SDS) and labels before use, following OSHA Hazard Communication. [Administrative]
- Keep chemicals in labeled containers. Never pour them into drink bottles. [Administrative]
- Store chemicals away from heat, food and drink, and keep products that react with each other apart. [Administrative]
- Have eye wash and a spill kit nearby, and wash hands before eating. [Administrative]
- Wear chemical-resistant gloves and safety glasses or goggles as listed on the SDS. [PPE]
- Use a respirator with the right cartridge if the SDS calls for one. [PPE]
	Medium
	

	5
	Clean up
	Poor housekeeping and waste
Slips and trips
	Medium
	- Order materials to size and send packaging back where you can. [Elimination]
- Put dumpsters and waste chutes close to the work. [Engineering]
- Clean as you go, and do a full clean up at the end of each day. [Administrative]
- Keep exits, stairs and walkways clear at all times. [Administrative]
- Stack materials neatly on level ground, away from edges. [Administrative]
- Wear gloves when handling waste. [PPE]
- Plan walkways and keep them clear of materials, hoses and leads. [Elimination]
- Run cords and hoses overhead on hooks or stands, or along walls, not across walkways. [Engineering]
- Fill or cover holes, and lay boards or mats on muddy access paths. [Engineering]
- Clean up offcuts, packaging and spills as you go, not at the end of the day. [Administrative]
- Keep work areas, stairs and access paths well lit. [Administrative]
- Wear safety boots with good grip, laced up. [PPE]
	Low
	


3. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Cut-resistant gloves
Safety glasses (ANSI Z87.1)
Safety-toe boots (ASTM F2413)
Work gloves
Hearing protection (earmuffs or plugs)
Safety goggles (ANSI Z87.1)
Face shield (ANSI Z87.1)
Chemical-resistant gloves
Half-face respirator (P100 cartridges)
Coveralls
	Power drill
Hand tools
	None required


4. EMERGENCY ARRANGEMENTS
	Emergency number: 911
	

	Nearest hospital
	

	Assembly point
	

	First aid / CPR person
	

	First aid kit location
	

	Fire extinguisher location
	


5. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: OSH Act Section 5(a)(1) and 29 CFR 1926, Safety and Health Regulations for Construction (incl. 1926.20 and 1926.21).
Keep this JHA on site during the job, and keep it with the training and inspection records for at least 1 year after the job (longer if your state plan or general contractor requires it). OSHA does not set a retention period for JHAs themselves.
6. SIGN-OFF
By signing below, each person confirms they have read and understood this JHA and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/us/jha/glazing/shower-screen-installation/
