JOB HAZARD ANALYSIS (JHA)
Epoxy floor coating · Painting · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client / general contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by
	

	Document number and revision
	

	Competent person
	

	Review date
	


2. JOB STEPS, HAZARDS AND CONTROLS
	#
	Job step
	Hazards
	Risk before
	Controls
	Risk after
	Responsible

	1
	Close the area and set up fresh air ventilation
	Hazardous chemicals
Confined space entry
	High
	- Choose the least harmful product that does the job, for example water-based instead of solvent-based. [Substitution]
- Use chemicals in well-ventilated areas, or use fans and extraction in closed rooms. [Engineering]
- Hazardous chemicals: see step 3 for the full controls [Administrative]
- Do the work from outside the space where you can, using cameras or long-reach tools. [Elimination]
- Isolate and lock out all pipes, power and moving parts going into the space. [Engineering (guarding)]
- Test the air for oxygen, flammable and toxic gases before entry, and keep testing during the work. [Engineering]
- Use forced ventilation to keep the air clean. [Engineering]
- Use a permit-required confined space program with a written entry permit (29 CFR 1926 Subpart AA). Only trained workers enter. [Administrative]
- Keep a trained standby person outside at all times, in contact with those inside. [Administrative]
- Set up a rescue plan and rescue gear before entry. Never go in to rescue without the right gear. [Administrative]
- Wear a harness for retrieval and the respirator the air test calls for. [PPE]
	Medium
	

	2
	Grind the slab with extraction to prepare the surface
	Silica dust from concrete, brick, stone and tiles
Loud noise
Angle grinder injuries
	Critical
	- Order materials cut to size, or use low-dust methods such as score and snap or a block splitter. [Substitution]
- Cut outdoors or in a separate area, with other people well away and upwind. [Engineering (guarding)]
- Use wet cutting or on-tool dust collection with a HEPA vacuum, as set out in Table 1 of 29 CFR 1926.1153. [Engineering]
- Clean up with a vacuum or wet methods. Never dry sweep or use compressed air. [Administrative]
- Have a written exposure control plan and a competent person for silica (29 CFR 1926.1153). [Administrative]
- Workers who must wear a respirator 30 or more days a year get a free medical exam every 3 years (29 CFR 1926.1153(h)). [Administrative]
- Wear the respirator Table 1 lists for the task: APF 10 (a fit-tested N95 or half mask) for most tasks, APF 25 (such as a loose-fitting PAPR) for tuckpointing with a handheld grinder for more than 4 hours a shift. [PPE]
- Use quieter tools and methods, such as cut-to-size materials, low-noise machines and battery tools. [Substitution]
- Keep noisy plant away from work areas, and use screens or distance between the noise and people. [Engineering (guarding)]
- Keep tools maintained and use mufflers on compressors and generators. [Engineering]
- Limit time on noisy tools and rotate workers. [Administrative]
- If you have to shout to be heard at arm's length, wear hearing protection. [Administrative]
- Use a guarded saw or a different tool where you can. [Substitution]
- Keep the guard on and use the side handle. Never remove the guard. [Engineering]
- Use the right disc for the job, rated for the grinder's speed. Check it for cracks first. [Administrative]
- Only trained people change discs, with the grinder unplugged or the battery out. [Administrative]
- Keep both hands on the grinder and let the disc stop before putting it down. [Administrative]
	Medium
	

	3
	Mix epoxy with gloves and goggles, and avoid skin contact
	Hazardous chemicals
Eye injuries
	Medium
	- Choose the least harmful product that does the job, for example water-based instead of solvent-based. [Substitution]
- Use chemicals in well-ventilated areas, or use fans and extraction in closed rooms. [Engineering]
- Read the Safety Data Sheet (SDS) and labels before use, following OSHA Hazard Communication. [Administrative]
- Keep chemicals in labeled containers. Never pour them into drink bottles. [Administrative]
- Store chemicals away from heat, food and drink, and keep products that react with each other apart. [Administrative]
- Have eye wash and a spill kit nearby, and wash hands before eating. [Administrative]
- Wear chemical-resistant gloves and safety glasses or goggles as listed on the SDS. [PPE]
- Use a respirator with the right cartridge if the SDS calls for one. [PPE]
- Use tool guards and screens to stop flying particles. [Engineering]
- Use dust extraction and water to keep dust out of the air. [Engineering]
- Keep others out of the area when cutting, grinding or chipping. [Administrative]
- Keep an eye wash station or eye wash bottles on site. [Administrative]
- Wear safety glasses at all times, goggles for dust and chemicals, and a face shield for grinding. [PPE]
	Medium
	

	4
	Roll coats on, working towards the exit
	Repetitive work and awkward postures
Flammable liquids and gases
	High
	- Use tools that cut the effort: powered screwdrivers, long-handled tools and extension poles for overhead work. [Substitution]
- Set work up at waist height on benches or trestles where you can. [Engineering]
- Use light tools with good grips, and keep blades and bits sharp. [Engineering]
- Rotate tasks and take short breaks every hour on repetitive work. [Administrative]
- Warm up before heavy physical work and report aches and pains early. [Administrative]
- Wear knee pads for kneeling work and gloves for grip. [PPE]
- Use non-flammable or water-based products where you can. [Substitution]
- Keep ignition sources away: no smoking, no hot work and no running engines near flammables. [Engineering (guarding)]
- Store fuels and solvents in approved, closed containers in a ventilated area away from the work. [Engineering]
- Refuel equipment outdoors with the engine off and cool. [Administrative]
- Keep only what you need for the day on site. [Administrative]
- Store gas cylinders upright, secured and outdoors. [Administrative]
- Keep a suitable fire extinguisher where flammables are used or stored. [Administrative]
- Wear chemical gloves and safety glasses when pouring or mixing. [PPE]
	Medium
	

	5
	Keep the floor closed until cured and dispose of empty kits
	Slips and trips
Poor housekeeping and waste
	Medium
	- Plan walkways and keep them clear of materials, hoses and leads. [Elimination]
- Run cords and hoses overhead on hooks or stands, or along walls, not across walkways. [Engineering]
- Fill or cover holes, and lay boards or mats on muddy access paths. [Engineering]
- Clean up offcuts, packaging and spills as you go, not at the end of the day. [Administrative]
- Keep work areas, stairs and access paths well lit. [Administrative]
- Wear safety boots with good grip, laced up. [PPE]
- Order materials to size and send packaging back where you can. [Elimination]
- Put dumpsters and waste chutes close to the work. [Engineering]
- Clean as you go, and do a full clean up at the end of each day. [Administrative]
- Keep exits, stairs and walkways clear at all times. [Administrative]
- Stack materials neatly on level ground, away from edges. [Administrative]
- Wear gloves when handling waste. [PPE]
	Low
	


3. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Half-face respirator (P100 cartridges)
Chemical-resistant gloves
Safety goggles (ANSI Z87.1)
Knee pads
Safety-toe boots (ASTM F2413)
Coveralls
Safety glasses (ANSI Z87.1)
Hearing protection (earmuffs or plugs)
Face shield (ANSI Z87.1)
Cut-resistant gloves
Work gloves
	Angle grinder
HEPA vacuum
Hand tools
	None required


4. EMERGENCY ARRANGEMENTS
	Emergency number: 911
	

	Nearest hospital
	

	Assembly point
	

	First aid / CPR person
	

	First aid kit location
	

	Fire extinguisher location
	


5. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: OSH Act Section 5(a)(1) and 29 CFR 1926, Safety and Health Regulations for Construction (incl. 1926.20 and 1926.21).
Keep this JHA on site during the job, and keep it with the training and inspection records for at least 1 year after the job (longer if your state plan or general contractor requires it). OSHA does not set a retention period for JHAs themselves.
6. SIGN-OFF
By signing below, each person confirms they have read and understood this JHA and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/us/jha/painting/epoxy-floor-coating/
