JOB HAZARD ANALYSIS (JHA)
Scaffold inspection and handover · Scaffolding · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client / general contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by
	

	Document number and revision
	

	Competent person
	

	Review date
	


2. JOB STEPS, HAZARDS AND CONTROLS
	#
	Job step
	Hazards
	Risk before
	Controls
	Risk after
	Responsible

	1
	Inspect after erection, weekly, and after storms or changes
	Scaffold collapse or fall from scaffold
Strong wind and storms
	Critical
	- Scaffold is built, moved and taken down under the supervision of a competent person. [Engineering]
- Fit guardrails, mid rails and toe boards on every platform more than 10 feet above a lower level, or use personal fall arrest (29 CFR 1926.451(g)(1)). [Engineering]
- Scaffold collapse or fall from scaffold: see step 2 for the full controls [Administrative]
- Check the forecast each morning and plan work at height and lifting around the weather. [Elimination]
- Tie down or weigh down loose sheets, panels, boards and rubbish at the end of each shift. [Engineering]
- Set wind limits for roof work, platforms and cranes, using the manufacturer's limits, and stop when they are reached. [Administrative]
- Stop work and get down in lightning. Wait 30 minutes after the last thunder before going back up. [Administrative]
- Check scaffold, fencing and edge protection after strong wind before anyone uses them. [Administrative]
- Do not carry large sheets on roofs in wind. [Administrative]
- Wear a hard hat with a chin strap at height in windy conditions. [PPE]
	Medium
	

	2
	Check base, ties, bracing, planks, guardrails and toe boards
	Scaffold collapse or fall from scaffold
Falling tools and materials
	Critical
	- Scaffold is built, moved and taken down under the supervision of a competent person. [Engineering]
- Fit guardrails, mid rails and toe boards on every platform more than 10 feet above a lower level, or use personal fall arrest (29 CFR 1926.451(g)(1)). [Engineering]
- Use mobile scaffolds only on firm, level ground with casters locked, and guy, tie, brace or fit outriggers once the height is more than 4 times the base width (29 CFR 1926.451(c)(1)). Never move one with anyone on it. [Engineering]
- Every worker on the scaffold is trained by a qualified person (29 CFR 1926.454). [Administrative]
- A competent person inspects the scaffold before each shift and after anything that could affect it (29 CFR 1926.451(f)(3)). [Administrative]
- Do not overload platforms. Know the rated load (light, medium or heavy duty) and stack materials over the legs, not mid-span (29 CFR 1926.451(f)(1)). [Administrative]
- Never remove ties, braces, guardrails or planks. Only the erection crew alters the scaffold, under the direction of the competent person (29 CFR 1926.451(f)(7)). [Administrative]
- Wear a hard hat and safety boots on and around the scaffold. [PPE]
- Barricade and sign the drop zone under overhead work so nobody walks beneath. [Engineering (guarding)]
- Fit toe boards, kick plates and mesh screens on scaffolds and edges. [Engineering]
- Use catch fans, debris netting or covered walkways where people pass below. [Engineering]
- Tether hand tools when working at height. [Engineering]
- Keep platforms tidy. Do not stack materials near edges or above toe board height. [Administrative]
- Lower materials with a hoist, chute or rope. Never throw or drop anything down. [Administrative]
- Wear a hard hat anywhere objects could fall. [PPE]
	Medium
	

	3
	Check access, ladder gates and loading limits
	Falling from height
Falling from a ladder
	Critical
	- Do the work from the ground where you can, for example pre-assemble on the ground or use extension poles. [Elimination]
- Install guardrails or edge protection on all open edges before work starts. [Engineering (guarding)]
- Use a scaffold, mobile work platform or aerial lift instead of working off a ladder. [Engineering]
- Where edge protection is not practical, use a fall restraint or fall arrest system on a rated anchor point. [Engineering]
- Provide fall protection at 6 feet or more and train workers to recognize fall hazards (29 CFR 1926.503). [Administrative]
- Have a rescue plan so a worker hanging in a harness can be brought down within minutes. [Administrative]
- Wear a full body harness with a shock-absorbing lanyard, clipped on at all times when using fall arrest. [PPE]
- Use a platform ladder, mobile scaffold or aerial lift for longer jobs instead of a straight ladder. [Substitution]
- Use Type I, IA or IAA ladders in good condition. Tag and remove any damaged ladder. [Engineering]
- Set extension ladders at a 4 to 1 angle on firm, level ground, secured, and reaching 3 feet above the landing. [Engineering]
- Use ladders only for short, light work. Do not carry heavy or awkward loads up a ladder. [Administrative]
- Keep three points of contact and your belt buckle between the stiles. Do not overreach. [Administrative]
- Do not stand on the top three rungs of an extension ladder or the top step of a stepladder. [Administrative]
- Check the ladder before each use: feet, rungs, side rails and locks. [Administrative]
- Wear non-slip safety boots with clean soles. [PPE]
	Medium
	

	4
	Tag the scaffold safe or not safe and record it
	Scaffold collapse or fall from scaffold
	Critical
	- Scaffold collapse or fall from scaffold: see step 2 for the full controls [Administrative]
	Medium
	


3. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Safety-toe boots (ASTM F2413)
Hard hat (ANSI Z89.1)
High-visibility safety apparel, ANSI/ISEA 107 Class 2 or 3 (Type R near roadways)
Safety glasses (ANSI Z87.1)
	Supported scaffold (Erected under a competent person (29 CFR 1926.451))
Mobile (rolling) scaffold (Erected under a competent person (29 CFR 1926.451))
	Written fall protection plan (only where guardrails, nets or personal fall arrest are not feasible, 1926.502(k))


4. EMERGENCY ARRANGEMENTS
	Emergency number: 911
	

	Nearest hospital
	

	Assembly point
	

	First aid / CPR person
	

	First aid kit location
	

	Fire extinguisher location
	


5. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: OSH Act Section 5(a)(1) and 29 CFR 1926, Safety and Health Regulations for Construction (incl. 1926.20 and 1926.21).
Keep this JHA on site during the job, and keep it with the training and inspection records for at least 1 year after the job (longer if your state plan or general contractor requires it). OSHA does not set a retention period for JHAs themselves.
6. SIGN-OFF
By signing below, each person confirms they have read and understood this JHA and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/us/jha/scaffolding/scaffold-inspection-handover/
