JOB HAZARD ANALYSIS (JHA)
Solar panel removal and reinstall · Solar · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client / general contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by
	

	Document number and revision
	

	Competent person
	

	Review date
	


2. JOB STEPS, HAZARDS AND CONTROLS
	#
	Job step
	Hazards
	Risk before
	Controls
	Risk after
	Responsible

	1
	Shut down the system and isolate AC and DC
	Electric shock from live wiring
Stored energy
	Critical
	- Isolate the power before any work. Do not work live. [Elimination]
- Lock out and tag the disconnecting means with your own personal lock and tag so the circuit cannot be energized (29 CFR 1926.417). [Engineering (guarding)]
- Test before you touch: prove dead at the point of work with a tested voltage tester. [Engineering]
- Only qualified persons work on or near exposed energized parts. [Administrative]
- Check for back feeds from solar, batteries and generators that can keep a circuit live after the main switch is off. [Administrative]
- If energized work cannot be avoided, use an energized work permit, a safety observer and insulated tools, following NFPA 70E. [Administrative]
- Wear insulated gloves, arc-rated clothing and a face shield when testing or working near live parts. [PPE]
- Release or block all stored energy before work: release the pressure in pipes, tanks and hoses, bleed hydraulics, release springs, lower loads. [Elimination]
- Lock out and tag all energy sources with personal locks. [Engineering (guarding)]
- Put mechanical blocks or props under raised parts like buckets, tipper bodies and doors. [Engineering]
- Test that the system is dead and nothing can move before you start. [Administrative]
- Follow the maker's procedure, for example for garage door and roller door springs. [Administrative]
- Wear safety glasses and gloves. [PPE]
	Medium
	

	2
	Set up edge protection and roof access
	Falling from a roof edge
Falling from a ladder
	Critical
	- Do what you can from the ground or from a scaffold at the gutter line, for example pre-assemble parts on the ground. [Elimination]
- Install edge protection or guardrails on all open roof edges before work starts. [Engineering (guarding)]
- Use a perimeter scaffold with handrails and toe boards along the eaves where practical. [Engineering]
- Where guardrails cannot be fitted, use fall restraint on certified roof anchors so workers cannot reach the edge. [Engineering]
- Low-slope roofs: guardrails, safety nets, personal fall arrest, or a warning line combined with one of these or with a safety monitor (a safety monitor alone only on roofs 50 feet wide or less). Steep roofs: guardrails with toe boards, safety nets or personal fall arrest (29 CFR 1926.501(b)(10), (11)). [Administrative]
- Use one safe, controlled access point and keep others off the roof. [Administrative]
- Stop roof work in strong wind or rain, and when the roof is wet, icy or covered in dust or frost. [Administrative]
- Wear a harness clipped to a rated anchor when using restraint or fall arrest, and soft-soled non-slip boots. [PPE]
- Use a platform ladder, mobile scaffold or aerial lift for longer jobs instead of a straight ladder. [Substitution]
- Use Type I, IA or IAA ladders in good condition. Tag and remove any damaged ladder. [Engineering]
- Set extension ladders at a 4 to 1 angle on firm, level ground, secured, and reaching 3 feet above the landing. [Engineering]
- Use ladders only for short, light work. Do not carry heavy or awkward loads up a ladder. [Administrative]
- Keep three points of contact and your belt buckle between the stiles. Do not overreach. [Administrative]
- Do not stand on the top three rungs of an extension ladder or the top step of a stepladder. [Administrative]
- Check the ladder before each use: feet, rungs, side rails and locks. [Administrative]
- Wear non-slip safety boots with clean soles. [PPE]
	Medium
	

	3
	Disconnect panels, covering connectors
	Electric shock from live wiring
	Critical
	- Electric shock from live wiring: see step 1 for the full controls [Administrative]
	Medium
	

	4
	Lower panels by hoist and store them flat
	Lifting and carrying heavy loads
Falling tools and materials
Glass handling and breakage
	High
	- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Elimination]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Substitution]
- Use trolleys, pallet jacks, hoists, vacuum lifters or plant instead of carrying by hand. [Engineering]
- Use a two-person lift for anything heavy, long or awkward. Plan the route first and clear it. [Administrative]
- Keep the load close, back straight and no twisting. Turn with your feet. [Administrative]
- Barricade and sign the drop zone under overhead work so nobody walks beneath. [Engineering (guarding)]
- Fit toe boards, kick plates and mesh screens on scaffolds and edges. [Engineering]
- Use catch fans, debris netting or covered walkways where people pass below. [Engineering]
- Tether hand tools when working at height. [Engineering]
- Keep platforms tidy. Do not stack materials near edges or above toe board height. [Administrative]
- Use suction lifters, glass trolleys or a glazing robot for large panes. [Engineering]
- Store glass upright on racks and secure it. Never lay it flat or lean it loosely. [Engineering]
- Use two or more people for large panes, and clear the carry route first. [Administrative]
- Mark new glass with tape or stickers so nobody walks into it. [Administrative]
- Clean up broken glass straight away into a marked container. [Administrative]
	Medium
	

	5
	Reinstall, test and recommission
	Electric shock from live wiring
Poor housekeeping and waste
	Critical
	- Electric shock from live wiring: see step 1 for the full controls [Administrative]
- Order materials to size and send packaging back where you can. [Elimination]
- Put dumpsters and waste chutes close to the work. [Engineering]
- Clean as you go, and do a full clean up at the end of each day. [Administrative]
- Keep exits, stairs and walkways clear at all times. [Administrative]
- Stack materials neatly on level ground, away from edges. [Administrative]
- Wear gloves when handling waste. [PPE]
	Medium
	


3. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Safety-toe boots (ASTM F2413)
Personal fall arrest system (harness)
Rubber insulating gloves
Safety glasses (ANSI Z87.1)
Arc flash PPE (NFPA 70E)
Work gloves
Sun protection (sunscreen, hat, long sleeves)
Hard hat (ANSI Z89.1)
Cut-resistant gloves
	Extension ladder
Supported scaffold (Erected under a competent person (29 CFR 1926.451))
Electrical test meter
Hand tools
	Lockout/tagout (1926.417)
Written fall protection plan (only where guardrails, nets or personal fall arrest are not feasible, 1926.502(k))


4. EMERGENCY ARRANGEMENTS
	Emergency number: 911
	

	Nearest hospital
	

	Assembly point
	

	First aid / CPR person
	

	First aid kit location
	

	Fire extinguisher location
	


5. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: OSH Act Section 5(a)(1) and 29 CFR 1926, Safety and Health Regulations for Construction (incl. 1926.20 and 1926.21).
Keep this JHA on site during the job, and keep it with the training and inspection records for at least 1 year after the job (longer if your state plan or general contractor requires it). OSHA does not set a retention period for JHAs themselves.
6. SIGN-OFF
By signing below, each person confirms they have read and understood this JHA and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/us/jha/solar/solar-removal-reinstall/
