JOB HAZARD ANALYSIS (JHA)
Floor tiling · Tiling · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client / general contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by
	

	Document number and revision
	

	Competent person
	

	Review date
	


2. JOB STEPS, HAZARDS AND CONTROLS
	#
	Job step
	Hazards
	Risk before
	Controls
	Risk after
	Responsible

	1
	Prepare and level the floor, grinding with extraction
	Silica dust from concrete, brick, stone and tiles
Loud noise
	Critical
	- Order materials cut to size, or use low-dust methods such as score and snap or a block splitter. [Substitution]
- Cut outdoors or in a separate area, with other people well away and upwind. [Engineering (guarding)]
- Use wet cutting or on-tool dust collection with a HEPA vacuum, as set out in Table 1 of 29 CFR 1926.1153. [Engineering]
- Clean up with a vacuum or wet methods. Never dry sweep or use compressed air. [Administrative]
- Have a written exposure control plan and a competent person for silica (29 CFR 1926.1153). [Administrative]
- Workers who must wear a respirator 30 or more days a year get a free medical exam every 3 years (29 CFR 1926.1153(h)). [Administrative]
- Wear the respirator Table 1 lists for the task: APF 10 (a fit-tested N95 or half mask) for most tasks, APF 25 (such as a loose-fitting PAPR) for tuckpointing with a handheld grinder for more than 4 hours a shift. [PPE]
- Use quieter tools and methods, such as cut-to-size materials, low-noise machines and battery tools. [Substitution]
- Keep noisy plant away from work areas, and use screens or distance between the noise and people. [Engineering (guarding)]
- Keep tools maintained and use mufflers on compressors and generators. [Engineering]
- Limit time on noisy tools and rotate workers. [Administrative]
- If you have to shout to be heard at arm's length, wear hearing protection. [Administrative]
- Wear earplugs or earmuffs rated for the noise. [PPE]
	Medium
	

	2
	Move tile boxes with a trolley
	Lifting and carrying heavy loads
	High
	- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Elimination]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Substitution]
- Use trolleys, pallet jacks, hoists, vacuum lifters or plant instead of carrying by hand. [Engineering]
- Use a two-person lift for anything heavy, long or awkward. Plan the route first and clear it. [Administrative]
- Keep the load close, back straight and no twisting. Turn with your feet. [Administrative]
- Rotate tasks and take breaks on long lifting jobs. [Administrative]
- Wear gloves for grip and safety boots to protect your feet. [PPE]
	Medium
	

	3
	Cut tiles wet
	Silica dust from concrete, brick, stone and tiles
Saw cuts and kickback
Electric shock from cords and power tools
	Critical
	- Silica dust from concrete, brick, stone and tiles: see step 1 for the full controls [Administrative]
- Keep blade guards fitted and working, and use the riving knife on table saws. [Engineering]
- Use push sticks and clamps, and support long pieces so they do not pinch the blade. [Engineering]
- Use a sharp, undamaged blade made for the material. [Administrative]
- Stand to one side of the blade line, out of the kickback path. [Administrative]
- Let the blade stop fully before reaching in or putting the saw down. [Administrative]
- Use battery-powered tools where you can. [Substitution]
- Use GFCIs on all 120-volt, 15, 20 and 30 amp temporary receptacles, or a written assured equipment grounding conductor program run by a competent person with recorded tests (29 CFR 1926.404(b)(1)). [Engineering]
- Keep cords off the ground and out of water, using stands or hooks. [Engineering]
- Check cords, plugs and tools before every use. Tag out and remove anything damaged. [Administrative]
- Do not use tools in rain or wet areas unless they are rated for it. [Administrative]
	Medium
	

	4
	Lay tiles, taking breaks from kneeling
	Repetitive work and awkward postures
Cuts from sharp edges
	Medium
	- Use tools that cut the effort: powered screwdrivers, long-handled tools and extension poles for overhead work. [Substitution]
- Set work up at waist height on benches or trestles where you can. [Engineering]
- Use light tools with good grips, and keep blades and bits sharp. [Engineering]
- Rotate tasks and take short breaks every hour on repetitive work. [Administrative]
- Warm up before heavy physical work and report aches and pains early. [Administrative]
- Wear knee pads for kneeling work and gloves for grip. [PPE]
- Deburr or cover sharp edges, and fit edge protectors on exposed sheet metal. [Engineering]
- Use knives with retractable or self-retracting blades. [Engineering]
- Cut away from your body and keep your other hand clear. [Administrative]
- Put used blades in a blade bin or sharps container. [Administrative]
- Use two people to handle large sheets of metal or glass. [Administrative]
- Wear cut-resistant gloves and long sleeves. [PPE]
	Medium
	

	5
	Grout, seal and keep traffic off
	Hazardous chemicals
Slips and trips
	Medium
	- Choose the least harmful product that does the job, for example water-based instead of solvent-based. [Substitution]
- Use chemicals in well-ventilated areas, or use fans and extraction in closed rooms. [Engineering]
- Read the Safety Data Sheet (SDS) and labels before use, following OSHA Hazard Communication. [Administrative]
- Keep chemicals in labeled containers. Never pour them into drink bottles. [Administrative]
- Store chemicals away from heat, food and drink, and keep products that react with each other apart. [Administrative]
- Have eye wash and a spill kit nearby, and wash hands before eating. [Administrative]
- Wear chemical-resistant gloves and safety glasses or goggles as listed on the SDS. [PPE]
- Use a respirator with the right cartridge if the SDS calls for one. [PPE]
- Plan walkways and keep them clear of materials, hoses and leads. [Elimination]
- Run cords and hoses overhead on hooks or stands, or along walls, not across walkways. [Engineering]
- Fill or cover holes, and lay boards or mats on muddy access paths. [Engineering]
- Clean up offcuts, packaging and spills as you go, not at the end of the day. [Administrative]
- Keep work areas, stairs and access paths well lit. [Administrative]
- Wear safety boots with good grip, laced up. [PPE]
	Medium
	


3. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Knee pads
Safety glasses (ANSI Z87.1)
N95 respirator
Chemical-resistant gloves
Safety-toe boots (ASTM F2413)
Half-face respirator (P100 cartridges)
Hearing protection (earmuffs or plugs)
Work gloves
Cut-resistant gloves
Safety goggles (ANSI Z87.1)
Coveralls
	Wet tile saw
Angle grinder
Hand tools
	None required


4. EMERGENCY ARRANGEMENTS
	Emergency number: 911
	

	Nearest hospital
	

	Assembly point
	

	First aid / CPR person
	

	First aid kit location
	

	Fire extinguisher location
	


5. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: OSH Act Section 5(a)(1) and 29 CFR 1926, Safety and Health Regulations for Construction (incl. 1926.20 and 1926.21).
Keep this JHA on site during the job, and keep it with the training and inspection records for at least 1 year after the job (longer if your state plan or general contractor requires it). OSHA does not set a retention period for JHAs themselves.
6. SIGN-OFF
By signing below, each person confirms they have read and understood this JHA and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/us/jha/tiling/floor-tiling/
