JOB HAZARD ANALYSIS (JHA)
Workshop steel fabrication · Welding and fabrication · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client / general contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by
	

	Document number and revision
	

	Competent person
	

	Review date
	


2. JOB STEPS, HAZARDS AND CONTROLS
	#
	Job step
	Hazards
	Risk before
	Controls
	Risk after
	Responsible

	1
	Move steel with a forklift or overhead crane, keeping walkways clear
	Being hit by heavy equipment
Crane and lifting failure
	Critical
	- Separate people and equipment with barriers, exclusion zones and marked walkways. [Engineering (guarding)]
- Use equipment with working backup alarms, cameras and lights. [Engineering]
- Have a site traffic plan showing equipment routes, loading areas and pedestrian paths. [Administrative]
- Use a spotter when backing up or working near people. [Administrative]
- Make eye contact with the operator before going near. Stay out of the swing radius. [Administrative]
- Operators are trained and authorized for each machine. Forklift and telehandler operators are trained, evaluated and certified by the employer (29 CFR 1910.178(l), via 1926.602(d)). [Administrative]
- Do a pre-start check on each machine every day and record it. [Administrative]
- Wear hi-vis clothing and a hard hat. [PPE]
- Barricade the lift zone and keep everyone out from under the load. [Engineering (guarding)]
- Use a crane rated for the load at the radius, set up on firm ground with outrigger pads. [Engineering]
- Check slings, chains, shackles and hooks before use. Remove anything damaged or not tagged. [Engineering]
- Plan the lift: weight, radius, ground, path and landing area. Use a written lift plan for complex lifts. [Administrative]
- Use a certified crane operator who has also been evaluated by the employer, with the evaluation documented on site (29 CFR 1926.1427), plus a qualified rigger (1926.1425) and a qualified signal person (1926.1428). [Administrative]
- Use tag lines to control loads and agree on clear radio or hand signals. [Administrative]
- Stop lifting in high wind or when the operator cannot see the signal person. [Administrative]
- Never ride on a load or hook. [Administrative]
- Wear a hard hat, hi-vis, gloves and safety boots. [PPE]
	Medium
	

	2
	Cut and drill steel with guards in place
	Saw cuts and kickback
Angle grinder injuries
Loud noise
	High
	- Keep blade guards fitted and working, and use the riving knife on table saws. [Engineering]
- Use push sticks and clamps, and support long pieces so they do not pinch the blade. [Engineering]
- Use a sharp, undamaged blade made for the material. [Administrative]
- Stand to one side of the blade line, out of the kickback path. [Administrative]
- Let the blade stop fully before reaching in or putting the saw down. [Administrative]
- Use a guarded saw or a different tool where you can. [Substitution]
- Keep the guard on and use the side handle. Never remove the guard. [Engineering]
- Use the right disc for the job, rated for the grinder's speed. Check it for cracks first. [Administrative]
- Only trained people change discs, with the grinder unplugged or the battery out. [Administrative]
- Keep both hands on the grinder and let the disc stop before putting it down. [Administrative]
- Use quieter tools and methods, such as cut-to-size materials, low-noise machines and battery tools. [Substitution]
- Keep noisy plant away from work areas, and use screens or distance between the noise and people. [Engineering (guarding)]
- Keep tools maintained and use mufflers on compressors and generators. [Engineering]
- Limit time on noisy tools and rotate workers. [Administrative]
- If you have to shout to be heard at arm's length, wear hearing protection. [Administrative]
	Medium
	

	3
	Weld in a booth with extraction
	Welding and cutting fumes
Eye injuries
Fire from hot works
	Critical
	- Remove paint, galvanizing and coatings from the weld area first, or use a process that makes less fume. [Substitution]
- Use fume extraction (local exhaust ventilation) close to the weld. [Engineering]
- Weld outdoors or in a well-ventilated area, and keep your head out of the fume plume. [Engineering]
- Never weld or cut in a confined space without testing the air and using forced ventilation. [Administrative]
- Wear a powered air respirator or fitted respirator when extraction is not enough. [PPE]
- Use tool guards and screens to stop flying particles. [Engineering]
- Use dust extraction and water to keep dust out of the air. [Engineering]
- Keep others out of the area when cutting, grinding or chipping. [Administrative]
- Keep an eye wash station or eye wash bottles on site. [Administrative]
- Wear safety glasses at all times, goggles for dust and chemicals, and a face shield for grinding. [PPE]
- Use cold work methods where you can, such as bolting, press fittings or cutting with a saw instead of a torch. [Elimination]
- Move anything that can burn at least 35 feet away, or cover it with fire blankets. [Engineering (guarding)]
- Use fire-resistant screens to stop sparks reaching people or gaps in walls and floors. [Engineering]
- Get a hot work permit before starting. [Administrative]
- Keep a charged fire extinguisher and fire blanket at the work spot. [Administrative]
	Medium
	

	4
	Handle hot and sharp parts with gloves
	Burns from hot surfaces
Cuts from sharp edges
	Medium
	- Isolate heating systems and let parts cool before you touch them. [Elimination]
- Fit guards or insulation on hot pipes and equipment. [Engineering]
- Mark hot items with chalk or a "HOT" sign so others know. [Administrative]
- Keep a first aid kit and cool running water nearby for burns. [Administrative]
- Wear heat-resistant gloves and long sleeves. [PPE]
- Deburr or cover sharp edges, and fit edge protectors on exposed sheet metal. [Engineering]
- Use knives with retractable or self-retracting blades. [Engineering]
- Cut away from your body and keep your other hand clear. [Administrative]
- Put used blades in a blade bin or sharps container. [Administrative]
- Use two people to handle large sheets of metal or glass. [Administrative]
- Wear cut-resistant gloves and long sleeves. [PPE]
	Low
	

	5
	Store gas bottles upright and chained
	Flammable liquids and gases
Compressed air
	High
	- Use non-flammable or water-based products where you can. [Substitution]
- Keep ignition sources away: no smoking, no hot work and no running engines near flammables. [Engineering (guarding)]
- Store fuels and solvents in approved, closed containers in a ventilated area away from the work. [Engineering]
- Refuel equipment outdoors with the engine off and cool. [Administrative]
- Keep only what you need for the day on site. [Administrative]
- Store gas cylinders upright, secured and outdoors. [Administrative]
- Keep a suitable fire extinguisher where flammables are used or stored. [Administrative]
- Wear chemical gloves and safety glasses when pouring or mixing. [PPE]
- Fit whip checks (safety cables) on hose joints and check hoses before use. [Engineering]
- Fit a pressure regulator and keep pressure to the tool's rating. [Engineering]
- Turn off and bleed the line before disconnecting. [Administrative]
- Never point air at anyone or use it on clothes or skin. Air for cleaning must be under 30 psi with chip guarding (29 CFR 1926.302(b)(4)). [Administrative]
- Wear safety glasses and hearing protection. [PPE]
	Medium
	

	6
	Sweep up slag and offcuts
	Poor housekeeping and waste
	Medium
	- Order materials to size and send packaging back where you can. [Elimination]
- Put dumpsters and waste chutes close to the work. [Engineering]
- Clean as you go, and do a full clean up at the end of each day. [Administrative]
- Keep exits, stairs and walkways clear at all times. [Administrative]
- Stack materials neatly on level ground, away from edges. [Administrative]
- Wear gloves when handling waste. [PPE]
	Low
	


3. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Welding helmet (ANSI Z87.1)
Welding gloves
Safety-toe boots (ASTM F2413)
Safety glasses (ANSI Z87.1)
Hearing protection (earmuffs or plugs)
Coveralls
High-visibility safety apparel, ANSI/ISEA 107 Class 2 or 3 (Type R near roadways)
Hard hat (ANSI Z89.1)
Work gloves
N95 respirator
Face shield (ANSI Z87.1)
Cut-resistant gloves
Half-face respirator (P100 cartridges)
Safety goggles (ANSI Z87.1)
	Welding machine
Angle grinder
Oxy-acetylene torch
Forklift (Trained and evaluated operator, certified by the employer with name, training date, evaluation date and evaluator; re-evaluated every 3 years (29 CFR 1910.178(l), via 1926.602(d)))
Mobile crane (Operator certified by an accredited body or audited employer program (29 CFR 1926.1427) and evaluated by the employer, with a signed evaluation on site (1926.1427(f)); qualified rigger (1926.1425) and qualified signal person (1926.1428))
	Critical lift plan
Hot work permit (fire watch at least 60 minutes after, NFPA 51B)


4. EMERGENCY ARRANGEMENTS
	Emergency number: 911
	

	Nearest hospital
	

	Assembly point
	

	First aid / CPR person
	

	First aid kit location
	

	Fire extinguisher location
	


5. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: OSH Act Section 5(a)(1) and 29 CFR 1926, Safety and Health Regulations for Construction (incl. 1926.20 and 1926.21).
Keep this JHA on site during the job, and keep it with the training and inspection records for at least 1 year after the job (longer if your state plan or general contractor requires it). OSHA does not set a retention period for JHAs themselves.
6. SIGN-OFF
By signing below, each person confirms they have read and understood this JHA and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/us/jha/welding-fabrication/steel-fabrication-workshop/
